<?xml version="1.0" encoding="UTF-8" standalone="yes"?>
<RSLogix5000Content SchemaRevision="1.0" SoftwareRevision="36.00" TargetName="UDT_ALARMS_SIO_FIO" TargetType="DataType" ContainsContext="true" ExportDate="Fri Jun 13 12:14:11 2025" ExportOptions="References NoRawData L5KData DecoratedData Context Dependencies ForceProtectedEncoding AllProjDocTrans">
<Controller Use="Context" Name="BaseProgram">
<DataTypes Use="Context">
<DataType Name="UDT_CTRL_DPM" Family="NoFamily" Class="User">
<Members>
<Member Name="STS" DataType="UDT_CTRL_DPM_STS" Dimension="0" Radix="NullType" Hidden="false" ExternalAccess="Read/Write">
<Description>
<![CDATA[Status of DPM]]>
</Description>
</Member>
</Members>
<Dependencies>
<Dependency Type="DataType" Name="UDT_CTRL_DPM_STS"/>
</Dependencies>
</DataType>
<DataType Name="UDT_CTRL_DPM_STS" Family="NoFamily" Class="User">
<Members>
<Member Name="ZZZZZZZZZZUDT_CTRL_D0" DataType="SINT" Dimension="0" Radix="Decimal" Hidden="true" ExternalAccess="Read/Write"/>
<Member Name="Communication_Fault" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_D0" BitNumber="0" ExternalAccess="Read/Write">
<Description>
<![CDATA[Ethernet Communication is Faulted]]>
</Description>
</Member>
</Members>
</DataType>
<DataType Name="UDT_CTRL_MCM" Family="NoFamily" Class="User">
<Members>
<Member Name="CMD" DataType="UDT_CTRL_MCM_CMD" Dimension="0" Radix="NullType" Hidden="false" ExternalAccess="Read/Write">
<Description>
<![CDATA[Command To MCM]]>
</Description>
</Member>
<Member Name="STS" DataType="UDT_CTRL_MCM_STS" Dimension="0" Radix="NullType" Hidden="false" ExternalAccess="Read/Write">
<Description>
<![CDATA[Status From MCM]]>
</Description>
</Member>
</Members>
<Dependencies>
<Dependency Type="DataType" Name="UDT_CTRL_MCM_CMD"/>
<Dependency Type="DataType" Name="UDT_CTRL_MCM_STS"/>
</Dependencies>
</DataType>
<DataType Name="UDT_CTRL_MCM_CMD" Family="NoFamily" Class="User">
<Members>
<Member Name="ZZZZZZZZZZUDT_CTRL_M0" DataType="SINT" Dimension="0" Radix="Decimal" Hidden="true" ExternalAccess="Read/Write"/>
<Member Name="EStop_Actuated" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_M0" BitNumber="0" ExternalAccess="Read/Write">
<Description>
<![CDATA[Emergency Stop Actuated]]>
</Description>
</Member>
<Member Name="Started" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_M0" BitNumber="1" ExternalAccess="Read/Write">
<Description>
<![CDATA[MCM]]>
</Description>
</Member>
<Member Name="Maintenance_Mode" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_M0" BitNumber="2" ExternalAccess="Read/Write">
<Description>
<![CDATA[In Maitenance Mode]]>
</Description>
</Member>
<Member Name="Jam_Fault" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_M0" BitNumber="3" ExternalAccess="Read/Write">
<Description>
<![CDATA[Conveyor is Jammed]]>
</Description>
</Member>
<Member Name="Communication_Was_Faulted" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_M0" BitNumber="4" ExternalAccess="Read/Write">
<Description>
<![CDATA[Ethernet Communication was Faulted]]>
</Description>
</Member>
<Member Name="VFD_Was_Faulted" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_M0" BitNumber="5" ExternalAccess="Read/Write">
<Description>
<![CDATA[VFD Was Faulted]]>
</Description>
</Member>
<Member Name="EStop_Was_Actuated" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_M0" BitNumber="6" ExternalAccess="Read/Write">
<Description>
<![CDATA[Emergency Stop was Actuated]]>
</Description>
</Member>
<Member Name="Log" DataType="STRING" Dimension="0" Radix="NullType" Hidden="false" ExternalAccess="Read/Write">
<Description>
<![CDATA[Log]]>
</Description>
</Member>
<Member Name="ZZZZZZZZZZUDT_CTRL_M9" DataType="SINT" Dimension="0" Radix="Decimal" Hidden="true" ExternalAccess="Read/Write"/>
<Member Name="Acknowledge_Log" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_M9" BitNumber="0" ExternalAccess="Read/Write">
<Description>
<![CDATA[Acknowledge Log]]>
</Description>
</Member>
<Member Name="All_Unacknowledge_Log" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_M9" BitNumber="1" ExternalAccess="Read/Write">
<Description>
<![CDATA[All Unacknowledge Logs]]>
</Description>
</Member>
<Member Name="VFD_Faulted" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_M9" BitNumber="2" ExternalAccess="Read/Write">
<Description>
<![CDATA[VFD Faulted]]>
</Description>
</Member>
<Member Name="Communication_Faulted" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_M9" BitNumber="3" ExternalAccess="Read/Write">
<Description>
<![CDATA[Ethernet Communication Faulted]]>
</Description>
</Member>
<Member Name="Log_Quantity" DataType="DINT" Dimension="0" Radix="Decimal" Hidden="false" ExternalAccess="Read/Write">
<Description>
<![CDATA[Log Quantity]]>
</Description>
</Member>
<Member Name="ZZZZZZZZZZUDT_CTRL_M15" DataType="SINT" Dimension="0" Radix="Decimal" Hidden="true" ExternalAccess="Read/Write"/>
<Member Name="VFD_In_Power_Saving_Mode" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_M15" BitNumber="0" ExternalAccess="Read/Write">
<Description>
<![CDATA[VFD in Power Saving Mode]]>
</Description>
</Member>
<Member Name="Encoder_Fault" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_M15" BitNumber="1" ExternalAccess="Read/Write">
<Description>
<![CDATA[Encoder Faulted or Conveyor is running at Low Speed]]>
</Description>
</Member>
<Member Name="LAP_PB" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_M15" BitNumber="2" ExternalAccess="Read/Write">
<Description>
<![CDATA[Low Air Pressure PushButton]]>
</Description>
</Member>
<Member Name="LAP_PB_LT" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_M15" BitNumber="3" ExternalAccess="Read/Write">
<Description>
<![CDATA[Low Air Pressure PushButton Light]]>
</Description>
</Member>
<Member Name="Start_PB" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_M15" BitNumber="4" ExternalAccess="Read/Write">
<Description>
<![CDATA[Start PushButton]]>
</Description>
</Member>
<Member Name="Stop_PB" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_M15" BitNumber="5" ExternalAccess="Read/Write">
<Description>
<![CDATA[Stop PushButton]]>
</Description>
</Member>
<Member Name="VFD_Fault_Reset_PB" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_M15" BitNumber="6" ExternalAccess="Read/Write">
<Description>
<![CDATA[VFD Fault Reset PushButton]]>
</Description>
</Member>
<Member Name="Jam_Restart_PB" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_M15" BitNumber="7" ExternalAccess="Read/Write">
<Description>
<![CDATA[Jam Reset PushButton]]>
</Description>
</Member>
<Member Name="ZZZZZZZZZZUDT_CTRL_M24" DataType="SINT" Dimension="0" Radix="Decimal" Hidden="true" ExternalAccess="Read/Write"/>
<Member Name="EStop_PB" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_M24" BitNumber="0" ExternalAccess="Read/Write">
<Description>
<![CDATA[Emergency Stop PushButton]]>
</Description>
</Member>
</Members>
</DataType>
<DataType Name="UDT_CTRL_MCM_STS" Family="NoFamily" Class="User">
<Members>
<Member Name="ZZZZZZZZZZUDT_CTRL_M0" DataType="SINT" Dimension="0" Radix="Decimal" Hidden="true" ExternalAccess="Read/Write"/>
<Member Name="EStopped" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_M0" BitNumber="0" ExternalAccess="Read/Write">
<Description>
<![CDATA[Emergency Stopped]]>
</Description>
</Member>
<Member Name="Maintenance_Mode" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_M0" BitNumber="1" ExternalAccess="Read/Write">
<Description>
<![CDATA[In Maitenance Mode]]>
</Description>
</Member>
<Member Name="System_Started" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_M0" BitNumber="2" ExternalAccess="Read/Write">
<Description>
<![CDATA[The System is Started]]>
</Description>
</Member>
<Member Name="VFD_Faulted" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_M0" BitNumber="3" ExternalAccess="Read/Write">
<Description>
<![CDATA[VFD Faulted]]>
</Description>
</Member>
<Member Name="Jam_Fault" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_M0" BitNumber="4" ExternalAccess="Read/Write">
<Description>
<![CDATA[Conveyor Jammed]]>
</Description>
</Member>
<Member Name="Communication_Fault" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_M0" BitNumber="5" ExternalAccess="Read/Write">
<Description>
<![CDATA[Ethernet Communication Faulted]]>
</Description>
</Member>
<Member Name="Log" DataType="STRING" Dimension="0" Radix="NullType" Hidden="false" ExternalAccess="Read/Write">
<Description>
<![CDATA[Log]]>
</Description>
</Member>
<Member Name="Acknowledge_Log" DataType="STRING" Dimension="0" Radix="NullType" Hidden="false" ExternalAccess="Read/Write">
<Description>
<![CDATA[Acknowledge Log]]>
</Description>
</Member>
<Member Name="ZZZZZZZZZZUDT_CTRL_M9" DataType="SINT" Dimension="0" Radix="Decimal" Hidden="true" ExternalAccess="Read/Write"/>
<Member Name="All_Unacknowledge_Log" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_M9" BitNumber="0" ExternalAccess="Read/Write">
<Description>
<![CDATA[All Unacknowledged Logs]]>
</Description>
</Member>
<Member Name="Start_Request" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_M9" BitNumber="1" ExternalAccess="Read/Write">
<Description>
<![CDATA[System Start Requested]]>
</Description>
</Member>
<Member Name="Log_Quantity" DataType="DINT" Dimension="0" Radix="Decimal" Hidden="false" ExternalAccess="Read/Write">
<Description>
<![CDATA[Log Quantity]]>
</Description>
</Member>
<Member Name="ZZZZZZZZZZUDT_CTRL_M13" DataType="SINT" Dimension="0" Radix="Decimal" Hidden="true" ExternalAccess="Read/Write"/>
<Member Name="Encoder_Fault" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_M13" BitNumber="0" ExternalAccess="Read/Write">
<Description>
<![CDATA[Encoder Faulted or Conveyor is running at Low Speed]]>
</Description>
</Member>
<Member Name="LAP_PB" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_M13" BitNumber="1" ExternalAccess="Read/Write">
<Description>
<![CDATA[Low Air Pressure PushButton]]>
</Description>
</Member>
<Member Name="LAP_PB_LT" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_M13" BitNumber="2" ExternalAccess="Read/Write">
<Description>
<![CDATA[Low Air Pressure PushButton Light]]>
</Description>
</Member>
<Member Name="Start_PB" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_M13" BitNumber="3" ExternalAccess="Read/Write">
<Description>
<![CDATA[Start PushButton]]>
</Description>
</Member>
<Member Name="Stop_PB" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_M13" BitNumber="4" ExternalAccess="Read/Write">
<Description>
<![CDATA[Stop PushButton]]>
</Description>
</Member>
<Member Name="Motor_Fault_Reset_PB" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_M13" BitNumber="5" ExternalAccess="Read/Write">
<Description>
<![CDATA[Motor Fault Reset PushButton]]>
</Description>
</Member>
<Member Name="Jam_Restart_PB" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_M13" BitNumber="6" ExternalAccess="Read/Write">
<Description>
<![CDATA[Jam Restart PushButton]]>
</Description>
</Member>
<Member Name="EStop_PB" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_M13" BitNumber="7" ExternalAccess="Read/Write">
<Description>
<![CDATA[Emergency Stop PushButton]]>
</Description>
</Member>
<Member Name="ZZZZZZZZZZUDT_CTRL_M22" DataType="SINT" Dimension="0" Radix="Decimal" Hidden="true" ExternalAccess="Read/Write"/>
<Member Name="Unacknowldge_All" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_M22" BitNumber="0" ExternalAccess="Read/Write">
<Description>
<![CDATA[Unacknowledge all Alarms]]>
</Description>
</Member>
<Member Name="Aknowledgement_ID" DataType="STRING" Dimension="0" Radix="NullType" Hidden="false" ExternalAccess="Read/Write">
<Description>
<![CDATA[Aknowledgement ID]]>
</Description>
</Member>
<Member Name="ZZZZZZZZZZUDT_CTRL_M25" DataType="SINT" Dimension="0" Radix="Decimal" Hidden="true" ExternalAccess="Read/Write"/>
<Member Name="Setup_Speeds" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_M25" BitNumber="0" ExternalAccess="Read/Write">
<Description>
<![CDATA[Set Up Speeds of Conveyors]]>
</Description>
</Member>
</Members>
</DataType>
<DataType Use="Target" Name="UDT_ALARMS_SIO_FIO" Family="NoFamily" Class="User">
<Members>
<Member Name="ZZZZZZZZZZUDT_ALARMS0" DataType="SINT" Dimension="0" Radix="Decimal" Hidden="true" ExternalAccess="Read/Write"/>
<Member Name="Communication_Fault" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_ALARMS0" BitNumber="0" ExternalAccess="Read/Write">
<Description>
<![CDATA[Ethernet Communication Faulted]]>
</Description>
</Member>
</Members>
</DataType>
<DataType Use="Target" Name="UDT_AOI_SIO_FIO" Family="NoFamily" Class="User">
<Members>
<Member Name="AOI" DataType="AOI_SIO_FIO" Dimension="0" Radix="NullType" Hidden="false" ExternalAccess="Read/Write"/>
<Member Name="HMI" DataType="UDT_HMI_SIO_FIO" Dimension="0" Radix="NullType" Hidden="false" ExternalAccess="Read/Write"/>
<Member Name="CTRL" DataType="UDT_CTRL_SIO_FIO" Dimension="0" Radix="NullType" Hidden="false" ExternalAccess="Read/Write"/>
</Members>
<Dependencies>
<Dependency Type="AddOnInstructionDefinition" Name="AOI_SIO_FIO"/>
<Dependency Type="DataType" Name="UDT_HMI_SIO_FIO"/>
<Dependency Type="DataType" Name="UDT_CTRL_SIO_FIO"/>
</Dependencies>
</DataType>
<DataType Use="Target" Name="UDT_CTRL_SIO_FIO" Family="NoFamily" Class="User">
<Members>
<Member Name="STS" DataType="UDT_CTRL_SIO_FIO_STS" Dimension="0" Radix="NullType" Hidden="false" ExternalAccess="Read/Write"/>
</Members>
<Dependencies>
<Dependency Type="DataType" Name="UDT_CTRL_SIO_FIO_STS"/>
</Dependencies>
</DataType>
<DataType Use="Target" Name="UDT_CTRL_SIO_FIO_STS" Family="NoFamily" Class="User">
<Members>
<Member Name="ZZZZZZZZZZUDT_CTRL_S0" DataType="SINT" Dimension="0" Radix="Decimal" Hidden="true" ExternalAccess="Read/Write"/>
<Member Name="Communication_Fault" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_S0" BitNumber="0" ExternalAccess="Read/Write">
<Description>
<![CDATA[Ethernet Communication Faulted]]>
</Description>
</Member>
</Members>
</DataType>
<DataType Use="Target" Name="UDT_HMI_SIO_FIO" Family="NoFamily" Class="User">
<Members>
<Member Name="Name" DataType="STRING" Dimension="0" Radix="NullType" Hidden="false" ExternalAccess="Read/Write">
<Description>
<![CDATA[FIO Name]]>
</Description>
</Member>
<Member Name="Alarm" DataType="UDT_ALARMS_SIO_FIO" Dimension="0" Radix="NullType" Hidden="false" ExternalAccess="Read/Write">
<Description>
<![CDATA[SIO/FIO Alarms]]>
</Description>
</Member>
<Member Name="Color" DataType="DINT" Dimension="0" Radix="Decimal" Hidden="false" ExternalAccess="Read/Write">
<Description>
<![CDATA[Color of Animations]]>
</Description>
</Member>
<Member Name="Description" DataType="STRING" Dimension="16" Radix="NullType" Hidden="false" ExternalAccess="Read/Write"/>
<Member Name="IP_Address" DataType="STRING" Dimension="0" Radix="NullType" Hidden="false" ExternalAccess="Read/Write">
<Description>
<![CDATA[IP Address]]>
</Description>
</Member>
</Members>
<Dependencies>
<Dependency Type="DataType" Name="UDT_ALARMS_SIO_FIO"/>
</Dependencies>
</DataType>
</DataTypes>
<AddOnInstructionDefinitions Use="Context">
<AddOnInstructionDefinition Name="AOI_SIO_FIO" Revision="1.0" Vendor="Automation Standard" ExecutePrescan="true" ExecutePostscan="false" ExecuteEnableInFalse="false" CreatedDate="2021-06-02T10:38:08.709Z" CreatedBy="KONON\Artem" EditedDate="2025-05-30T13:48:31.710Z" EditedBy="LCIBATUMI\guga.kakhadze" SoftwareRevision="v36.00"
>
<Parameters>
<Parameter Name="EnableIn" TagType="Base" DataType="BOOL" Usage="Input" Radix="Decimal" Required="false" Visible="false" ExternalAccess="Read Only">
<Description>
<![CDATA[Enable Input - System Defined Parameter]]>
</Description>
</Parameter>
<Parameter Name="EnableOut" TagType="Base" DataType="BOOL" Usage="Output" Radix="Decimal" Required="false" Visible="false" ExternalAccess="Read Only">
<Description>
<![CDATA[Enable Output - System Defined Parameter]]>
</Description>
</Parameter>
<Parameter Name="HMI" TagType="Base" DataType="UDT_HMI_SIO_FIO" Usage="InOut" Required="true" Visible="true" Constant="false"/>
<Parameter Name="CTRL" TagType="Base" DataType="UDT_CTRL_SIO_FIO" Usage="InOut" Required="true" Visible="true" Constant="false"/>
<Parameter Name="Module" TagType="Base" DataType="MODULE" Usage="InOut" Required="true" Visible="true"/>
<Parameter Name="MCM" TagType="Base" DataType="UDT_CTRL_MCM" Usage="InOut" Required="true" Visible="true" Constant="false"/>
<Parameter Name="DPM" TagType="Base" DataType="UDT_CTRL_DPM" Usage="InOut" Required="true" Visible="true" Constant="false"/>
<Parameter Name="Communication_Fault" TagType="Base" DataType="BOOL" Usage="Output" Radix="Decimal" Required="false" Visible="true" ExternalAccess="Read/Write">
<Description>
<![CDATA[Communication Fault]]>
</Description>
<DefaultData Format="L5K">
<![CDATA[0]]>
</DefaultData>
<DefaultData Format="Decorated">
<DataValue DataType="BOOL" Radix="Decimal" Value="0"/>
</DefaultData>
</Parameter>
<Parameter Name="MCM_DPM_Communication_Fault" TagType="Base" DataType="BOOL" Usage="Output" Radix="Decimal" Required="false" Visible="true" ExternalAccess="Read Only">
<Description>
<![CDATA[MCM/DPM Communication Fault 
NEEDS CLARIFICATION]]>
</Description>
<DefaultData Format="L5K">
<![CDATA[0]]>
</DefaultData>
<DefaultData Format="Decorated">
<DataValue DataType="BOOL" Radix="Decimal" Value="0"/>
</DefaultData>
</Parameter>
</Parameters>
<LocalTags>
<LocalTag Name="Communication_Fault_Code" DataType="DINT" Radix="Decimal" ExternalAccess="None">
<Description>
<![CDATA[Communication Fault Code]]>
</Description>
<DefaultData Format="L5K">
<![CDATA[0]]>
</DefaultData>
<DefaultData Format="Decorated">
<DataValue DataType="DINT" Radix="Decimal" Value="0"/>
</DefaultData>
</LocalTag>
<LocalTag Name="Concatenated_String" DataType="STRING" ExternalAccess="None">
<Description>
<![CDATA[String for Log]]>
</Description>
<DefaultData Format="L5K">
<![CDATA[[0,'$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00']]]>
</DefaultData>
<DefaultData Format="String" Length="0">
<![CDATA['']]>
</DefaultData>
</LocalTag>
<LocalTag Name="Acknowledge_ONS" DataType="BOOL" Radix="Decimal" ExternalAccess="None">
<Description>
<![CDATA[To Unlatch Acknowledge Bit Once Communication Faulted]]>
</Description>
<DefaultData Format="L5K">
<![CDATA[0]]>
</DefaultData>
<DefaultData Format="Decorated">
<DataValue DataType="BOOL" Radix="Decimal" Value="0"/>
</DefaultData>
</LocalTag>
<LocalTag Name="Acknowledge" DataType="BOOL" Radix="Decimal" ExternalAccess="None">
<Description>
<![CDATA[Acknowldge]]>
</Description>
<DefaultData Format="L5K">
<![CDATA[0]]>
</DefaultData>
<DefaultData Format="Decorated">
<DataValue DataType="BOOL" Radix="Decimal" Value="0"/>
</DefaultData>
</LocalTag>
<LocalTag Name="Communication_Fault_Latch" DataType="BOOL" Radix="Decimal" ExternalAccess="None">
<Description>
<![CDATA[Communication Fault Latch]]>
</Description>
<DefaultData Format="L5K">
<![CDATA[0]]>
</DefaultData>
<DefaultData Format="Decorated">
<DataValue DataType="BOOL" Radix="Decimal" Value="0"/>
</DefaultData>
</LocalTag>
<LocalTag Name="Lost_Communication" DataType="STRING" ExternalAccess="None">
<DefaultData Format="L5K">
<![CDATA[[0,'$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00']]]>
</DefaultData>
<DefaultData Format="String" Length="0">
<![CDATA['']]>
</DefaultData>
</LocalTag>
<LocalTag Name="Empty_String" DataType="STRING" ExternalAccess="None">
<DefaultData Format="L5K">
<![CDATA[[0,'$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00']]]>
</DefaultData>
<DefaultData Format="String" Length="0">
<![CDATA['']]>
</DefaultData>
</LocalTag>
</LocalTags>
<Routines>
<Routine Name="Logic" Type="RLL">
<RLLContent>
<Rung Number="0" Type="N">
<Text>
<![CDATA[NOP();]]>
</Text>
</Rung>
<Rung Number="1" Type="N">
<Comment>
<![CDATA[Motor Ethernet Fault]]>
</Comment>
<Text>
<![CDATA[[CLR(Communication_Fault_Code) GSV(Module,Module,FaultCode,Communication_Fault_Code) NE(Communication_Fault_Code,0) OTE(Communication_Fault) OTE(HMI.Alarm.Communication_Fault) OTL(MCM.CMD.Communication_Faulted) OTL(Communication_Fault_Latch) ,XIC(DPM.STS.Communication_Fault) OTE(MCM_DPM_Communication_Fault) ]OTE(CTRL.STS.Communication_Fault);]]>
</Text>
</Rung>
<Rung Number="2" Type="N">
<Text>
<![CDATA[XIO(Communication_Fault)OTU(Communication_Fault_Latch);]]>
</Text>
</Rung>
<Rung Number="3" Type="N">
<Text>
<![CDATA[XIC(Communication_Fault_Latch)OTL(MCM.CMD.Communication_Was_Faulted);]]>
</Text>
</Rung>
<Rung Number="4" Type="N">
<Comment>
<![CDATA[Communication On - Light Grey (211.211.211)
]]>
</Comment>
<Text>
<![CDATA[XIO(Communication_Fault)MOVE(10,HMI.Color);]]>
</Text>
</Rung>
<Rung Number="5" Type="N">
<Comment>
<![CDATA[Communication Fault - Red (255.0.0)
]]>
</Comment>
<Text>
<![CDATA[XIC(Communication_Fault)MOVE(2,HMI.Color);]]>
</Text>
</Rung>
<Rung Number="6" Type="N">
<Text>
<![CDATA[XIC(MCM.STS.All_Unacknowledge_Log)OTU(Acknowledge);]]>
</Text>
</Rung>
<Rung Number="7" Type="N">
<Text>
<![CDATA[[XIC(Communication_Fault) ONS(Acknowledge_ONS) OTU(Acknowledge) ,XIC(Communication_Fault) XIO(Acknowledge) COP(Lost_Communication,Concatenated_String,1) CONCAT(HMI.Name,Concatenated_String,MCM.CMD.Log) ADD(MCM.CMD.Log_Quantity,1,MCM.CMD.Log_Quantity) ,NE(MCM.STS.Acknowledge_Log,Empty_String) EQ(MCM.CMD.Log,MCM.STS.Acknowledge_Log) OTL(Acknowledge) COP(MCM.STS.Acknowledge_Log,Empty_String,1) ];]]>
</Text>
</Rung>
</RLLContent>
</Routine>
<Routine Name="Prescan" Type="RLL">
<RLLContent>
<Rung Number="0" Type="N">
<Text>
<![CDATA[OTU(Acknowledge);]]>
</Text>
</Rung>
</RLLContent>
</Routine>
</Routines>
<Dependencies>
<Dependency Type="DataType" Name="UDT_CTRL_SIO_FIO"/>
<Dependency Type="DataType" Name="UDT_CTRL_DPM"/>
<Dependency Type="DataType" Name="UDT_HMI_SIO_FIO"/>
<Dependency Type="DataType" Name="UDT_CTRL_MCM"/>
</Dependencies>
</AddOnInstructionDefinition>
</AddOnInstructionDefinitions>
</Controller>
</RSLogix5000Content>
