<?xml version="1.0" encoding="UTF-8" standalone="yes"?>
<!--DATA POWER MODULE-->
<RSLogix5000Content SchemaRevision="1.0" SoftwareRevision="36.00" TargetName="AOI_DPM" TargetType="AddOnInstructionDefinition" TargetClass="Standard" TargetRevision="1.0 " TargetLastEdited="2025-05-19T20:06:16.540Z" ContainsContext="true" ExportDate="Fri May 23 22:11:43 2025" ExportOptions="References NoRawData L5KData DecoratedData Context Dependencies ForceProtectedEncoding AllProjDocTrans">
<Controller Use="Context" Name="MTN6_Simulations">
<DataTypes Use="Context">
<DataType Name="UDT_ALARMS_DPM" Family="NoFamily" Class="User">
<Members>
<Member Name="ZZZZZZZZZZUDT_ALARMS0" DataType="SINT" Dimension="0" Radix="Decimal" Hidden="true" ExternalAccess="Read/Write"/>
<Member Name="Communication_Fault" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_ALARMS0" BitNumber="0" ExternalAccess="Read/Write">
<Description>
<![CDATA[Ethernet Communication is Faulted]]>
</Description>
</Member>
</Members>
</DataType>
<DataType Name="UDT_CTRL_DPM" Family="NoFamily" Class="User">
<Members>
<Member Name="STS" DataType="UDT_CTRL_DPM_STS" Dimension="0" Radix="NullType" Hidden="false" ExternalAccess="Read/Write">
<Description>
<![CDATA[Status of DPM]]>
</Description>
</Member>
</Members>
<Dependencies>
<Dependency Type="DataType" Name="UDT_CTRL_DPM_STS"/>
</Dependencies>
</DataType>
<DataType Name="UDT_CTRL_DPM_STS" Family="NoFamily" Class="User">
<Members>
<Member Name="ZZZZZZZZZZUDT_CTRL_D0" DataType="SINT" Dimension="0" Radix="Decimal" Hidden="true" ExternalAccess="Read/Write"/>
<Member Name="Communication_Fault" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_D0" BitNumber="0" ExternalAccess="Read/Write">
<Description>
<![CDATA[Ethernet Communication is Faulted]]>
</Description>
</Member>
</Members>
</DataType>
<DataType Name="UDT_CTRL_MCM" Family="NoFamily" Class="User">
<Members>
<Member Name="CMD" DataType="UDT_CTRL_MCM_CMD" Dimension="0" Radix="NullType" Hidden="false" ExternalAccess="Read/Write">
<Description>
<![CDATA[Command To MCM]]>
</Description>
</Member>
<Member Name="STS" DataType="UDT_CTRL_MCM_STS" Dimension="0" Radix="NullType" Hidden="false" ExternalAccess="Read/Write">
<Description>
<![CDATA[Status From MCM]]>
</Description>
</Member>
</Members>
<Dependencies>
<Dependency Type="DataType" Name="UDT_CTRL_MCM_CMD"/>
<Dependency Type="DataType" Name="UDT_CTRL_MCM_STS"/>
</Dependencies>
</DataType>
<DataType Name="UDT_CTRL_MCM_CMD" Family="NoFamily" Class="User">
<Members>
<Member Name="ZZZZZZZZZZUDT_CTRL_M0" DataType="SINT" Dimension="0" Radix="Decimal" Hidden="true" ExternalAccess="Read/Write"/>
<Member Name="EStop_Actuated" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_M0" BitNumber="0" ExternalAccess="Read/Write">
<Description>
<![CDATA[Emergency Stop Actuated]]>
</Description>
</Member>
<Member Name="Started" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_M0" BitNumber="1" ExternalAccess="Read/Write">
<Description>
<![CDATA[MCM]]>
</Description>
</Member>
<Member Name="Maintenance_Mode" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_M0" BitNumber="2" ExternalAccess="Read/Write">
<Description>
<![CDATA[In Maitenance Mode]]>
</Description>
</Member>
<Member Name="Jam_Fault" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_M0" BitNumber="3" ExternalAccess="Read/Write">
<Description>
<![CDATA[Conveyor is Jammed]]>
</Description>
</Member>
<Member Name="Communication_Was_Faulted" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_M0" BitNumber="4" ExternalAccess="Read/Write">
<Description>
<![CDATA[Ethernet Communication was Faulted]]>
</Description>
</Member>
<Member Name="VFD_Was_Faulted" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_M0" BitNumber="5" ExternalAccess="Read/Write">
<Description>
<![CDATA[VFD Was Faulted]]>
</Description>
</Member>
<Member Name="EStop_Was_Actuated" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_M0" BitNumber="6" ExternalAccess="Read/Write">
<Description>
<![CDATA[Emergency Stop was Actuated]]>
</Description>
</Member>
<Member Name="Log" DataType="STRING" Dimension="0" Radix="NullType" Hidden="false" ExternalAccess="Read/Write">
<Description>
<![CDATA[Log]]>
</Description>
</Member>
<Member Name="ZZZZZZZZZZUDT_CTRL_M9" DataType="SINT" Dimension="0" Radix="Decimal" Hidden="true" ExternalAccess="Read/Write"/>
<Member Name="Acknowledge_Log" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_M9" BitNumber="0" ExternalAccess="Read/Write">
<Description>
<![CDATA[Acknowledge Log]]>
</Description>
</Member>
<Member Name="All_Unacknowledge_Log" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_M9" BitNumber="1" ExternalAccess="Read/Write">
<Description>
<![CDATA[All Unacknowledge Logs]]>
</Description>
</Member>
<Member Name="VFD_Faulted" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_M9" BitNumber="2" ExternalAccess="Read/Write">
<Description>
<![CDATA[VFD Faulted]]>
</Description>
</Member>
<Member Name="Communication_Faulted" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_M9" BitNumber="3" ExternalAccess="Read/Write">
<Description>
<![CDATA[Ethernet Communication Faulted]]>
</Description>
</Member>
<Member Name="Log_Quantity" DataType="DINT" Dimension="0" Radix="Decimal" Hidden="false" ExternalAccess="Read/Write">
<Description>
<![CDATA[Log Quantity]]>
</Description>
</Member>
<Member Name="ZZZZZZZZZZUDT_CTRL_M15" DataType="SINT" Dimension="0" Radix="Decimal" Hidden="true" ExternalAccess="Read/Write"/>
<Member Name="VFD_In_Power_Saving_Mode" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_M15" BitNumber="0" ExternalAccess="Read/Write">
<Description>
<![CDATA[VFD in Power Saving Mode]]>
</Description>
</Member>
<Member Name="Encoder_Fault" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_M15" BitNumber="1" ExternalAccess="Read/Write">
<Description>
<![CDATA[Encoder Faulted or Conveyor is running at Low Speed]]>
</Description>
</Member>
<Member Name="LAP_PB" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_M15" BitNumber="2" ExternalAccess="Read/Write">
<Description>
<![CDATA[Low Air Pressure PushButton]]>
</Description>
</Member>
<Member Name="LAP_PB_LT" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_M15" BitNumber="3" ExternalAccess="Read/Write">
<Description>
<![CDATA[Low Air Pressure PushButton Light]]>
</Description>
</Member>
<Member Name="Start_PB" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_M15" BitNumber="4" ExternalAccess="Read/Write">
<Description>
<![CDATA[Start PushButton]]>
</Description>
</Member>
<Member Name="Stop_PB" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_M15" BitNumber="5" ExternalAccess="Read/Write">
<Description>
<![CDATA[Stop PushButton]]>
</Description>
</Member>
<Member Name="VFD_Fault_Reset_PB" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_M15" BitNumber="6" ExternalAccess="Read/Write">
<Description>
<![CDATA[VFD Fault Reset PushButton]]>
</Description>
</Member>
<Member Name="Jam_Restart_PB" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_M15" BitNumber="7" ExternalAccess="Read/Write">
<Description>
<![CDATA[Jam Reset PushButton]]>
</Description>
</Member>
<Member Name="ZZZZZZZZZZUDT_CTRL_M24" DataType="SINT" Dimension="0" Radix="Decimal" Hidden="true" ExternalAccess="Read/Write"/>
<Member Name="EStop_PB" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_M24" BitNumber="0" ExternalAccess="Read/Write">
<Description>
<![CDATA[Emergency Stop PushButton]]>
</Description>
</Member>
</Members>
</DataType>
<DataType Name="UDT_CTRL_MCM_STS" Family="NoFamily" Class="User">
<Members>
<Member Name="ZZZZZZZZZZUDT_CTRL_M0" DataType="SINT" Dimension="0" Radix="Decimal" Hidden="true" ExternalAccess="Read/Write"/>
<Member Name="EStopped" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_M0" BitNumber="0" ExternalAccess="Read/Write">
<Description>
<![CDATA[Emergency Stopped]]>
</Description>
</Member>
<Member Name="Maintenance_Mode" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_M0" BitNumber="1" ExternalAccess="Read/Write">
<Description>
<![CDATA[In Maitenance Mode]]>
</Description>
</Member>
<Member Name="System_Started" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_M0" BitNumber="2" ExternalAccess="Read/Write">
<Description>
<![CDATA[The System is Started]]>
</Description>
</Member>
<Member Name="VFD_Faulted" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_M0" BitNumber="3" ExternalAccess="Read/Write">
<Description>
<![CDATA[VFD Faulted]]>
</Description>
</Member>
<Member Name="Jam_Fault" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_M0" BitNumber="4" ExternalAccess="Read/Write">
<Description>
<![CDATA[Conveyor Jammed]]>
</Description>
</Member>
<Member Name="Communication_Fault" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_M0" BitNumber="5" ExternalAccess="Read/Write">
<Description>
<![CDATA[Ethernet Communication Faulted]]>
</Description>
</Member>
<Member Name="Log" DataType="STRING" Dimension="0" Radix="NullType" Hidden="false" ExternalAccess="Read/Write">
<Description>
<![CDATA[Log]]>
</Description>
</Member>
<Member Name="Acknowledge_Log" DataType="STRING" Dimension="0" Radix="NullType" Hidden="false" ExternalAccess="Read/Write">
<Description>
<![CDATA[Acknowledge Log]]>
</Description>
</Member>
<Member Name="ZZZZZZZZZZUDT_CTRL_M9" DataType="SINT" Dimension="0" Radix="Decimal" Hidden="true" ExternalAccess="Read/Write"/>
<Member Name="All_Unacknowledge_Log" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_M9" BitNumber="0" ExternalAccess="Read/Write">
<Description>
<![CDATA[All Unacknowledged Logs]]>
</Description>
</Member>
<Member Name="Start_Request" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_M9" BitNumber="1" ExternalAccess="Read/Write">
<Description>
<![CDATA[System Start Requested]]>
</Description>
</Member>
<Member Name="Log_Quantity" DataType="DINT" Dimension="0" Radix="Decimal" Hidden="false" ExternalAccess="Read/Write">
<Description>
<![CDATA[Log Quantity]]>
</Description>
</Member>
<Member Name="ZZZZZZZZZZUDT_CTRL_M13" DataType="SINT" Dimension="0" Radix="Decimal" Hidden="true" ExternalAccess="Read/Write"/>
<Member Name="Encoder_Fault" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_M13" BitNumber="0" ExternalAccess="Read/Write">
<Description>
<![CDATA[Encoder Faulted or Conveyor is running at Low Speed]]>
</Description>
</Member>
<Member Name="LAP_PB" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_M13" BitNumber="1" ExternalAccess="Read/Write">
<Description>
<![CDATA[Low Air Pressure PushButton]]>
</Description>
</Member>
<Member Name="LAP_PB_LT" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_M13" BitNumber="2" ExternalAccess="Read/Write">
<Description>
<![CDATA[Low Air Pressure PushButton Light]]>
</Description>
</Member>
<Member Name="Start_PB" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_M13" BitNumber="3" ExternalAccess="Read/Write">
<Description>
<![CDATA[Start PushButton]]>
</Description>
</Member>
<Member Name="Stop_PB" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_M13" BitNumber="4" ExternalAccess="Read/Write">
<Description>
<![CDATA[Stop PushButton]]>
</Description>
</Member>
<Member Name="Motor_Fault_Reset_PB" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_M13" BitNumber="5" ExternalAccess="Read/Write">
<Description>
<![CDATA[Motor Fault Reset PushButton]]>
</Description>
</Member>
<Member Name="Jam_Restart_PB" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_M13" BitNumber="6" ExternalAccess="Read/Write">
<Description>
<![CDATA[Jam Restart PushButton]]>
</Description>
</Member>
<Member Name="EStop_PB" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_M13" BitNumber="7" ExternalAccess="Read/Write">
<Description>
<![CDATA[Emergency Stop PushButton]]>
</Description>
</Member>
<Member Name="ZZZZZZZZZZUDT_CTRL_M22" DataType="SINT" Dimension="0" Radix="Decimal" Hidden="true" ExternalAccess="Read/Write"/>
<Member Name="Unacknowldge_All" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_M22" BitNumber="0" ExternalAccess="Read/Write">
<Description>
<![CDATA[Unacknowledge all Alarms]]>
</Description>
</Member>
<Member Name="Aknowledgement_ID" DataType="STRING" Dimension="0" Radix="NullType" Hidden="false" ExternalAccess="Read/Write">
<Description>
<![CDATA[Aknowledgement ID]]>
</Description>
</Member>
<Member Name="ZZZZZZZZZZUDT_CTRL_M25" DataType="SINT" Dimension="0" Radix="Decimal" Hidden="true" ExternalAccess="Read/Write"/>
<Member Name="Setup_Speeds" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_M25" BitNumber="0" ExternalAccess="Read/Write">
<Description>
<![CDATA[Set Up Speeds of Conveyors]]>
</Description>
</Member>
</Members>
</DataType>
<DataType Name="UDT_HMI_DPM" Family="NoFamily" Class="User">
<Members>
<Member Name="Name" DataType="STRING" Dimension="0" Radix="NullType" Hidden="false" ExternalAccess="Read/Write">
<Description>
<![CDATA[DPM Name]]>
</Description>
</Member>
<Member Name="Alarm" DataType="UDT_ALARMS_DPM" Dimension="0" Radix="NullType" Hidden="false" ExternalAccess="Read/Write">
<Description>
<![CDATA[HMI
Alarms]]>
</Description>
</Member>
<Member Name="Color" DataType="DINT" Dimension="0" Radix="Decimal" Hidden="false" ExternalAccess="Read/Write">
<Description>
<![CDATA[Color Animation]]>
</Description>
</Member>
<Member Name="Description" DataType="STRING" Dimension="16" Radix="NullType" Hidden="false" ExternalAccess="Read/Write">
<Description>
<![CDATA[Description]]>
</Description>
</Member>
<Member Name="IP_Address" DataType="STRING" Dimension="0" Radix="NullType" Hidden="false" ExternalAccess="Read/Write">
<Description>
<![CDATA[IP address]]>
</Description>
</Member>
</Members>
<Dependencies>
<Dependency Type="DataType" Name="UDT_ALARMS_DPM"/>
</Dependencies>
</DataType>
</DataTypes>
<AddOnInstructionDefinitions Use="Context">
<AddOnInstructionDefinition Use="Target" Name="AOI_DPM" Class="Standard" Revision="1.0" Vendor="Automation Standard" ExecutePrescan="true" ExecutePostscan="false" ExecuteEnableInFalse="false" CreatedDate="2021-06-02T10:38:08.709Z" CreatedBy="KONON\Artem" EditedDate="2025-05-19T20:06:16.540Z"
 EditedBy="LCIBATUMI\ilia.gurielidze" SoftwareRevision="v36.00">
<Description>
<![CDATA[DATA POWER MODULE]]>
</Description>
<Parameters>
<Parameter Name="EnableIn" TagType="Base" DataType="BOOL" Usage="Input" Radix="Decimal" Required="false" Visible="false" ExternalAccess="Read Only">
<Description>
<![CDATA[Enable Input - System Defined Parameter]]>
</Description>
</Parameter>
<Parameter Name="EnableOut" TagType="Base" DataType="BOOL" Usage="Output" Radix="Decimal" Required="false" Visible="false" ExternalAccess="Read Only">
<Description>
<![CDATA[Enable Output - System Defined Parameter]]>
</Description>
</Parameter>
<Parameter Name="HMI" TagType="Base" DataType="UDT_HMI_DPM" Usage="InOut" Required="true" Visible="true" Constant="false"/>
<Parameter Name="CTRL" TagType="Base" DataType="UDT_CTRL_DPM" Usage="InOut" Required="true" Visible="true" Constant="false"/>
<Parameter Name="MSG" TagType="Base" DataType="MESSAGE" Usage="InOut" Required="true" Visible="true"/>
<Parameter Name="MCM" TagType="Base" DataType="UDT_CTRL_MCM" Usage="InOut" Required="true" Visible="true" Constant="false"/>
<Parameter Name="Communication_Fault" TagType="Base" DataType="BOOL" Usage="Output" Radix="Decimal" Required="false" Visible="true" ExternalAccess="Read/Write">
<DefaultData Format="L5K">
<![CDATA[0]]>
</DefaultData>
<DefaultData Format="Decorated">
<DataValue DataType="BOOL" Radix="Decimal" Value="0"/>
</DefaultData>
</Parameter>
<Parameter Name="MSG_Result" TagType="Base" DataType="DINT" Usage="Input" Radix="Decimal" Required="false" Visible="false" ExternalAccess="Read/Write">
<DefaultData Format="L5K">
<![CDATA[0]]>
</DefaultData>
<DefaultData Format="Decorated">
<DataValue DataType="DINT" Radix="Decimal" Value="0"/>
</DefaultData>
</Parameter>
</Parameters>
<LocalTags>
<LocalTag Name="CommFCode" DataType="DINT" Radix="Decimal" ExternalAccess="None">
<DefaultData Format="L5K">
<![CDATA[0]]>
</DefaultData>
<DefaultData Format="Decorated">
<DataValue DataType="DINT" Radix="Decimal" Value="0"/>
</DefaultData>
</LocalTag>
<LocalTag Name="MSG_Tmr" DataType="TIMER" ExternalAccess="None">
<DefaultData Format="L5K">
<![CDATA[[0,2000,804]]]>
</DefaultData>
<DefaultData Format="Decorated">
<Structure DataType="TIMER">
<DataValueMember Name="PRE" DataType="DINT" Radix="Decimal" Value="2000"/>
<DataValueMember Name="ACC" DataType="DINT" Radix="Decimal" Value="804"/>
<DataValueMember Name="EN" DataType="BOOL" Value="0"/>
<DataValueMember Name="TT" DataType="BOOL" Value="0"/>
<DataValueMember Name="DN" DataType="BOOL" Value="0"/>
</Structure>
</DefaultData>
</LocalTag>
<LocalTag Name="TImeout_Tmr" DataType="TIMER" ExternalAccess="None">
<DefaultData Format="L5K">
<![CDATA[[0,10000,0]]]>
</DefaultData>
<DefaultData Format="Decorated">
<Structure DataType="TIMER">
<DataValueMember Name="PRE" DataType="DINT" Radix="Decimal" Value="10000"/>
<DataValueMember Name="ACC" DataType="DINT" Radix="Decimal" Value="0"/>
<DataValueMember Name="EN" DataType="BOOL" Value="0"/>
<DataValueMember Name="TT" DataType="BOOL" Value="0"/>
<DataValueMember Name="DN" DataType="BOOL" Value="0"/>
</Structure>
</DefaultData>
</LocalTag>
<LocalTag Name="AckONS" DataType="DINT" Radix="Decimal" ExternalAccess="None">
<DefaultData Format="L5K">
<![CDATA[0]]>
</DefaultData>
<DefaultData Format="Decorated">
<DataValue DataType="DINT" Radix="Decimal" Value="0"/>
</DefaultData>
</LocalTag>
<LocalTag Name="Ack" DataType="DINT" Radix="Decimal" ExternalAccess="None">
<DefaultData Format="L5K">
<![CDATA[0]]>
</DefaultData>
<DefaultData Format="Decorated">
<DataValue DataType="DINT" Radix="Decimal" Value="0"/>
</DefaultData>
</LocalTag>
<LocalTag Name="Concat_Str" DataType="STRING" ExternalAccess="None">
<DefaultData Format="L5K">
<![CDATA[[0,'$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00']]]>
</DefaultData>
<DefaultData Format="String" Length="0">
<![CDATA['']]>
</DefaultData>
</LocalTag>
<LocalTag Name="CommFaultLatch" DataType="BOOL" Radix="Decimal" ExternalAccess="None">
<DefaultData Format="L5K">
<![CDATA[0]]>
</DefaultData>
<DefaultData Format="Decorated">
<DataValue DataType="BOOL" Radix="Decimal" Value="0"/>
</DefaultData>
</LocalTag>
</LocalTags>
<Routines>
<Routine Name="Logic" Type="RLL">
<RLLContent>
<Rung Number="0" Type="N">
<Text>
<![CDATA[NOP();]]>
</Text>
</Rung>
<Rung Number="1" Type="N">
<Text>
<![CDATA[XIO(MSG_Tmr.DN)TON(MSG_Tmr,?,?);]]>
</Text>
</Rung>
<Rung Number="2" Type="N">
<Text>
<![CDATA[XIC(MSG_Tmr.DN)MSG(MSG);]]>
</Text>
</Rung>
<Rung Number="3" Type="N">
<Text>
<![CDATA[XIO(MSG.DN)TON(TImeout_Tmr,?,?)XIC(TImeout_Tmr.DN)OTE(Communication_Fault)OTE(CTRL.STS.Communication_Fault)OTE(HMI.Alarm.Communication_Fault)OTL(MCM.CMD.Communication_Faulted)OTL(CommFaultLatch);]]>
</Text>
</Rung>
<Rung Number="4" Type="N">
<Text>
<![CDATA[XIO(Communication_Fault)OTU(CommFaultLatch);]]>
</Text>
</Rung>
<Rung Number="5" Type="N">
<Text>
<![CDATA[XIC(CommFaultLatch)OTL(MCM.CMD.Communication_Was_Faulted);]]>
</Text>
</Rung>
<Rung Number="6" Type="N">
<Comment>
<![CDATA[Off - Light grey Color (211.211.211)]]>
</Comment>
<Text>
<![CDATA[XIO(Communication_Fault)MOVE(10,HMI.Color);]]>
</Text>
</Rung>
<Rung Number="7" Type="N">
<Comment>
<![CDATA[Fault - Red Color (255.0.0)]]>
</Comment>
<Text>
<![CDATA[XIC(Communication_Fault)MOVE(2,HMI.Color);]]>
</Text>
</Rung>
<Rung Number="8" Type="N">
<Text>
<![CDATA[XIC(MCM.STS.All_Unacknowledge_Log)MOVE(0,Ack);]]>
</Text>
</Rung>
<Rung Number="9" Type="N">
<Text>
<![CDATA[[XIC(Communication_Fault) ONS(AckONS.0) OTU(Ack.0) ,XIC(Communication_Fault) XIO(Ack.0) MOVE(' LOST COMM',Concat_Str) CONCAT(HMI.Name,Concat_Str,MCM.CMD.Log) ,NE(MCM.STS.Acknowledge_Log,'') EQ(MCM.CMD.Log,MCM.STS.Acknowledge_Log) OTL(Ack.0) MOVE('',MCM.STS.Acknowledge_Log) ];]]>
</Text>
</Rung>
</RLLContent>
</Routine>
<Routine Name="Prescan" Type="RLL">
<RLLContent>
<Rung Number="0" Type="N">
<Text>
<![CDATA[MOVE(1000,MSG_Tmr.PRE)MOVE(5000,TImeout_Tmr.PRE)MOVE(0,Ack);]]>
</Text>
</Rung>
</RLLContent>
</Routine>
</Routines>
<Dependencies>
<Dependency Type="DataType" Name="UDT_CTRL_DPM"/>
<Dependency Type="DataType" Name="UDT_HMI_DPM"/>
<Dependency Type="DataType" Name="UDT_CTRL_MCM"/>
</Dependencies>
</AddOnInstructionDefinition>
</AddOnInstructionDefinitions>
</Controller>
</RSLogix5000Content>
