<?xml version="1.0" encoding="UTF-8" standalone="yes"?>
<RSLogix5000Content SchemaRevision="1.0" SoftwareRevision="36.00" TargetName="UDT_ALARMS_VFD" TargetType="DataType" ContainsContext="true" ExportDate="Fri Jun 13 12:17:13 2025" ExportOptions="References NoRawData L5KData DecoratedData Context Dependencies ForceProtectedEncoding AllProjDocTrans">
<Controller Use="Context" Name="BaseProgram">
<DataTypes Use="Context">
<DataType Name="UDT_CTRL_MCM" Family="NoFamily" Class="User">
<Members>
<Member Name="CMD" DataType="UDT_CTRL_MCM_CMD" Dimension="0" Radix="NullType" Hidden="false" ExternalAccess="Read/Write">
<Description>
<![CDATA[Command To MCM]]>
</Description>
</Member>
<Member Name="STS" DataType="UDT_CTRL_MCM_STS" Dimension="0" Radix="NullType" Hidden="false" ExternalAccess="Read/Write">
<Description>
<![CDATA[Status From MCM]]>
</Description>
</Member>
</Members>
<Dependencies>
<Dependency Type="DataType" Name="UDT_CTRL_MCM_CMD"/>
<Dependency Type="DataType" Name="UDT_CTRL_MCM_STS"/>
</Dependencies>
</DataType>
<DataType Name="UDT_CTRL_MCM_CMD" Family="NoFamily" Class="User">
<Members>
<Member Name="ZZZZZZZZZZUDT_CTRL_M0" DataType="SINT" Dimension="0" Radix="Decimal" Hidden="true" ExternalAccess="Read/Write"/>
<Member Name="EStop_Actuated" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_M0" BitNumber="0" ExternalAccess="Read/Write">
<Description>
<![CDATA[Emergency Stop Actuated]]>
</Description>
</Member>
<Member Name="Started" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_M0" BitNumber="1" ExternalAccess="Read/Write">
<Description>
<![CDATA[MCM]]>
</Description>
</Member>
<Member Name="Maintenance_Mode" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_M0" BitNumber="2" ExternalAccess="Read/Write">
<Description>
<![CDATA[In Maitenance Mode]]>
</Description>
</Member>
<Member Name="Jam_Fault" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_M0" BitNumber="3" ExternalAccess="Read/Write">
<Description>
<![CDATA[Conveyor is Jammed]]>
</Description>
</Member>
<Member Name="Communication_Was_Faulted" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_M0" BitNumber="4" ExternalAccess="Read/Write">
<Description>
<![CDATA[Ethernet Communication was Faulted]]>
</Description>
</Member>
<Member Name="VFD_Was_Faulted" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_M0" BitNumber="5" ExternalAccess="Read/Write">
<Description>
<![CDATA[VFD Was Faulted]]>
</Description>
</Member>
<Member Name="EStop_Was_Actuated" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_M0" BitNumber="6" ExternalAccess="Read/Write">
<Description>
<![CDATA[Emergency Stop was Actuated]]>
</Description>
</Member>
<Member Name="Log" DataType="STRING" Dimension="0" Radix="NullType" Hidden="false" ExternalAccess="Read/Write">
<Description>
<![CDATA[Log]]>
</Description>
</Member>
<Member Name="ZZZZZZZZZZUDT_CTRL_M9" DataType="SINT" Dimension="0" Radix="Decimal" Hidden="true" ExternalAccess="Read/Write"/>
<Member Name="Acknowledge_Log" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_M9" BitNumber="0" ExternalAccess="Read/Write">
<Description>
<![CDATA[Acknowledge Log]]>
</Description>
</Member>
<Member Name="All_Unacknowledge_Log" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_M9" BitNumber="1" ExternalAccess="Read/Write">
<Description>
<![CDATA[All Unacknowledge Logs]]>
</Description>
</Member>
<Member Name="VFD_Faulted" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_M9" BitNumber="2" ExternalAccess="Read/Write">
<Description>
<![CDATA[VFD Faulted]]>
</Description>
</Member>
<Member Name="Communication_Faulted" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_M9" BitNumber="3" ExternalAccess="Read/Write">
<Description>
<![CDATA[Ethernet Communication Faulted]]>
</Description>
</Member>
<Member Name="Log_Quantity" DataType="DINT" Dimension="0" Radix="Decimal" Hidden="false" ExternalAccess="Read/Write">
<Description>
<![CDATA[Log Quantity]]>
</Description>
</Member>
<Member Name="ZZZZZZZZZZUDT_CTRL_M15" DataType="SINT" Dimension="0" Radix="Decimal" Hidden="true" ExternalAccess="Read/Write"/>
<Member Name="VFD_In_Power_Saving_Mode" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_M15" BitNumber="0" ExternalAccess="Read/Write">
<Description>
<![CDATA[VFD in Power Saving Mode]]>
</Description>
</Member>
<Member Name="Encoder_Fault" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_M15" BitNumber="1" ExternalAccess="Read/Write">
<Description>
<![CDATA[Encoder Faulted or Conveyor is running at Low Speed]]>
</Description>
</Member>
<Member Name="LAP_PB" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_M15" BitNumber="2" ExternalAccess="Read/Write">
<Description>
<![CDATA[Low Air Pressure PushButton]]>
</Description>
</Member>
<Member Name="LAP_PB_LT" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_M15" BitNumber="3" ExternalAccess="Read/Write">
<Description>
<![CDATA[Low Air Pressure PushButton Light]]>
</Description>
</Member>
<Member Name="Start_PB" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_M15" BitNumber="4" ExternalAccess="Read/Write">
<Description>
<![CDATA[Start PushButton]]>
</Description>
</Member>
<Member Name="Stop_PB" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_M15" BitNumber="5" ExternalAccess="Read/Write">
<Description>
<![CDATA[Stop PushButton]]>
</Description>
</Member>
<Member Name="VFD_Fault_Reset_PB" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_M15" BitNumber="6" ExternalAccess="Read/Write">
<Description>
<![CDATA[VFD Fault Reset PushButton]]>
</Description>
</Member>
<Member Name="Jam_Restart_PB" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_M15" BitNumber="7" ExternalAccess="Read/Write">
<Description>
<![CDATA[Jam Reset PushButton]]>
</Description>
</Member>
<Member Name="ZZZZZZZZZZUDT_CTRL_M24" DataType="SINT" Dimension="0" Radix="Decimal" Hidden="true" ExternalAccess="Read/Write"/>
<Member Name="EStop_PB" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_M24" BitNumber="0" ExternalAccess="Read/Write">
<Description>
<![CDATA[Emergency Stop PushButton]]>
</Description>
</Member>
</Members>
</DataType>
<DataType Name="UDT_CTRL_MCM_STS" Family="NoFamily" Class="User">
<Members>
<Member Name="ZZZZZZZZZZUDT_CTRL_M0" DataType="SINT" Dimension="0" Radix="Decimal" Hidden="true" ExternalAccess="Read/Write"/>
<Member Name="EStopped" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_M0" BitNumber="0" ExternalAccess="Read/Write">
<Description>
<![CDATA[Emergency Stopped]]>
</Description>
</Member>
<Member Name="Maintenance_Mode" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_M0" BitNumber="1" ExternalAccess="Read/Write">
<Description>
<![CDATA[In Maitenance Mode]]>
</Description>
</Member>
<Member Name="System_Started" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_M0" BitNumber="2" ExternalAccess="Read/Write">
<Description>
<![CDATA[The System is Started]]>
</Description>
</Member>
<Member Name="VFD_Faulted" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_M0" BitNumber="3" ExternalAccess="Read/Write">
<Description>
<![CDATA[VFD Faulted]]>
</Description>
</Member>
<Member Name="Jam_Fault" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_M0" BitNumber="4" ExternalAccess="Read/Write">
<Description>
<![CDATA[Conveyor Jammed]]>
</Description>
</Member>
<Member Name="Communication_Fault" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_M0" BitNumber="5" ExternalAccess="Read/Write">
<Description>
<![CDATA[Ethernet Communication Faulted]]>
</Description>
</Member>
<Member Name="Log" DataType="STRING" Dimension="0" Radix="NullType" Hidden="false" ExternalAccess="Read/Write">
<Description>
<![CDATA[Log]]>
</Description>
</Member>
<Member Name="Acknowledge_Log" DataType="STRING" Dimension="0" Radix="NullType" Hidden="false" ExternalAccess="Read/Write">
<Description>
<![CDATA[Acknowledge Log]]>
</Description>
</Member>
<Member Name="ZZZZZZZZZZUDT_CTRL_M9" DataType="SINT" Dimension="0" Radix="Decimal" Hidden="true" ExternalAccess="Read/Write"/>
<Member Name="All_Unacknowledge_Log" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_M9" BitNumber="0" ExternalAccess="Read/Write">
<Description>
<![CDATA[All Unacknowledged Logs]]>
</Description>
</Member>
<Member Name="Start_Request" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_M9" BitNumber="1" ExternalAccess="Read/Write">
<Description>
<![CDATA[System Start Requested]]>
</Description>
</Member>
<Member Name="Log_Quantity" DataType="DINT" Dimension="0" Radix="Decimal" Hidden="false" ExternalAccess="Read/Write">
<Description>
<![CDATA[Log Quantity]]>
</Description>
</Member>
<Member Name="ZZZZZZZZZZUDT_CTRL_M13" DataType="SINT" Dimension="0" Radix="Decimal" Hidden="true" ExternalAccess="Read/Write"/>
<Member Name="Encoder_Fault" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_M13" BitNumber="0" ExternalAccess="Read/Write">
<Description>
<![CDATA[Encoder Faulted or Conveyor is running at Low Speed]]>
</Description>
</Member>
<Member Name="LAP_PB" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_M13" BitNumber="1" ExternalAccess="Read/Write">
<Description>
<![CDATA[Low Air Pressure PushButton]]>
</Description>
</Member>
<Member Name="LAP_PB_LT" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_M13" BitNumber="2" ExternalAccess="Read/Write">
<Description>
<![CDATA[Low Air Pressure PushButton Light]]>
</Description>
</Member>
<Member Name="Start_PB" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_M13" BitNumber="3" ExternalAccess="Read/Write">
<Description>
<![CDATA[Start PushButton]]>
</Description>
</Member>
<Member Name="Stop_PB" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_M13" BitNumber="4" ExternalAccess="Read/Write">
<Description>
<![CDATA[Stop PushButton]]>
</Description>
</Member>
<Member Name="Motor_Fault_Reset_PB" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_M13" BitNumber="5" ExternalAccess="Read/Write">
<Description>
<![CDATA[Motor Fault Reset PushButton]]>
</Description>
</Member>
<Member Name="Jam_Restart_PB" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_M13" BitNumber="6" ExternalAccess="Read/Write">
<Description>
<![CDATA[Jam Restart PushButton]]>
</Description>
</Member>
<Member Name="EStop_PB" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_M13" BitNumber="7" ExternalAccess="Read/Write">
<Description>
<![CDATA[Emergency Stop PushButton]]>
</Description>
</Member>
<Member Name="ZZZZZZZZZZUDT_CTRL_M22" DataType="SINT" Dimension="0" Radix="Decimal" Hidden="true" ExternalAccess="Read/Write"/>
<Member Name="Unacknowldge_All" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_M22" BitNumber="0" ExternalAccess="Read/Write">
<Description>
<![CDATA[Unacknowledge all Alarms]]>
</Description>
</Member>
<Member Name="Aknowledgement_ID" DataType="STRING" Dimension="0" Radix="NullType" Hidden="false" ExternalAccess="Read/Write">
<Description>
<![CDATA[Aknowledgement ID]]>
</Description>
</Member>
<Member Name="ZZZZZZZZZZUDT_CTRL_M25" DataType="SINT" Dimension="0" Radix="Decimal" Hidden="true" ExternalAccess="Read/Write"/>
<Member Name="Setup_Speeds" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_M25" BitNumber="0" ExternalAccess="Read/Write">
<Description>
<![CDATA[Set Up Speeds of Conveyors]]>
</Description>
</Member>
</Members>
</DataType>
<DataType Name="UDT_CTRL_SIO_FIO" Family="NoFamily" Class="User">
<Members>
<Member Name="STS" DataType="UDT_CTRL_SIO_FIO_STS" Dimension="0" Radix="NullType" Hidden="false" ExternalAccess="Read/Write"/>
</Members>
<Dependencies>
<Dependency Type="DataType" Name="UDT_CTRL_SIO_FIO_STS"/>
</Dependencies>
</DataType>
<DataType Name="UDT_CTRL_SIO_FIO_STS" Family="NoFamily" Class="User">
<Members>
<Member Name="ZZZZZZZZZZUDT_CTRL_S0" DataType="SINT" Dimension="0" Radix="Decimal" Hidden="true" ExternalAccess="Read/Write"/>
<Member Name="Communication_Fault" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_S0" BitNumber="0" ExternalAccess="Read/Write">
<Description>
<![CDATA[Ethernet Communication Faulted]]>
</Description>
</Member>
</Members>
</DataType>
<DataType Use="Target" Name="UDT_ALARMS_VFD" Family="NoFamily" Class="User">
<Members>
<Member Name="ZZZZZZZZZZUDT_ALARMS0" DataType="SINT" Dimension="0" Radix="Decimal" Hidden="true" ExternalAccess="Read/Write"/>
<Member Name="Communication_Fault" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_ALARMS0" BitNumber="0" ExternalAccess="Read/Write">
<Description>
<![CDATA[Ethernet Communication is Faulted]]>
</Description>
</Member>
<Member Name="Disconnected" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_ALARMS0" BitNumber="1" ExternalAccess="Read/Write">
<Description>
<![CDATA[Disconnected VFD]]>
</Description>
</Member>
<Member Name="VFD_Fault" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_ALARMS0" BitNumber="2" ExternalAccess="Read/Write">
<Description>
<![CDATA[VFD Faulted]]>
</Description>
</Member>
<Member Name="Safe_Off_Fault" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_ALARMS0" BitNumber="3" ExternalAccess="Read/Write">
<Description>
<![CDATA[VFD Safety Torque Fault]]>
</Description>
</Member>
<Member Name="Reset_VFD" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_ALARMS0" BitNumber="4" ExternalAccess="Read/Write">
<Description>
<![CDATA[VFD Reset]]>
</Description>
</Member>
<Member Name="Reset_Communication_Fault" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_ALARMS0" BitNumber="5" ExternalAccess="Read/Write">
<Description>
<![CDATA[Reset Comunication Fault]]>
</Description>
</Member>
</Members>
</DataType>
<DataType Use="Target" Name="UDT_AOI_VFD" Family="NoFamily" Class="User">
<Members>
<Member Name="AOI" DataType="AOI_VFD" Dimension="0" Radix="NullType" Hidden="false" ExternalAccess="Read/Write"/>
<Member Name="HMI" DataType="UDT_HMI_VFD" Dimension="0" Radix="NullType" Hidden="false" ExternalAccess="Read/Write"/>
<Member Name="CTRL" DataType="UDT_CTRL_VFD" Dimension="0" Radix="NullType" Hidden="false" ExternalAccess="Read/Write"/>
</Members>
<Dependencies>
<Dependency Type="AddOnInstructionDefinition" Name="AOI_VFD"/>
<Dependency Type="DataType" Name="UDT_HMI_VFD"/>
<Dependency Type="DataType" Name="UDT_CTRL_VFD"/>
</Dependencies>
</DataType>
<DataType Use="Target" Name="UDT_CTRL_VFD" Family="NoFamily" Class="User">
<Members>
<Member Name="CMD" DataType="UDT_CTRL_VFD_CMD" Dimension="0" Radix="NullType" Hidden="false" ExternalAccess="Read/Write"/>
<Member Name="STS" DataType="UDT_CTRL_VFD_STS" Dimension="0" Radix="NullType" Hidden="false" ExternalAccess="Read/Write"/>
</Members>
<Dependencies>
<Dependency Type="DataType" Name="UDT_CTRL_VFD_CMD"/>
<Dependency Type="DataType" Name="UDT_CTRL_VFD_STS"/>
</Dependencies>
</DataType>
<DataType Use="Target" Name="UDT_CTRL_VFD_CMD" Family="NoFamily" Class="User">
<Members>
<Member Name="ZZZZZZZZZZUDT_CTRL_V0" DataType="SINT" Dimension="0" Radix="Decimal" Hidden="true" ExternalAccess="Read/Write"/>
<Member Name="Start" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_V0" BitNumber="0" ExternalAccess="Read/Write">
<Description>
<![CDATA[Start the Conveyor Locally in Auto Mode]]>
</Description>
</Member>
<Member Name="Stop_Require_Start" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_V0" BitNumber="1" ExternalAccess="Read/Write">
<Description>
<![CDATA[Stops the Motor
, requires Start command to Restart]]>
</Description>
</Member>
<Member Name="Stop_Auto_Restart" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_V0" BitNumber="2" ExternalAccess="Read/Write">
<Description>
<![CDATA[Stops the Motor, which will restart automatically when False]]>
</Description>
</Member>
<Member Name="Jammed" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_V0" BitNumber="3" ExternalAccess="Read/Write">
<Description>
<![CDATA[Conveyor]]>
</Description>
</Member>
<Member Name="Disable" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_V0" BitNumber="4" ExternalAccess="Read/Write">
<Description>
<![CDATA[Conveyor]]>
</Description>
</Member>
<Member Name="Run_Up_Enabled" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_V0" BitNumber="5" ExternalAccess="Read/Write">
<Description>
<![CDATA[When Downstream Conveyors are Stopped, Conveyor keeps running unill Discharge PE is Blocked]]>
</Description>
</Member>
<Member Name="Power_Saving_Mode_ON" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_V0" BitNumber="6" ExternalAccess="Read/Write">
<Description>
<![CDATA[VFD
is in Power Saving Mode]]>
</Description>
</Member>
<Member Name="Interlock" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_V0" BitNumber="7" ExternalAccess="Read/Write">
<Description>
<![CDATA[Downstream is Running]]>
</Description>
</Member>
<Member Name="ZZZZZZZZZZUDT_CTRL_V9" DataType="SINT" Dimension="0" Radix="Decimal" Hidden="true" ExternalAccess="Read/Write"/>
<Member Name="Stopped_By_Stop_PB" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_V9" BitNumber="0" ExternalAccess="Read/Write">
<Description>
<![CDATA[Conveyor
Stopped by Station Stop PushButton]]>
</Description>
</Member>
<Member Name="Log" DataType="STRING" Dimension="0" Radix="NullType" Hidden="false" ExternalAccess="Read/Write">
<Description>
<![CDATA[Log]]>
</Description>
</Member>
<Member Name="Acknowledge_Log" DataType="STRING" Dimension="0" Radix="NullType" Hidden="false" ExternalAccess="Read/Write">
<Description>
<![CDATA[Acknowledge Log]]>
</Description>
</Member>
<Member Name="ZZZZZZZZZZUDT_CTRL_V13" DataType="SINT" Dimension="0" Radix="Decimal" Hidden="true" ExternalAccess="Read/Write"/>
<Member Name="Full" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_V13" BitNumber="0" ExternalAccess="Read/Write">
<Description>
<![CDATA[Conveyor]]>
</Description>
</Member>
<Member Name="Encoder_Fault" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_V13" BitNumber="1" ExternalAccess="Read/Write">
<Description>
<![CDATA[Encoder Faulted or Conveyor is Running at Low Speed]]>
</Description>
</Member>
<Member Name="Speed_FPM" DataType="DINT" Dimension="0" Radix="Decimal" Hidden="false" ExternalAccess="Read/Write">
<Description>
<![CDATA[Speed in Feet per Minute]]>
</Description>
</Member>
</Members>
</DataType>
<DataType Use="Target" Name="UDT_CTRL_VFD_STS" Family="NoFamily" Class="User">
<Members>
<Member Name="ZZZZZZZZZZUDT_CTRL_V0" DataType="SINT" Dimension="0" Radix="Decimal" Hidden="true" ExternalAccess="Read/Write"/>
<Member Name="Running" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_V0" BitNumber="0" ExternalAccess="Read/Write">
<Description>
<![CDATA[Running]]>
</Description>
</Member>
<Member Name="VFD_Fault" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_V0" BitNumber="1" ExternalAccess="Read/Write">
<Description>
<![CDATA[VFD Faulted]]>
</Description>
</Member>
<Member Name="Communication_Fault" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_V0" BitNumber="2" ExternalAccess="Read/Write">
<Description>
<![CDATA[Ethernet Communicationb Faulted]]>
</Description>
</Member>
<Member Name="Interlock" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_V0" BitNumber="3" ExternalAccess="Read/Write">
<Description>
<![CDATA[Downstream Conveyor is Running]]>
</Description>
</Member>
<Member Name="Current_Speed" DataType="DINT" Dimension="0" Radix="Decimal" Hidden="false" ExternalAccess="Read/Write">
<Description>
<![CDATA[Current Speed of Conveyor in FPM]]>
</Description>
</Member>
<Member Name="Requested_Speed" DataType="DINT" Dimension="0" Radix="Decimal" Hidden="false" ExternalAccess="Read/Write">
<Description>
<![CDATA[Requested Speed of Conveyor in FPM]]>
</Description>
</Member>
<Member Name="ZZZZZZZZZZUDT_CTRL_V7" DataType="SINT" Dimension="0" Radix="Decimal" Hidden="true" ExternalAccess="Read/Write"/>
<Member Name="In_Power_Saving_Mode" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_V7" BitNumber="0" ExternalAccess="Read/Write">
<Description>
<![CDATA[In Power Saving Mode]]>
</Description>
</Member>
<Member Name="Maintenance_Mode" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_V7" BitNumber="1" ExternalAccess="Read/Write">
<Description>
<![CDATA[In Maintenance Mode]]>
</Description>
</Member>
<Member Name="MCM_Started" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_V7" BitNumber="2" ExternalAccess="Read/Write">
<Description>
<![CDATA[MCM Started]]>
</Description>
</Member>
<Member Name="EStopped" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_V7" BitNumber="3" ExternalAccess="Read/Write">
<Description>
<![CDATA[Conveyor Emergency Stopped]]>
</Description>
</Member>
<Member Name="Jammed" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_V7" BitNumber="4" ExternalAccess="Read/Write">
<Description>
<![CDATA[Conveyor]]>
</Description>
</Member>
<Member Name="Full" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_V7" BitNumber="5" ExternalAccess="Read/Write">
<Description>
<![CDATA[Conveyor]]>
</Description>
</Member>
<Member Name="Enabled" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_V7" BitNumber="6" ExternalAccess="Read/Write">
<Description>
<![CDATA[Conveyor]]>
</Description>
</Member>
<Member Name="Local_Stopped" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_V7" BitNumber="7" ExternalAccess="Read/Write">
<Description>
<![CDATA[Conveyor is Stopped Locally]]>
</Description>
</Member>
<Member Name="Log" DataType="STRING" Dimension="0" Radix="NullType" Hidden="false" ExternalAccess="Read/Write">
<Description>
<![CDATA[Log]]>
</Description>
</Member>
<Member Name="ZZZZZZZZZZUDT_CTRL_V17" DataType="SINT" Dimension="0" Radix="Decimal" Hidden="true" ExternalAccess="Read/Write"/>
<Member Name="Encoder_Fault" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_V17" BitNumber="0" ExternalAccess="Read/Write">
<Description>
<![CDATA[Encoder Faulted or Conveyor is Running at Low Speed]]>
</Description>
</Member>
<Member Name="MCM_JR_PB_Pressed" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_V17" BitNumber="1" ExternalAccess="Read/Write">
<Description>
<![CDATA[Jam Reset PushButton Pressed on MCM]]>
</Description>
</Member>
<Member Name="Disabled" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_V17" BitNumber="2" ExternalAccess="Read/Write">
<Description>
<![CDATA[Conveyor]]>
</Description>
</Member>
<Member Name="MCM_Start_PB_Pressed" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_V17" BitNumber="3" ExternalAccess="Read/Write">
<Description>
<![CDATA[Start PushButton Pressed on MCM]]>
</Description>
</Member>
<Member Name="MCM_EStop_PB_Pressed" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_V17" BitNumber="4" ExternalAccess="Read/Write">
<Description>
<![CDATA[Emergency Stop PushButton Pressed on MCM]]>
</Description>
</Member>
</Members>
</DataType>
<DataType Use="Target" Name="UDT_HMI_VFD" Family="NoFamily" Class="User">
<Members>
<Member Name="ALARMST" DataType="DINT" Dimension="0" Radix="Decimal" Hidden="false" ExternalAccess="Read/Write">
<Description>
<![CDATA[Color Animation]]>
</Description>
</Member>
<Member Name="Name" DataType="STRING" Dimension="0" Radix="NullType" Hidden="false" ExternalAccess="Read/Write">
<Description>
<![CDATA[Conveyor Name]]>
</Description>
</Member>
<Member Name="MCM_Name" DataType="STRING" Dimension="0" Radix="NullType" Hidden="false" ExternalAccess="Read/Write">
<Description>
<![CDATA[MCM Name]]>
</Description>
</Member>
<Member Name="IP_Address" DataType="STRING" Dimension="0" Radix="NullType" Hidden="false" ExternalAccess="Read/Write">
<Description>
<![CDATA[IP Address]]>
</Description>
</Member>
<Member Name="Alarm" DataType="UDT_ALARMS_VFD" Dimension="0" Radix="NullType" Hidden="false" ExternalAccess="Read/Write">
<Description>
<![CDATA[VFD Alarms]]>
</Description>
</Member>
<Member Name="STATE" DataType="DINT" Dimension="0" Radix="Decimal" Hidden="false" ExternalAccess="Read/Write">
<Description>
<![CDATA[Color Animation]]>
</Description>
</Member>
<Member Name="ZZZZZZZZZZUDT_HMI_VF6" DataType="SINT" Dimension="0" Radix="Decimal" Hidden="true" ExternalAccess="Read/Write"/>
<Member Name="Maintenance_Start_PB_Pressed" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_HMI_VF6" BitNumber="0" ExternalAccess="Read/Write">
<Description>
<![CDATA[Maintenance Mode Start PushButton
Pressed]]>
</Description>
</Member>
<Member Name="Maintenance_Stop_PB_Pressed" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_HMI_VF6" BitNumber="1" ExternalAccess="Read/Write">
<Description>
<![CDATA[Maintenance Mode Stop PushButton Pressed]]>
</Description>
</Member>
<Member Name="Maintenance_Jog_PB_Pressed" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_HMI_VF6" BitNumber="2" ExternalAccess="Read/Write">
<Description>
<![CDATA[Maintenance Mode Jog PushButton Pressed]]>
</Description>
</Member>
<Member Name="Maintenance_Direction_PB_Pressed" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_HMI_VF6" BitNumber="3" ExternalAccess="Read/Write">
<Description>
<![CDATA[Conveyor Direction Command Toggle Button Pressed]]>
</Description>
</Member>
<Member Name="Maintenance_Conveyor_Run_LT" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_HMI_VF6" BitNumber="4" ExternalAccess="Read/Write">
<Description>
<![CDATA[Light when Conveyor is Running]]>
</Description>
</Member>
<Member Name="Maintenance_Stop_LT" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_HMI_VF6" BitNumber="5" ExternalAccess="Read/Write">
<Description>
<![CDATA[Light when Conveyor is Running]]>
</Description>
</Member>
<Member Name="Maintenance_Jog_LT" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_HMI_VF6" BitNumber="6" ExternalAccess="Read/Write">
<Description>
<![CDATA[Light when Maintenance in Jog Mode]]>
</Description>
</Member>
<Member Name="Maintenance_Direction_LT" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_HMI_VF6" BitNumber="7" ExternalAccess="Read/Write">
<Description>
<![CDATA[Light Direction indicator of Maintenance]]>
</Description>
</Member>
<Member Name="Speed_At_60Hz" DataType="DINT" Dimension="0" Radix="Decimal" Hidden="false" ExternalAccess="Read/Write">
<Description>
<![CDATA[Speed of Conveyor at 60hz frequency to calculate ratio]]>
</Description>
</Member>
<Member Name="Maintenance_Conveyor_Speed" DataType="DINT" Dimension="0" Radix="Decimal" Hidden="false" ExternalAccess="Read/Write">
<Description>
<![CDATA[Speed Of Conveyor In Maintenance Mode]]>
</Description>
</Member>
<Member Name="Amperage" DataType="INT" Dimension="0" Radix="Decimal" Hidden="false" ExternalAccess="Read/Write">
<Description>
<![CDATA[Output Amperage]]>
</Description>
</Member>
<Member Name="Voltage" DataType="INT" Dimension="0" Radix="Decimal" Hidden="false" ExternalAccess="Read/Write">
<Description>
<![CDATA[Output Voltage]]>
</Description>
</Member>
<Member Name="Frequency" DataType="INT" Dimension="0" Radix="Decimal" Hidden="false" ExternalAccess="Read/Write">
<Description>
<![CDATA[Output Frequency]]>
</Description>
</Member>
<Member Name="FPM" DataType="INT" Dimension="0" Radix="Decimal" Hidden="false" ExternalAccess="Read/Write">
<Description>
<![CDATA[Conveyor FPM]]>
</Description>
</Member>
<Member Name="Speed" DataType="DINT" Dimension="0" Radix="Decimal" Hidden="false" ExternalAccess="Read/Write">
<Description>
<![CDATA[Adjustable Full Speed from SCADA]]>
</Description>
</Member>
<Member Name="Communication_Fault_Code" DataType="DINT" Dimension="0" Radix="Decimal" Hidden="false" ExternalAccess="Read/Write">
<Description>
<![CDATA[VFD Ethernet Communication Fault Code]]>
</Description>
</Member>
<Member Name="VFD_Fault_Code" DataType="DINT" Dimension="0" Radix="Decimal" Hidden="false" ExternalAccess="Read/Write">
<Description>
<![CDATA[VFD Fault Code]]>
</Description>
</Member>
<Member Name="Last_VFD_Fault_Code" DataType="DINT" Dimension="0" Radix="Decimal" Hidden="false" ExternalAccess="Read/Write">
<Description>
<![CDATA[Last VFD Fault Code]]>
</Description>
</Member>
<Member Name="ZZZZZZZZZZUDT_HMI_VF25" DataType="SINT" Dimension="0" Radix="Decimal" Hidden="true" ExternalAccess="Read/Write"/>
<Member Name="Maintenance_Mode" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_HMI_VF25" BitNumber="0" ExternalAccess="Read/Write">
<Description>
<![CDATA[Maint Mode Activated]]>
</Description>
</Member>
<Member Name="Power_Save_Time" DataType="DINT" Dimension="0" Radix="Decimal" Hidden="false" ExternalAccess="Read/Write"/>
<Member Name="ZZZZZZZZZZUDT_HMI_VF28" DataType="SINT" Dimension="0" Radix="Decimal" Hidden="true" ExternalAccess="Read/Write"/>
<Member Name="Maintenance_Bypas_PB" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_HMI_VF28" BitNumber="0" ExternalAccess="Read/Write"/>
<Member Name="Maintenance_Bypas_PB_LT" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_HMI_VF28" BitNumber="1" ExternalAccess="Read/Write"/>
<Member Name="VFD_Status" DataType="DINT" Dimension="0" Radix="Decimal" Hidden="false" ExternalAccess="Read/Write"/>
<Member Name="DISC" DataType="DINT" Dimension="0" Radix="Decimal" Hidden="false" ExternalAccess="Read/Write">
<Description>
<![CDATA[Color Animation]]>
</Description>
</Member>
</Members>
<Dependencies>
<Dependency Type="DataType" Name="UDT_ALARMS_VFD"/>
</Dependencies>
</DataType>
</DataTypes>
<AddOnInstructionDefinitions Use="Context">
<AddOnInstructionDefinition Name="AOI_VFD" Revision="1.0" ExecutePrescan="false" ExecutePostscan="false" ExecuteEnableInFalse="false" CreatedDate="2025-05-17T10:35:36.642Z" CreatedBy="LCIBATUMI\gigi.mamaladze" EditedDate="2025-05-24T19:23:40.942Z" EditedBy="LCIBATUMI\ilia.gurielidze" SoftwareRevision="v36.00">
<Description>
<![CDATA[Varible Frequency Drive]]>
</Description>
<Parameters>
<Parameter Name="EnableIn" TagType="Base" DataType="BOOL" Usage="Input" Radix="Decimal" Required="false" Visible="false" ExternalAccess="Read Only">
<Description>
<![CDATA[Enable Input - System Defined Parameter]]>
</Description>
</Parameter>
<Parameter Name="EnableOut" TagType="Base" DataType="BOOL" Usage="Output" Radix="Decimal" Required="false" Visible="false" ExternalAccess="Read Only">
<Description>
<![CDATA[Enable Output - System Defined Parameter]]>
</Description>
</Parameter>
<Parameter Name="HMI" TagType="Base" DataType="UDT_HMI_VFD" Usage="InOut" Required="true" Visible="true" Constant="false"/>
<Parameter Name="CTRL" TagType="Base" DataType="UDT_CTRL_VFD" Usage="InOut" Required="true" Visible="true" Constant="false"/>
<Parameter Name="Module" TagType="Base" DataType="MODULE" Usage="InOut" Required="true" Visible="true"/>
<Parameter Name="InVFD" TagType="Base" DataType="AB:PowerFlex525V_E_142E84CE:I:0" Usage="InOut" Required="true" Visible="true" Constant="false"/>
<Parameter Name="OutVFD" TagType="Base" DataType="AB:PowerFlex525V_EENET_Drive:O:0" Usage="InOut" Required="true" Visible="true" Constant="false"/>
<Parameter Name="MCM" TagType="Base" DataType="UDT_CTRL_MCM" Usage="InOut" Required="true" Visible="true" Constant="false"/>
<Parameter Name="FIO" TagType="Base" DataType="UDT_CTRL_SIO_FIO" Usage="InOut" Required="true" Visible="true" Constant="false"/>
<Parameter Name="In_EStopped" TagType="Base" DataType="BOOL" Usage="Input" Radix="Decimal" Required="true" Visible="true" ExternalAccess="Read/Write">
<Description>
<![CDATA[VFD Emergency Stopped]]>
</Description>
<DefaultData Format="L5K">
<![CDATA[0]]>
</DefaultData>
<DefaultData Format="Decorated">
<DataValue DataType="BOOL" Radix="Decimal" Value="0"/>
</DefaultData>
</Parameter>
<Parameter Name="In_Communication_Fault" TagType="Base" DataType="BOOL" Usage="Input" Radix="Decimal" Required="true" Visible="true" ExternalAccess="Read/Write">
<Description>
<![CDATA[Ethernet Communication Fault(NC)]]>
</Description>
<DefaultData Format="L5K">
<![CDATA[0]]>
</DefaultData>
<DefaultData Format="Decorated">
<DataValue DataType="BOOL" Radix="Decimal" Value="0"/>
</DefaultData>
</Parameter>
<Parameter Name="In_Disconnect" TagType="Base" DataType="BOOL" Usage="Input" Radix="Decimal" Required="true" Visible="true" ExternalAccess="Read/Write">
<Description>
<![CDATA[VFD Disconnected]]>
</Description>
<DefaultData Format="L5K">
<![CDATA[0]]>
</DefaultData>
<DefaultData Format="Decorated">
<DataValue DataType="BOOL" Radix="Decimal" Value="0"/>
</DefaultData>
</Parameter>
<Parameter Name="Running" TagType="Base" DataType="BOOL" Usage="Output" Radix="Decimal" Required="false" Visible="false" ExternalAccess="Read/Write">
<Description>
<![CDATA[Conveyor Running]]>
</Description>
<DefaultData Format="L5K">
<![CDATA[0]]>
</DefaultData>
<DefaultData Format="Decorated">
<DataValue DataType="BOOL" Radix="Decimal" Value="0"/>
</DefaultData>
</Parameter>
<Parameter Name="Run_Enabled" TagType="Base" DataType="BOOL" Usage="Output" Radix="Decimal" Required="false" Visible="false" ExternalAccess="Read/Write">
<Description>
<![CDATA[Conveyor Run Enabled]]>
</Description>
<DefaultData Format="L5K">
<![CDATA[1]]>
</DefaultData>
<DefaultData Format="Decorated">
<DataValue DataType="BOOL" Radix="Decimal" Value="1"/>
</DefaultData>
</Parameter>
<Parameter Name="Run" TagType="Base" DataType="BOOL" Usage="Output" Radix="Decimal" Required="false" Visible="false" ExternalAccess="Read/Write">
<Description>
<![CDATA[Conveyor Command Run]]>
</Description>
<DefaultData Format="L5K">
<![CDATA[0]]>
</DefaultData>
<DefaultData Format="Decorated">
<DataValue DataType="BOOL" Radix="Decimal" Value="0"/>
</DefaultData>
</Parameter>
<Parameter Name="Maintenance_Running" TagType="Base" DataType="BOOL" Usage="Output" Radix="Decimal" Required="false" Visible="false" ExternalAccess="Read/Write">
<Description>
<![CDATA[Conveyor Maintenance Running]]>
</Description>
<DefaultData Format="L5K">
<![CDATA[0]]>
</DefaultData>
<DefaultData Format="Decorated">
<DataValue DataType="BOOL" Radix="Decimal" Value="0"/>
</DefaultData>
</Parameter>
<Parameter Name="Jammed" TagType="Base" DataType="BOOL" Usage="Output" Radix="Decimal" Required="false" Visible="true" ExternalAccess="Read/Write">
<Description>
<![CDATA[Conveyor Jammed]]>
</Description>
<DefaultData Format="L5K">
<![CDATA[0]]>
</DefaultData>
<DefaultData Format="Decorated">
<DataValue DataType="BOOL" Radix="Decimal" Value="0"/>
</DefaultData>
</Parameter>
<Parameter Name="EStopped" TagType="Base" DataType="BOOL" Usage="Output" Radix="Decimal" Required="false" Visible="true" ExternalAccess="Read/Write">
<Description>
<![CDATA[VFD Emergency Stopped]]>
</Description>
<DefaultData Format="L5K">
<![CDATA[0]]>
</DefaultData>
<DefaultData Format="Decorated">
<DataValue DataType="BOOL" Radix="Decimal" Value="0"/>
</DefaultData>
</Parameter>
<Parameter Name="Disabled" TagType="Base" DataType="BOOL" Usage="Output" Radix="Decimal" Required="false" Visible="true" ExternalAccess="Read Only">
<Description>
<![CDATA[Conveyor Disabled]]>
</Description>
<DefaultData Format="L5K">
<![CDATA[0]]>
</DefaultData>
<DefaultData Format="Decorated">
<DataValue DataType="BOOL" Radix="Decimal" Value="0"/>
</DefaultData>
</Parameter>
<Parameter Name="Speed_Not_Set_Up" TagType="Base" DataType="BOOL" Usage="Output" Radix="Decimal" Required="false" Visible="true" ExternalAccess="None">
<Description>
<![CDATA[Conveyor Speed No Set Up]]>
</Description>
<DefaultData Format="L5K">
<![CDATA[0]]>
</DefaultData>
<DefaultData Format="Decorated">
<DataValue DataType="BOOL" Radix="Decimal" Value="0"/>
</DefaultData>
</Parameter>
<Parameter Name="Motor_Fault_Latch" TagType="Base" DataType="BOOL" Usage="Output" Radix="Decimal" Required="false" Visible="true" ExternalAccess="None">
<Description>
<![CDATA[Motor Faulted]]>
</Description>
<DefaultData Format="L5K">
<![CDATA[0]]>
</DefaultData>
<DefaultData Format="Decorated">
<DataValue DataType="BOOL" Radix="Decimal" Value="0"/>
</DefaultData>
</Parameter>
<Parameter Name="Motor_Faulted" TagType="Base" DataType="BOOL" Usage="Output" Radix="Decimal" Required="false" Visible="true" ExternalAccess="Read/Write">
<Description>
<![CDATA[Motor Faulted]]>
</Description>
<DefaultData Format="L5K">
<![CDATA[0]]>
</DefaultData>
<DefaultData Format="Decorated">
<DataValue DataType="BOOL" Radix="Decimal" Value="0"/>
</DefaultData>
</Parameter>
<Parameter Name="Safety_Torque_Off" TagType="Base" DataType="BOOL" Usage="Output" Radix="Decimal" Required="false" Visible="true" ExternalAccess="Read/Write">
<Description>
<![CDATA[Loose Wire / Internal Relay Fault.]]>
</Description>
<DefaultData Format="L5K">
<![CDATA[0]]>
</DefaultData>
<DefaultData Format="Decorated">
<DataValue DataType="BOOL" Radix="Decimal" Value="0"/>
</DefaultData>
</Parameter>
<Parameter Name="Communication_Fault" TagType="Base" DataType="BOOL" Usage="Output" Radix="Decimal" Required="false" Visible="true" ExternalAccess="None">
<Description>
<![CDATA[Ethernet Communication Fault]]>
</Description>
<DefaultData Format="L5K">
<![CDATA[0]]>
</DefaultData>
<DefaultData Format="Decorated">
<DataValue DataType="BOOL" Radix="Decimal" Value="0"/>
</DefaultData>
</Parameter>
<Parameter Name="Disconnected" TagType="Base" DataType="BOOL" Usage="Output" Radix="Decimal" Required="false" Visible="true" ExternalAccess="None">
<Description>
<![CDATA[VFD Disconnected]]>
</Description>
<DefaultData Format="L5K">
<![CDATA[0]]>
</DefaultData>
<DefaultData Format="Decorated">
<DataValue DataType="BOOL" Radix="Decimal" Value="0"/>
</DefaultData>
</Parameter>
<Parameter Name="Power_Saving_Mode" TagType="Base" DataType="BOOL" Usage="Output" Radix="Decimal" Required="false" Visible="true" ExternalAccess="Read/Write">
<Description>
<![CDATA[Conveyor is Running in Power Saving Moder]]>
</Description>
<DefaultData Format="L5K">
<![CDATA[0]]>
</DefaultData>
<DefaultData Format="Decorated">
<DataValue DataType="BOOL" Radix="Decimal" Value="0"/>
</DefaultData>
</Parameter>
<Parameter Name="Start_Conveyor" TagType="Base" DataType="BOOL" Usage="Output" Radix="Decimal" Required="false" Visible="false" ExternalAccess="Read Only">
<Description>
<![CDATA[Start Conveyor]]>
</Description>
<DefaultData Format="L5K">
<![CDATA[0]]>
</DefaultData>
<DefaultData Format="Decorated">
<DataValue DataType="BOOL" Radix="Decimal" Value="0"/>
</DefaultData>
</Parameter>
<Parameter Name="Speed_To_HZ_Ratio" TagType="Base" DataType="REAL" Usage="Output" Radix="Float" Required="false" Visible="false" ExternalAccess="Read/Write">
<Description>
<![CDATA[Conveyor speed-to-frequency ratio for VFD control]]>
</Description>
<DefaultData Format="L5K">
<![CDATA[0.00000000e+000]]>
</DefaultData>
<DefaultData Format="Decorated">
<DataValue DataType="REAL" Radix="Float" Value="0.0"/>
</DefaultData>
</Parameter>
<Parameter Name="Maintenance_Mode" TagType="Base" DataType="BOOL" Usage="Output" Radix="Decimal" Required="false" Visible="true" ExternalAccess="Read/Write">
<Description>
<![CDATA[Maintenance Mode]]>
</Description>
<DefaultData Format="L5K">
<![CDATA[0]]>
</DefaultData>
<DefaultData Format="Decorated">
<DataValue DataType="BOOL" Radix="Decimal" Value="0"/>
</DefaultData>
</Parameter>
<Parameter Name="Stopped_By_Station_PB" TagType="Base" DataType="BOOL" Usage="Output" Radix="Decimal" Required="false" Visible="true" ExternalAccess="Read Only">
<Description>
<![CDATA[Conveyor Stopped by Station PushButton]]>
</Description>
<DefaultData Format="L5K">
<![CDATA[0]]>
</DefaultData>
<DefaultData Format="Decorated">
<DataValue DataType="BOOL" Radix="Decimal" Value="0"/>
</DefaultData>
</Parameter>
<Parameter Name="Full" TagType="Base" DataType="BOOL" Usage="Output" Radix="Decimal" Required="false" Visible="true" ExternalAccess="Read Only">
<Description>
<![CDATA[Conveyor Full]]>
</Description>
<DefaultData Format="L5K">
<![CDATA[0]]>
</DefaultData>
<DefaultData Format="Decorated">
<DataValue DataType="BOOL" Radix="Decimal" Value="0"/>
</DefaultData>
</Parameter>
<Parameter Name="Encoder_Fault" TagType="Base" DataType="BOOL" Usage="Output" Radix="Decimal" Required="false" Visible="true" ExternalAccess="Read Only">
<Description>
<![CDATA[Encoder Faulted or Conveyor is Running at Low Speed]]>
</Description>
<DefaultData Format="L5K">
<![CDATA[0]]>
</DefaultData>
<DefaultData Format="Decorated">
<DataValue DataType="BOOL" Radix="Decimal" Value="0"/>
</DefaultData>
</Parameter>
<Parameter Name="Stopped_Require_Start" TagType="Base" DataType="BOOL" Usage="Output" Radix="Decimal" Required="false" Visible="true" ExternalAccess="Read Only">
<Description>
<![CDATA[Stopped Conveyor and Require Start]]>
</Description>
<DefaultData Format="L5K">
<![CDATA[0]]>
</DefaultData>
<DefaultData Format="Decorated">
<DataValue DataType="BOOL" Radix="Decimal" Value="0"/>
</DefaultData>
</Parameter>
<Parameter Name="Stopped_Auto_Restart" TagType="Base" DataType="BOOL" Usage="Output" Radix="Decimal" Required="false" Visible="true" ExternalAccess="Read Only">
<Description>
<![CDATA[Stopped Conveyor and Will Automaticly Restart]]>
</Description>
<DefaultData Format="L5K">
<![CDATA[0]]>
</DefaultData>
<DefaultData Format="Decorated">
<DataValue DataType="BOOL" Radix="Decimal" Value="0"/>
</DefaultData>
</Parameter>
<Parameter Name="Zero_Speed" TagType="Base" DataType="BOOL" Usage="Output" Radix="Decimal" Required="false" Visible="true" ExternalAccess="Read Only">
<Description>
<![CDATA[Conveyor Speed is Zero]]>
</Description>
<DefaultData Format="L5K">
<![CDATA[0]]>
</DefaultData>
<DefaultData Format="Decorated">
<DataValue DataType="BOOL" Radix="Decimal" Value="0"/>
</DefaultData>
</Parameter>
<Parameter Name="No_Interlock" TagType="Base" DataType="BOOL" Usage="Output" Radix="Decimal" Required="false" Visible="true" ExternalAccess="Read/Write">
<Description>
<![CDATA[No Interlock]]>
</Description>
<DefaultData Format="L5K">
<![CDATA[0]]>
</DefaultData>
<DefaultData Format="Decorated">
<DataValue DataType="BOOL" Radix="Decimal" Value="0"/>
</DefaultData>
</Parameter>
<Parameter Name="MCM_Not_Started" TagType="Base" DataType="BOOL" Usage="Output" Radix="Decimal" Required="false" Visible="true" ExternalAccess="Read Only">
<Description>
<![CDATA[MCM Not Started]]>
</Description>
<DefaultData Format="L5K">
<![CDATA[0]]>
</DefaultData>
<DefaultData Format="Decorated">
<DataValue DataType="BOOL" Radix="Decimal" Value="0"/>
</DefaultData>
</Parameter>
</Parameters>
<LocalTags>
<LocalTag Name="Start_Delay_Timmer" DataType="TIMER" ExternalAccess="None">
<Description>
<![CDATA[Conveyor will Start after Timer is Done]]>
</Description>
<DefaultData Format="L5K">
<![CDATA[[0,5000,0]]]>
</DefaultData>
<DefaultData Format="Decorated">
<Structure DataType="TIMER">
<DataValueMember Name="PRE" DataType="DINT" Radix="Decimal" Value="5000"/>
<DataValueMember Name="ACC" DataType="DINT" Radix="Decimal" Value="0"/>
<DataValueMember Name="EN" DataType="BOOL" Value="0"/>
<DataValueMember Name="TT" DataType="BOOL" Value="0"/>
<DataValueMember Name="DN" DataType="BOOL" Value="0"/>
</Structure>
</DefaultData>
</LocalTag>
<LocalTag Name="Maintenance_Start_Conveyor" DataType="BOOL" Radix="Decimal" ExternalAccess="None">
<Description>
<![CDATA[Start Conveyor in Maintenance Mode]]>
</Description>
<DefaultData Format="L5K">
<![CDATA[0]]>
</DefaultData>
<DefaultData Format="Decorated">
<DataValue DataType="BOOL" Radix="Decimal" Value="0"/>
</DefaultData>
</LocalTag>
<LocalTag Name="Start_ONS" DataType="BOOL" Radix="Decimal" ExternalAccess="None">
<Description>
<![CDATA[Start to allow local control of the conveyor]]>
</Description>
<DefaultData Format="L5K">
<![CDATA[0]]>
</DefaultData>
<DefaultData Format="Decorated">
<DataValue DataType="BOOL" Radix="Decimal" Value="0"/>
</DefaultData>
</LocalTag>
<LocalTag Name="Frequency_Command" DataType="REAL" Radix="Float" ExternalAccess="None">
<Description>
<![CDATA[Frequency Command to Motor]]>
</Description>
<DefaultData Format="L5K">
<![CDATA[0.00000000e+000]]>
</DefaultData>
<DefaultData Format="Decorated">
<DataValue DataType="REAL" Radix="Float" Value="0.0"/>
</DefaultData>
</LocalTag>
<LocalTag Name="Safe_Off_Delay" DataType="TIMER" ExternalAccess="None">
<Description>
<![CDATA[VFD Safe off will be reported after Timer is Done]]>
</Description>
<DefaultData Format="L5K">
<![CDATA[[0,2000,0]]]>
</DefaultData>
<DefaultData Format="Decorated">
<Structure DataType="TIMER">
<DataValueMember Name="PRE" DataType="DINT" Radix="Decimal" Value="2000"/>
<DataValueMember Name="ACC" DataType="DINT" Radix="Decimal" Value="0"/>
<DataValueMember Name="EN" DataType="BOOL" Value="0"/>
<DataValueMember Name="TT" DataType="BOOL" Value="0"/>
<DataValueMember Name="DN" DataType="BOOL" Value="0"/>
</Structure>
</DefaultData>
</LocalTag>
<LocalTag Name="Power_Save_Time_Ms" DataType="DINT" Radix="Decimal" ExternalAccess="None">
<Description>
<![CDATA[Power Save Time in Milliseconds]]>
</Description>
<DefaultData Format="L5K">
<![CDATA[0]]>
</DefaultData>
<DefaultData Format="Decorated">
<DataValue DataType="DINT" Radix="Decimal" Value="0"/>
</DefaultData>
</LocalTag>
<LocalTag Name="Power_Save_Timer" DataType="TIMER" ExternalAccess="None">
<Description>
<![CDATA[Power Saving Timer]]>
</Description>
<DefaultData Format="L5K">
<![CDATA[[0,0,0]]]>
</DefaultData>
<DefaultData Format="Decorated">
<Structure DataType="TIMER">
<DataValueMember Name="PRE" DataType="DINT" Radix="Decimal" Value="0"/>
<DataValueMember Name="ACC" DataType="DINT" Radix="Decimal" Value="0"/>
<DataValueMember Name="EN" DataType="BOOL" Value="0"/>
<DataValueMember Name="TT" DataType="BOOL" Value="0"/>
<DataValueMember Name="DN" DataType="BOOL" Value="0"/>
</Structure>
</DefaultData>
</LocalTag>
<LocalTag Name="VFD_Fault_Code" DataType="DINT" Radix="Decimal" ExternalAccess="None">
<Description>
<![CDATA[VFD Fault Code]]>
</Description>
<DefaultData Format="L5K">
<![CDATA[0]]>
</DefaultData>
<DefaultData Format="Decorated">
<DataValue DataType="DINT" Radix="Decimal" Value="0"/>
</DefaultData>
</LocalTag>
<LocalTag Name="Maintenance_Conveyor_Direction" DataType="BOOL" Radix="Decimal" ExternalAccess="None">
<Description>
<![CDATA[0-Forward 
1-Reverse]]>
</Description>
<DefaultData Format="L5K">
<![CDATA[0]]>
</DefaultData>
<DefaultData Format="Decorated">
<DataValue DataType="BOOL" Radix="Decimal" Value="0"/>
</DefaultData>
</LocalTag>
<LocalTag Name="Last_Motor_Fault_Code" DataType="DINT" Radix="Decimal" ExternalAccess="None">
<Description>
<![CDATA[Last Motor Fault Code]]>
</Description>
<DefaultData Format="L5K">
<![CDATA[0]]>
</DefaultData>
<DefaultData Format="Decorated">
<DataValue DataType="DINT" Radix="Decimal" Value="0"/>
</DefaultData>
</LocalTag>
<LocalTag Name="Maintenance_Jog_Mode" DataType="BOOL" Radix="Decimal" ExternalAccess="None">
<Description>
<![CDATA[Conveyor in Jog Mode]]>
</Description>
<DefaultData Format="L5K">
<![CDATA[0]]>
</DefaultData>
<DefaultData Format="Decorated">
<DataValue DataType="BOOL" Radix="Decimal" Value="0"/>
</DefaultData>
</LocalTag>
<LocalTag Name="Jammed_Latch" DataType="BOOL" Radix="Decimal" ExternalAccess="None">
<Description>
<![CDATA[Conveyor Jammed]]>
</Description>
<DefaultData Format="L5K">
<![CDATA[0]]>
</DefaultData>
<DefaultData Format="Decorated">
<DataValue DataType="BOOL" Radix="Decimal" Value="0"/>
</DefaultData>
</LocalTag>
<LocalTag Name="Interlock" DataType="BOOL" Radix="Decimal" ExternalAccess="Read/Write">
<Description>
<![CDATA[Interlock]]>
</Description>
<DefaultData Format="L5K">
<![CDATA[0]]>
</DefaultData>
<DefaultData Format="Decorated">
<DataValue DataType="BOOL" Radix="Decimal" Value="0"/>
</DefaultData>
</LocalTag>
<LocalTag Name="Disconect_On_Delay" DataType="TIMER" ExternalAccess="None">
<Description>
<![CDATA[Conveyor will be interpreted as Disconnected after Timer is Done]]>
</Description>
<DefaultData Format="L5K">
<![CDATA[[0,45000,0]]]>
</DefaultData>
<DefaultData Format="Decorated">
<Structure DataType="TIMER">
<DataValueMember Name="PRE" DataType="DINT" Radix="Decimal" Value="45000"/>
<DataValueMember Name="ACC" DataType="DINT" Radix="Decimal" Value="0"/>
<DataValueMember Name="EN" DataType="BOOL" Value="0"/>
<DataValueMember Name="TT" DataType="BOOL" Value="0"/>
<DataValueMember Name="DN" DataType="BOOL" Value="0"/>
</Structure>
</DefaultData>
</LocalTag>
<LocalTag Name="Direction" DataType="BOOL" Radix="Decimal" ExternalAccess="None">
<Description>
<![CDATA[Conveyor Direction in Maintance Mode]]>
</Description>
<DefaultData Format="L5K">
<![CDATA[0]]>
</DefaultData>
<DefaultData Format="Decorated">
<DataValue DataType="BOOL" Radix="Decimal" Value="0"/>
</DefaultData>
</LocalTag>
<LocalTag Name="Concatenated_String" DataType="STRING" ExternalAccess="None">
<Description>
<![CDATA[String for Logs]]>
</Description>
<DefaultData Format="L5K">
<![CDATA[[0,'$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00']]]>
</DefaultData>
<DefaultData Format="String" Length="0">
<![CDATA['']]>
</DefaultData>
</LocalTag>
<LocalTag Name="Communication_Lost" DataType="BOOL" Radix="Decimal" ExternalAccess="None">
<Description>
<![CDATA[Ethernet Communication Lost]]>
</Description>
<DefaultData Format="L5K">
<![CDATA[0]]>
</DefaultData>
<DefaultData Format="Decorated">
<DataValue DataType="BOOL" Radix="Decimal" Value="0"/>
</DefaultData>
</LocalTag>
<LocalTag Name="Communication_Fault_Code" DataType="DINT" Radix="Decimal" ExternalAccess="None">
<Description>
<![CDATA[Ethernet Communication Fault Code]]>
</Description>
<DefaultData Format="L5K">
<![CDATA[0]]>
</DefaultData>
<DefaultData Format="Decorated">
<DataValue DataType="DINT" Radix="Decimal" Value="0"/>
</DefaultData>
</LocalTag>
<LocalTag Name="Communication_Fault_Latch" DataType="BOOL" Radix="Decimal" ExternalAccess="None">
<Description>
<![CDATA[Ethernet Communication Faulted]]>
</Description>
<DefaultData Format="L5K">
<![CDATA[0]]>
</DefaultData>
<DefaultData Format="Decorated">
<DataValue DataType="BOOL" Radix="Decimal" Value="0"/>
</DefaultData>
</LocalTag>
<LocalTag Name="Acknowledge_ONS" DataType="DINT" Radix="Decimal" ExternalAccess="None">
<Description>
<![CDATA[{{TODO}}]]>
</Description>
<DefaultData Format="L5K">
<![CDATA[0]]>
</DefaultData>
<DefaultData Format="Decorated">
<DataValue DataType="DINT" Radix="Decimal" Value="0"/>
</DefaultData>
</LocalTag>
<LocalTag Name="Acknowledge" DataType="DINT" Radix="Decimal" ExternalAccess="None">
<Description>
<![CDATA[Acknowledge Logs]]>
</Description>
<DefaultData Format="L5K">
<![CDATA[0]]>
</DefaultData>
<DefaultData Format="Decorated">
<DataValue DataType="DINT" Radix="Decimal" Value="0"/>
</DefaultData>
</LocalTag>
<LocalTag Name="Starting_String" DataType="STRING" ExternalAccess="None">
<Description>
<![CDATA[String contains " STARTING"]]>
</Description>
<DefaultData Format="L5K">
<![CDATA[[9,' STARTING$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00']]]>
</DefaultData>
<DefaultData Format="String" Length="9">
<![CDATA[' STARTING']]>
</DefaultData>
</LocalTag>
<LocalTag Name="Disconnect_Off_String" DataType="STRING" ExternalAccess="None">
<Description>
<![CDATA[String contains " DISC OFF"]]>
</Description>
<DefaultData Format="L5K">
<![CDATA[[0,'$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00']]]>
</DefaultData>
<DefaultData Format="String" Length="0">
<![CDATA['']]>
</DefaultData>
</LocalTag>
<LocalTag Name="Empty_String" DataType="STRING" ExternalAccess="None">
<Description>
<![CDATA[String contains ""]]>
</Description>
<DefaultData Format="L5K">
<![CDATA[[0,'$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00']]]>
</DefaultData>
<DefaultData Format="String" Length="0">
<![CDATA['']]>
</DefaultData>
</LocalTag>
<LocalTag Name="Motor_Fault_String" DataType="STRING" ExternalAccess="None">
<Description>
<![CDATA[String contains " MTR FLT"]]>
</Description>
<DefaultData Format="L5K">
<![CDATA[[8,' MTR FLT$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00']]]>
</DefaultData>
<DefaultData Format="String" Length="8">
<![CDATA[' MTR FLT']]>
</DefaultData>
</LocalTag>
<LocalTag Name="Safe_Off_String" DataType="STRING" ExternalAccess="None">
<Description>
<![CDATA[String contains " SAFE OFF"]]>
</Description>
<DefaultData Format="L5K">
<![CDATA[[0,'$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00']]]>
</DefaultData>
<DefaultData Format="String" Length="0">
<![CDATA['']]>
</DefaultData>
</LocalTag>
<LocalTag Name="Lost_Comm_String" DataType="STRING" ExternalAccess="None">
<Description>
<![CDATA[String contains " LOST COMM"]]>
</Description>
<DefaultData Format="L5K">
<![CDATA[[0,'$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00']]]>
</DefaultData>
<DefaultData Format="String" Length="0">
<![CDATA['']]>
</DefaultData>
</LocalTag>
<LocalTag Name="Jam_String" DataType="STRING" ExternalAccess="None">
<Description>
<![CDATA[String contains " JAM"]]>
</Description>
<DefaultData Format="L5K">
<![CDATA[[0,'$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00']]]>
</DefaultData>
<DefaultData Format="String" Length="0">
<![CDATA['']]>
</DefaultData>
</LocalTag>
<LocalTag Name="Full_String" DataType="STRING" ExternalAccess="None">
<Description>
<![CDATA[String contains " FULL"]]>
</Description>
<DefaultData Format="L5K">
<![CDATA[[0,'$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00']]]>
</DefaultData>
<DefaultData Format="String" Length="0">
<![CDATA['']]>
</DefaultData>
</LocalTag>
</LocalTags>
<Routines>
<Routine Name="Logic" Type="RLL">
<RLLContent>
<Rung Number="0" Type="N">
<Text>
<![CDATA[COP(CTRL.CMD.Log,CTRL.STS.Log,1);]]>
</Text>
</Rung>
<Rung Number="1" Type="N">
<Text>
<![CDATA[XIO(In_Disconnect)XIO(FIO.STS.Communication_Fault)OTE(Disconnected);]]>
</Text>
</Rung>
<Rung Number="2" Type="N">
<Text>
<![CDATA[XIC(CTRL.CMD.Jammed)OTE(Jammed);]]>
</Text>
</Rung>
<Rung Number="3" Type="N">
<Text>
<![CDATA[XIC(CTRL.CMD.Encoder_Fault)OTE(Encoder_Fault);]]>
</Text>
</Rung>
<Rung Number="4" Type="N">
<Text>
<![CDATA[XIC(CTRL.CMD.Full)OTE(Full);]]>
</Text>
</Rung>
<Rung Number="5" Type="N">
<Text>
<![CDATA[XIC(CTRL.CMD.Stop_Require_Start)OTE(Stopped_Require_Start);]]>
</Text>
</Rung>
<Rung Number="6" Type="N">
<Text>
<![CDATA[XIC(CTRL.CMD.Stop_Auto_Restart)OTE(Stopped_Auto_Restart);]]>
</Text>
</Rung>
<Rung Number="7" Type="N">
<Text>
<![CDATA[EQ(CTRL.CMD.Speed_FPM,0)OTE(Zero_Speed);]]>
</Text>
</Rung>
<Rung Number="8" Type="N">
<Text>
<![CDATA[XIC(EStopped)OTE(CTRL.STS.EStopped);]]>
</Text>
</Rung>
<Rung Number="9" Type="N">
<Text>
<![CDATA[XIO(CTRL.STS.EStopped)OTE(EStopped)OTL(MCM.CMD.EStop_Was_Actuated);]]>
</Text>
</Rung>
<Rung Number="10" Type="N">
<Text>
<![CDATA[XIC(MCM.STS.System_Started)OTE(CTRL.STS.MCM_Started);]]>
</Text>
</Rung>
<Rung Number="11" Type="N">
<Text>
<![CDATA[XIO(MCM.STS.System_Started)OTE(MCM_Not_Started);]]>
</Text>
</Rung>
<Rung Number="12" Type="N">
<Text>
<![CDATA[XIC(HMI.Maintenance_Mode)OTE(CTRL.STS.Maintenance_Mode)OTE(Maintenance_Mode);]]>
</Text>
</Rung>
<Rung Number="13" Type="N">
<Text>
<![CDATA[XIC(In_Disconnect)[TON(Disconect_On_Delay,?,?) ,XIO(Communication_Lost) MOVE(60000,Disconect_On_Delay.ACC) ];]]>
</Text>
</Rung>
<Rung Number="14" Type="N">
<Text>
<![CDATA[GSV(Module,Module,FaultCode,Communication_Fault_Code)NE(Communication_Fault_Code,0)OTE(Communication_Lost);]]>
</Text>
</Rung>
<Rung Number="15" Type="N">
<Text>
<![CDATA[CLR(Communication_Fault_Code)XIC(Disconect_On_Delay.DN)XIO(In_Communication_Fault)XIC(Communication_Lost)OTE(Communication_Fault)OTE(CTRL.STS.Communication_Fault)OTL(Communication_Fault_Latch)OTL(MCM.CMD.Communication_Faulted);]]>
</Text>
</Rung>
<Rung Number="16" Type="N">
<Text>
<![CDATA[CLR(VFD_Fault_Code)XIC(Disconect_On_Delay.DN)XIC(InVFD.Faulted)MOVE(InVFD.Fault1Code,VFD_Fault_Code)OTE(Motor_Faulted);]]>
</Text>
</Rung>
<Rung Number="17" Type="N">
<Text>
<![CDATA[NE(VFD_Fault_Code,0)MOVE(VFD_Fault_Code,Last_Motor_Fault_Code);]]>
</Text>
</Rung>
<Rung Number="18" Type="N">
<Text>
<![CDATA[XIC(InVFD.DriveStatus_param_SafetyActive)[XIC(Run) ,XIC(Safety_Torque_Off) ]MOVE(2000,Safe_Off_Delay.PRE)TON(Safe_Off_Delay,?,?)XIC(Safe_Off_Delay.DN)OTE(Safety_Torque_Off);]]>
</Text>
</Rung>
<Rung Number="19" Type="N">
<Text>
<![CDATA[XIC(MCM.STS.Motor_Fault_Reset_PB)XIC(Disconect_On_Delay.DN)XIO(Motor_Faulted)XIO(Safety_Torque_Off)OTU(Motor_Fault_Latch);]]>
</Text>
</Rung>
<Rung Number="20" Type="N">
<Text>
<![CDATA[XIC(MCM.STS.Motor_Fault_Reset_PB)XIO(Communication_Fault)OTU(Communication_Fault_Latch);]]>
</Text>
</Rung>
<Rung Number="21" Type="N">
<Text>
<![CDATA[XIO(s:fs)[XIO(Disconect_On_Delay.DN) ,XIC(Motor_Faulted) ,XIC(Safety_Torque_Off) ]OTL(MCM.CMD.VFD_Faulted)OTE(CTRL.STS.VFD_Fault)OTL(Motor_Fault_Latch);]]>
</Text>
</Rung>
<Rung Number="22" Type="N">
<Text>
<![CDATA[XIC(Motor_Fault_Latch)OTL(MCM.CMD.VFD_Was_Faulted);]]>
</Text>
</Rung>
<Rung Number="23" Type="N">
<Text>
<![CDATA[XIC(Communication_Fault_Latch)OTL(MCM.CMD.Communication_Was_Faulted);]]>
</Text>
</Rung>
<Rung Number="24" Type="N">
<Text>
<![CDATA[XIC(Jammed)OTE(CTRL.STS.Jammed)OTL(MCM.CMD.Jam_Fault);]]>
</Text>
</Rung>
<Rung Number="25" Type="N">
<Text>
<![CDATA[XIC(Encoder_Fault)OTE(CTRL.STS.Encoder_Fault)OTL(MCM.CMD.Encoder_Fault);]]>
</Text>
</Rung>
<Rung Number="26" Type="N">
<Text>
<![CDATA[XIC(MCM.STS.Unacknowldge_All)OTU(CTRL.STS.Disabled);]]>
</Text>
</Rung>
<Rung Number="27" Type="N">
<Text>
<![CDATA[[XIC(CTRL.CMD.Disable) OTL(CTRL.STS.Disabled) ,XIC(CTRL.STS.Disabled) ]OTE(Disabled);]]>
</Text>
</Rung>
<Rung Number="28" Type="N">
<Text>
<![CDATA[XIC(MCM.STS.System_Started)XIC(CTRL.CMD.Power_Saving_Mode_ON)[XIC(Running) MUL(HMI.Power_Save_Time,1000,Power_Save_Timer.PRE) TON(Power_Save_Timer,?,?) XIC(Power_Save_Timer.DN) ,XIC(Power_Saving_Mode) XIO(CTRL.CMD.Start) XIO(MCM.STS.Start_Request) ]OTE(CTRL.STS.In_Power_Saving_Mode)OTE(Power_Saving_Mode);]]>
</Text>
</Rung>
<Rung Number="29" Type="N">
<Text>
<![CDATA[XIC(MCM.STS.System_Started)XIO(EStopped)XIO(Motor_Fault_Latch)XIO(Communication_Fault_Latch)XIO(Jammed)XIO(Encoder_Fault)XIO(Full)XIO(Stopped_Auto_Restart)XIO(Disabled)OTE(Run_Enabled);]]>
</Text>
</Rung>
<Rung Number="30" Type="N">
<Text>
<![CDATA[XIC(CTRL.CMD.Stopped_By_Stop_PB)OTE(Stopped_By_Station_PB)OTE(CTRL.STS.Local_Stopped);]]>
</Text>
</Rung>
<Rung Number="31" Type="N">
<Text>
<![CDATA[XIO(Maintenance_Mode)XIC(Run_Enabled)[XIC(CTRL.CMD.Start) ,XIC(Start_Conveyor) ,ONS(Start_ONS) ]XIO(CTRL.CMD.Stop_Require_Start)OTE(Start_Conveyor);]]>
</Text>
</Rung>
<Rung Number="32" Type="N">
<Text>
<![CDATA[XIC(Maintenance_Mode)XIO(Motor_Fault_Latch)XIO(Communication_Fault_Latch)XIO(EStopped)[XIC(HMI.Maintenance_Start_PB_Pressed) ,XIC(Maintenance_Start_Conveyor) ]XIO(HMI.Maintenance_Stop_PB_Pressed)OTE(Maintenance_Start_Conveyor);]]>
</Text>
</Rung>
<Rung Number="33" Type="N">
<Text>
<![CDATA[XIC(Maintenance_Mode)XIC(InVFD.Active)OTE(Maintenance_Running);]]>
</Text>
</Rung>
<Rung Number="34" Type="N">
<Text>
<![CDATA[XIC(Maintenance_Mode)XIO(Motor_Fault_Latch)XIO(Communication_Fault_Latch)XIO(EStopped)XIC(HMI.Maintenance_Jog_PB_Pressed)OTE(Maintenance_Jog_Mode)OTE(HMI.Maintenance_Jog_LT);]]>
</Text>
</Rung>
<Rung Number="35" Type="N">
<Text>
<![CDATA[[XIC(Start_Conveyor) ,XIC(Maintenance_Start_Conveyor) ,XIC(Maintenance_Jog_Mode) ]MOVE(5000,Start_Delay_Timmer.PRE)TON(Start_Delay_Timmer,?,?);]]>
</Text>
</Rung>
<Rung Number="36" Type="N">
<Text>
<![CDATA[XIC(Start_Delay_Timmer.TT)COP(Starting_String,Concatenated_String,1)CONCAT(HMI.Name,Concatenated_String,MCM.CMD.Log)OTL(MCM.CMD.EStop_Was_Actuated);]]>
</Text>
</Rung>
<Rung Number="37" Type="N">
<Text>
<![CDATA[[XIC(Jammed_Latch) ,XIC(CTRL.CMD.Run_Up_Enabled) ]OTE(Interlock)OTE(CTRL.STS.Interlock);]]>
</Text>
</Rung>
<Rung Number="38" Type="N">
<Text>
<![CDATA[XIO(Interlock)OTE(No_Interlock);]]>
</Text>
</Rung>
<Rung Number="39" Type="N">
<Text>
<![CDATA[XIC(Start_Delay_Timmer.DN)[XIO(Maintenance_Mode) XIC(MCM.STS.System_Started) XIC(Interlock) OTE(CTRL.STS.Enabled) GT(CTRL.CMD.Speed_FPM,0) XIO(Power_Saving_Mode) ,XIC(Maintenance_Mode) ]OTE(Run);]]>
</Text>
</Rung>
<Rung Number="40" Type="N">
<Text>
<![CDATA[XIO(Run)OTE(OutVFD.Stop);]]>
</Text>
</Rung>
<Rung Number="41" Type="N">
<Text>
<![CDATA[XIC(Run)[XIO(Maintenance_Conveyor_Direction) OTE(OutVFD.Forward) ,XIC(Maintenance_Conveyor_Direction) OTE(OutVFD.Reverse) ]OTE(OutVFD.Start);]]>
</Text>
</Rung>
<Rung Number="42" Type="N">
<Text>
<![CDATA[XIC(InVFD.Active)OTE(Running)OTE(CTRL.STS.Running);]]>
</Text>
</Rung>
<Rung Number="43" Type="N">
<Text>
<![CDATA[XIC(InVFD.Faulted)[XIC(MCM.STS.Motor_Fault_Reset_PB) ,XIC(OutVFD.ClearFaults) ]OTE(OutVFD.ClearFaults);]]>
</Text>
</Rung>
<Rung Number="44" Type="N">
<Text>
<![CDATA[XIC(Maintenance_Mode)XIC(Maintenance_Running)OTE(HMI.Maintenance_Conveyor_Run_LT);]]>
</Text>
</Rung>
<Rung Number="45" Type="N">
<Text>
<![CDATA[XIC(Maintenance_Mode)XIO(Maintenance_Running)OTE(HMI.Maintenance_Stop_LT);]]>
</Text>
</Rung>
<Rung Number="46" Type="N">
<Text>
<![CDATA[XIO(Maintenance_Mode)OTU(HMI.Maintenance_Direction_PB_Pressed);]]>
</Text>
</Rung>
<Rung Number="47" Type="N">
<Text>
<![CDATA[XIC(HMI.Maintenance_Direction_PB_Pressed)OTE(Direction);]]>
</Text>
</Rung>
<Rung Number="48" Type="N">
<Text>
<![CDATA[XIC(Direction)OTE(Maintenance_Conveyor_Direction)OTE(HMI.Maintenance_Direction_LT);]]>
</Text>
</Rung>
<Rung Number="49" Type="N">
<Text>
<![CDATA[NE(HMI.Speed_At_60Hz,0)DIV(6000,HMI.Speed_At_60Hz,Speed_To_HZ_Ratio);]]>
</Text>
</Rung>
<Rung Number="50" Type="N">
<Text>
<![CDATA[EQ(Speed_To_HZ_Ratio,0)OTE(Speed_Not_Set_Up);]]>
</Text>
</Rung>
<Rung Number="51" Type="N">
<Text>
<![CDATA[XIO(Maintenance_Mode)MOVE(CTRL.CMD.Speed_FPM,CTRL.STS.Requested_Speed)MUL(CTRL.CMD.Speed_FPM,Speed_To_HZ_Ratio,Frequency_Command);]]>
</Text>
</Rung>
<Rung Number="52" Type="N">
<Text>
<![CDATA[XIC(Maintenance_Mode)MOVE(HMI.Maintenance_Conveyor_Speed,CTRL.STS.Requested_Speed)MUL(HMI.Maintenance_Conveyor_Speed,Speed_To_HZ_Ratio,Frequency_Command);]]>
</Text>
</Rung>
<Rung Number="53" Type="N">
<Text>
<![CDATA[XIC(MCM.STS.Setup_Speeds)MOVE(6000,Frequency_Command);]]>
</Text>
</Rung>
<Rung Number="54" Type="N">
<Text>
<![CDATA[MOVE(Frequency_Command,OutVFD.FreqCommand);]]>
</Text>
</Rung>
<Rung Number="55" Type="N">
<Text>
<![CDATA[DIV(InVFD.OutputFreq,Speed_To_HZ_Ratio,CTRL.STS.Current_Speed);]]>
</Text>
</Rung>
<Rung Number="56" Type="N">
<Text>
<![CDATA[NOP();]]>
</Text>
</Rung>
<Rung Number="57" Type="N">
<Text>
<![CDATA[MOVE(CTRL.STS.Current_Speed,HMI.FPM)DIV(InVFD.OutputCurrent,100,HMI.Amperage)DIV(InVFD.OutputVoltage,10,HMI.Voltage)DIV(InVFD.OutputFreq,100,HMI.Frequency);]]>
</Text>
</Rung>
<Rung Number="58" Type="N">
<Comment>
<![CDATA[Alarms
]]>
</Comment>
<Text>
<![CDATA[XIC(Disconnected)OTE(HMI.Alarm.Disconnected);]]>
</Text>
</Rung>
<Rung Number="59" Type="N">
<Text>
<![CDATA[XIC(Communication_Fault)OTE(HMI.Alarm.Communication_Fault);]]>
</Text>
</Rung>
<Rung Number="60" Type="N">
<Text>
<![CDATA[XIC(Motor_Faulted)OTE(HMI.Alarm.VFD_Fault);]]>
</Text>
</Rung>
<Rung Number="61" Type="N">
<Text>
<![CDATA[XIC(Safety_Torque_Off)OTE(HMI.Alarm.Safe_Off_Fault);]]>
</Text>
</Rung>
<Rung Number="62" Type="N">
<Text>
<![CDATA[XIO(CTRL.STS.VFD_Fault)XIC(Motor_Fault_Latch)OTE(HMI.Alarm.Reset_VFD);]]>
</Text>
</Rung>
<Rung Number="63" Type="N">
<Text>
<![CDATA[XIO(CTRL.STS.Communication_Fault)XIC(Communication_Fault_Latch)OTE(HMI.Alarm.Reset_Communication_Fault);]]>
</Text>
</Rung>
<Rung Number="64" Type="N">
<Text>
<![CDATA[MOVE(Communication_Fault_Code,HMI.Communication_Fault_Code)MOVE(VFD_Fault_Code,HMI.VFD_Fault_Code)MOVE(Last_Motor_Fault_Code,HMI.Last_VFD_Fault_Code);]]>
</Text>
</Rung>
<Rung Number="65" Type="N">
<Comment>
<![CDATA[Colors of Animation
]]>
</Comment>
<Text>
<![CDATA[[XIC(Disabled) ,XIO(MCM.STS.System_Started) XIO(Running) ]MOVE(13,HMI.STATE);]]>
</Text>
</Rung>
<Rung Number="66" Type="N">
<Text>
<![CDATA[XIC(MCM.STS.System_Started)XIO(Running)MOVE(12,HMI.STATE);]]>
</Text>
</Rung>
<Rung Number="67" Type="N">
<Text>
<![CDATA[XIC(Power_Saving_Mode)MOVE(11,HMI.STATE);]]>
</Text>
</Rung>
<Rung Number="68" Type="N">
<Text>
<![CDATA[XIC(Running)MOVE(10,HMI.STATE);]]>
</Text>
</Rung>
<Rung Number="69" Type="N">
<Text>
<![CDATA[[XIC(Jammed) ,XIC(Encoder_Fault) ]MOVE(4,HMI.STATE);]]>
</Text>
</Rung>
<Rung Number="70" Type="N">
<Text>
<![CDATA[XIC(Full)MOVE(6,HMI.STATE);]]>
</Text>
</Rung>
<Rung Number="71" Type="N">
<Text>
<![CDATA[XIC(Maintenance_Mode)MOVE(14,HMI.STATE);]]>
</Text>
</Rung>
<Rung Number="72" Type="N">
<Text>
<![CDATA[[XIC(Motor_Fault_Latch) ,XIC(Communication_Fault_Latch) ]MOVE(2,HMI.STATE);]]>
</Text>
</Rung>
<Rung Number="73" Type="N">
<Text>
<![CDATA[XIC(EStopped)MOVE(1,HMI.STATE);]]>
</Text>
</Rung>
<Rung Number="74" Type="N">
<Text>
<![CDATA[XIO(Disconnected)XIC(Motor_Faulted)[XIO(MCM.STS.Start_PB) MOVE(2,HMI.VFD_Status) ,XIC(MCM.STS.Start_PB) MOVE(10,HMI.VFD_Status) ];]]>
</Text>
</Rung>
<Rung Number="75" Type="N">
<Text>
<![CDATA[XIC(Disconnected)XIO(Motor_Faulted)MOVE(0,HMI.VFD_Status);]]>
</Text>
</Rung>
<Rung Number="76" Type="N">
<Text>
<![CDATA[XIC(Disconnected)XIC(Motor_Faulted)[XIO(MCM.STS.Start_PB) MOVE(0,HMI.VFD_Status) ,XIC(MCM.STS.Start_PB) MOVE(2,HMI.VFD_Status) ];]]>
</Text>
</Rung>
<Rung Number="77" Type="N">
<Text>
<![CDATA[XIO(Disconnected)XIO(Motor_Faulted)MOVE(10,HMI.VFD_Status);]]>
</Text>
</Rung>
<Rung Number="78" Type="N">
<Text>
<![CDATA[XIC(MCM.STS.All_Unacknowledge_Log)MOVE(0,Acknowledge);]]>
</Text>
</Rung>
<Rung Number="79" Type="N">
<Text>
<![CDATA[[XIC(Disconnected) ONS(Acknowledge_ONS.0) OTU(Acknowledge.0) ,XIC(Disconnected) XIO(Acknowledge.0) COP(Disconnect_Off_String,Concatenated_String,1) CONCAT(HMI.Name,Concatenated_String,MCM.CMD.Log) ADD(MCM.CMD.Log_Quantity,1,MCM.CMD.Log_Quantity) ,NE(MCM.STS.Acknowledge_Log,Empty_String) EQ(MCM.CMD.Log,MCM.STS.Acknowledge_Log) OTL(Acknowledge.0) COP(Empty_String,MCM.STS.Acknowledge_Log,1) ];]]>
</Text>
</Rung>
<Rung Number="80" Type="N">
<Text>
<![CDATA[[XIC(Motor_Faulted) ONS(Acknowledge_ONS.1) OTU(Acknowledge.1) ,XIC(Motor_Faulted) XIO(Acknowledge.1) COP(Motor_Fault_String,Concatenated_String,1) CONCAT(HMI.Name,Concatenated_String,MCM.CMD.Log) ADD(MCM.CMD.Log_Quantity,1,MCM.CMD.Log_Quantity) ,NE(MCM.STS.Acknowledge_Log,Empty_String) EQ(MCM.CMD.Log,MCM.STS.Acknowledge_Log) OTL(Acknowledge.1) COP(Empty_String,MCM.STS.Acknowledge_Log,1) ];]]>
</Text>
</Rung>
<Rung Number="81" Type="N">
<Text>
<![CDATA[[XIC(Safety_Torque_Off) ONS(Acknowledge_ONS.2) OTU(Acknowledge.2) ,XIC(Safety_Torque_Off) XIO(Acknowledge.2) COP(Safe_Off_String,Concatenated_String,1) CONCAT(HMI.Name,Concatenated_String,MCM.CMD.Log) ADD(MCM.CMD.Log_Quantity,1,MCM.CMD.Log_Quantity) ,NE(MCM.STS.Acknowledge_Log,Empty_String) EQ(MCM.CMD.Log,MCM.STS.Acknowledge_Log) OTL(Acknowledge.2) COP(Empty_String,MCM.STS.Acknowledge_Log,1) ];]]>
</Text>
</Rung>
<Rung Number="82" Type="N">
<Text>
<![CDATA[[XIC(Communication_Fault) ONS(Acknowledge_ONS.3) OTU(Acknowledge.3) ,XIC(Communication_Fault) XIO(Acknowledge.3) COP(Lost_Comm_String,Concatenated_String,1) CONCAT(HMI.Name,Concatenated_String,MCM.CMD.Log) ADD(MCM.CMD.Log_Quantity,1,MCM.CMD.Log_Quantity) ,NE(MCM.STS.Acknowledge_Log,Empty_String) EQ(MCM.CMD.Log,MCM.STS.Acknowledge_Log) OTL(Acknowledge.3) COP(Empty_String,MCM.STS.Acknowledge_Log,1) ];]]>
</Text>
</Rung>
<Rung Number="83" Type="N">
<Text>
<![CDATA[[XIC(Jammed) ONS(Acknowledge_ONS.4) OTU(Acknowledge.4) ,XIC(Jammed) XIO(Acknowledge.4) COP(Jam_String,Concatenated_String,1) CONCAT(HMI.Name,Concatenated_String,MCM.CMD.Log) ADD(MCM.CMD.Log_Quantity,1,MCM.CMD.Log_Quantity) ,NE(MCM.STS.Acknowledge_Log,Empty_String) EQ(MCM.CMD.Log,MCM.STS.Acknowledge_Log) OTL(Acknowledge.4) COP(Empty_String,MCM.STS.Acknowledge_Log,1) ];]]>
</Text>
</Rung>
<Rung Number="84" Type="N">
<Text>
<![CDATA[[XIC(Full) ONS(Acknowledge_ONS.5) OTU(Acknowledge.5) ,XIC(Full) XIO(Acknowledge.5) COP(Full_String,Concatenated_String,1) CONCAT(HMI.Name,Concatenated_String,MCM.CMD.Log) ADD(MCM.CMD.Log_Quantity,1,MCM.CMD.Log_Quantity) ,NE(MCM.STS.Acknowledge_Log,Empty_String) EQ(MCM.CMD.Log,MCM.STS.Acknowledge_Log) OTL(Acknowledge.5) COP(Empty_String,MCM.STS.Acknowledge_Log,1) ];]]>
</Text>
</Rung>
<Rung Number="85" Type="N">
<Text>
<![CDATA[NOP();]]>
</Text>
</Rung>
<Rung Number="86" Type="N">
<Text>
<![CDATA[XIC(HMI.Maintenance_Start_PB_Pressed)OTU(HMI.Maintenance_Start_PB_Pressed);]]>
</Text>
</Rung>
<Rung Number="87" Type="N">
<Text>
<![CDATA[XIC(HMI.Maintenance_Stop_PB_Pressed)OTU(HMI.Maintenance_Stop_PB_Pressed);]]>
</Text>
</Rung>
<Rung Number="88" Type="N">
<Text>
<![CDATA[OTU(CTRL.CMD.Start)OTU(CTRL.CMD.Stop_Require_Start)OTU(CTRL.CMD.Stop_Auto_Restart)OTU(CTRL.CMD.Encoder_Fault)OTU(CTRL.CMD.Jammed)OTU(CTRL.CMD.Full)OTU(CTRL.CMD.Disable)OTU(CTRL.CMD.Run_Up_Enabled)OTU(CTRL.CMD.Stopped_By_Stop_PB)COP(Empty_String,CTRL.CMD.Log,1);]]>
</Text>
</Rung>
</RLLContent>
</Routine>
</Routines>
<Dependencies>
<Dependency Type="DataType" Name="UDT_CTRL_VFD"/>
<Dependency Type="DataType" Name="UDT_CTRL_SIO_FIO"/>
<Dependency Type="DataType" Name="UDT_HMI_VFD"/>
<Dependency Type="DataType" Name="UDT_CTRL_MCM"/>
</Dependencies>
</AddOnInstructionDefinition>
</AddOnInstructionDefinitions>
</Controller>
</RSLogix5000Content>
