<?xml version="1.0" encoding="UTF-8" standalone="yes"?>
<!--EMERGENSY STOP STATION PUSH BUTTON-->
<RSLogix5000Content SchemaRevision="1.0" SoftwareRevision="36.00" TargetName="AOI_STATION_EPC" TargetType="AddOnInstructionDefinition" TargetClass="Standard" TargetRevision="1.0 " TargetLastEdited="2025-05-22T12:50:54.097Z" ContainsContext="true" ExportDate="Fri May 23 22:12:12 2025" ExportOptions="References NoRawData L5KData DecoratedData Context Dependencies ForceProtectedEncoding AllProjDocTrans">
<Controller Use="Context" Name="MTN6_Simulations">
<DataTypes Use="Context">
<DataType Name="UDT_ALARMS_STATION" Family="NoFamily" Class="User">
<Members>
<Member Name="ZZZZZZZZZZUDT_ALARMS0" DataType="SINT" Dimension="0" Radix="Decimal" Hidden="true" ExternalAccess="Read/Write"/>
<Member Name="EStopped" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_ALARMS0" BitNumber="0" ExternalAccess="Read/Write">
<Description>
<![CDATA[Conveyor Emergency Stopped]]>
</Description>
</Member>
<Member Name="Stopped" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_ALARMS0" BitNumber="1" ExternalAccess="Read/Write">
<Description>
<![CDATA[Conveyor Stopped]]>
</Description>
</Member>
</Members>
</DataType>
<DataType Name="UDT_CTRL_MCM" Family="NoFamily" Class="User">
<Members>
<Member Name="CMD" DataType="UDT_CTRL_MCM_CMD" Dimension="0" Radix="NullType" Hidden="false" ExternalAccess="Read/Write">
<Description>
<![CDATA[Command To MCM]]>
</Description>
</Member>
<Member Name="STS" DataType="UDT_CTRL_MCM_STS" Dimension="0" Radix="NullType" Hidden="false" ExternalAccess="Read/Write">
<Description>
<![CDATA[Status From MCM]]>
</Description>
</Member>
</Members>
<Dependencies>
<Dependency Type="DataType" Name="UDT_CTRL_MCM_CMD"/>
<Dependency Type="DataType" Name="UDT_CTRL_MCM_STS"/>
</Dependencies>
</DataType>
<DataType Name="UDT_CTRL_MCM_CMD" Family="NoFamily" Class="User">
<Members>
<Member Name="ZZZZZZZZZZUDT_CTRL_M0" DataType="SINT" Dimension="0" Radix="Decimal" Hidden="true" ExternalAccess="Read/Write"/>
<Member Name="EStop_Actuated" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_M0" BitNumber="0" ExternalAccess="Read/Write">
<Description>
<![CDATA[Emergency Stop Actuated]]>
</Description>
</Member>
<Member Name="Started" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_M0" BitNumber="1" ExternalAccess="Read/Write">
<Description>
<![CDATA[MCM]]>
</Description>
</Member>
<Member Name="Maintenance_Mode" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_M0" BitNumber="2" ExternalAccess="Read/Write">
<Description>
<![CDATA[In Maitenance Mode]]>
</Description>
</Member>
<Member Name="Jam_Fault" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_M0" BitNumber="3" ExternalAccess="Read/Write">
<Description>
<![CDATA[Conveyor is Jammed]]>
</Description>
</Member>
<Member Name="Communication_Was_Faulted" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_M0" BitNumber="4" ExternalAccess="Read/Write">
<Description>
<![CDATA[Ethernet Communication was Faulted]]>
</Description>
</Member>
<Member Name="VFD_Was_Faulted" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_M0" BitNumber="5" ExternalAccess="Read/Write">
<Description>
<![CDATA[VFD Was Faulted]]>
</Description>
</Member>
<Member Name="EStop_Was_Actuated" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_M0" BitNumber="6" ExternalAccess="Read/Write">
<Description>
<![CDATA[Emergency Stop was Actuated]]>
</Description>
</Member>
<Member Name="Log" DataType="STRING" Dimension="0" Radix="NullType" Hidden="false" ExternalAccess="Read/Write">
<Description>
<![CDATA[Log]]>
</Description>
</Member>
<Member Name="ZZZZZZZZZZUDT_CTRL_M9" DataType="SINT" Dimension="0" Radix="Decimal" Hidden="true" ExternalAccess="Read/Write"/>
<Member Name="Acknowledge_Log" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_M9" BitNumber="0" ExternalAccess="Read/Write">
<Description>
<![CDATA[Acknowledge Log]]>
</Description>
</Member>
<Member Name="All_Unacknowledge_Log" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_M9" BitNumber="1" ExternalAccess="Read/Write">
<Description>
<![CDATA[All Unacknowledge Logs]]>
</Description>
</Member>
<Member Name="VFD_Faulted" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_M9" BitNumber="2" ExternalAccess="Read/Write">
<Description>
<![CDATA[VFD Faulted]]>
</Description>
</Member>
<Member Name="Communication_Faulted" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_M9" BitNumber="3" ExternalAccess="Read/Write">
<Description>
<![CDATA[Ethernet Communication Faulted]]>
</Description>
</Member>
<Member Name="Log_Quantity" DataType="DINT" Dimension="0" Radix="Decimal" Hidden="false" ExternalAccess="Read/Write">
<Description>
<![CDATA[Log Quantity]]>
</Description>
</Member>
<Member Name="ZZZZZZZZZZUDT_CTRL_M15" DataType="SINT" Dimension="0" Radix="Decimal" Hidden="true" ExternalAccess="Read/Write"/>
<Member Name="VFD_In_Power_Saving_Mode" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_M15" BitNumber="0" ExternalAccess="Read/Write">
<Description>
<![CDATA[VFD in Power Saving Mode]]>
</Description>
</Member>
<Member Name="Encoder_Fault" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_M15" BitNumber="1" ExternalAccess="Read/Write">
<Description>
<![CDATA[Encoder Faulted or Conveyor is running at Low Speed]]>
</Description>
</Member>
<Member Name="LAP_PB" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_M15" BitNumber="2" ExternalAccess="Read/Write">
<Description>
<![CDATA[Low Air Pressure PushButton]]>
</Description>
</Member>
<Member Name="LAP_PB_LT" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_M15" BitNumber="3" ExternalAccess="Read/Write">
<Description>
<![CDATA[Low Air Pressure PushButton Light]]>
</Description>
</Member>
<Member Name="Start_PB" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_M15" BitNumber="4" ExternalAccess="Read/Write">
<Description>
<![CDATA[Start PushButton]]>
</Description>
</Member>
<Member Name="Stop_PB" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_M15" BitNumber="5" ExternalAccess="Read/Write">
<Description>
<![CDATA[Stop PushButton]]>
</Description>
</Member>
<Member Name="VFD_Fault_Reset_PB" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_M15" BitNumber="6" ExternalAccess="Read/Write">
<Description>
<![CDATA[VFD Fault Reset PushButton]]>
</Description>
</Member>
<Member Name="Jam_Restart_PB" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_M15" BitNumber="7" ExternalAccess="Read/Write">
<Description>
<![CDATA[Jam Reset PushButton]]>
</Description>
</Member>
<Member Name="ZZZZZZZZZZUDT_CTRL_M24" DataType="SINT" Dimension="0" Radix="Decimal" Hidden="true" ExternalAccess="Read/Write"/>
<Member Name="EStop_PB" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_M24" BitNumber="0" ExternalAccess="Read/Write">
<Description>
<![CDATA[Emergency Stop PushButton]]>
</Description>
</Member>
</Members>
</DataType>
<DataType Name="UDT_CTRL_MCM_STS" Family="NoFamily" Class="User">
<Members>
<Member Name="ZZZZZZZZZZUDT_CTRL_M0" DataType="SINT" Dimension="0" Radix="Decimal" Hidden="true" ExternalAccess="Read/Write"/>
<Member Name="EStopped" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_M0" BitNumber="0" ExternalAccess="Read/Write">
<Description>
<![CDATA[Emergency Stopped]]>
</Description>
</Member>
<Member Name="Maintenance_Mode" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_M0" BitNumber="1" ExternalAccess="Read/Write">
<Description>
<![CDATA[In Maitenance Mode]]>
</Description>
</Member>
<Member Name="System_Started" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_M0" BitNumber="2" ExternalAccess="Read/Write">
<Description>
<![CDATA[The System is Started]]>
</Description>
</Member>
<Member Name="VFD_Faulted" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_M0" BitNumber="3" ExternalAccess="Read/Write">
<Description>
<![CDATA[VFD Faulted]]>
</Description>
</Member>
<Member Name="Jam_Fault" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_M0" BitNumber="4" ExternalAccess="Read/Write">
<Description>
<![CDATA[Conveyor Jammed]]>
</Description>
</Member>
<Member Name="Communication_Fault" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_M0" BitNumber="5" ExternalAccess="Read/Write">
<Description>
<![CDATA[Ethernet Communication Faulted]]>
</Description>
</Member>
<Member Name="Log" DataType="STRING" Dimension="0" Radix="NullType" Hidden="false" ExternalAccess="Read/Write">
<Description>
<![CDATA[Log]]>
</Description>
</Member>
<Member Name="Acknowledge_Log" DataType="STRING" Dimension="0" Radix="NullType" Hidden="false" ExternalAccess="Read/Write">
<Description>
<![CDATA[Acknowledge Log]]>
</Description>
</Member>
<Member Name="ZZZZZZZZZZUDT_CTRL_M9" DataType="SINT" Dimension="0" Radix="Decimal" Hidden="true" ExternalAccess="Read/Write"/>
<Member Name="All_Unacknowledge_Log" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_M9" BitNumber="0" ExternalAccess="Read/Write">
<Description>
<![CDATA[All Unacknowledged Logs]]>
</Description>
</Member>
<Member Name="Start_Request" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_M9" BitNumber="1" ExternalAccess="Read/Write">
<Description>
<![CDATA[System Start Requested]]>
</Description>
</Member>
<Member Name="Log_Quantity" DataType="DINT" Dimension="0" Radix="Decimal" Hidden="false" ExternalAccess="Read/Write">
<Description>
<![CDATA[Log Quantity]]>
</Description>
</Member>
<Member Name="ZZZZZZZZZZUDT_CTRL_M13" DataType="SINT" Dimension="0" Radix="Decimal" Hidden="true" ExternalAccess="Read/Write"/>
<Member Name="Encoder_Fault" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_M13" BitNumber="0" ExternalAccess="Read/Write">
<Description>
<![CDATA[Encoder Faulted or Conveyor is running at Low Speed]]>
</Description>
</Member>
<Member Name="LAP_PB" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_M13" BitNumber="1" ExternalAccess="Read/Write">
<Description>
<![CDATA[Low Air Pressure PushButton]]>
</Description>
</Member>
<Member Name="LAP_PB_LT" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_M13" BitNumber="2" ExternalAccess="Read/Write">
<Description>
<![CDATA[Low Air Pressure PushButton Light]]>
</Description>
</Member>
<Member Name="Start_PB" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_M13" BitNumber="3" ExternalAccess="Read/Write">
<Description>
<![CDATA[Start PushButton]]>
</Description>
</Member>
<Member Name="Stop_PB" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_M13" BitNumber="4" ExternalAccess="Read/Write">
<Description>
<![CDATA[Stop PushButton]]>
</Description>
</Member>
<Member Name="Motor_Fault_Reset_PB" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_M13" BitNumber="5" ExternalAccess="Read/Write">
<Description>
<![CDATA[Motor Fault Reset PushButton]]>
</Description>
</Member>
<Member Name="Jam_Restart_PB" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_M13" BitNumber="6" ExternalAccess="Read/Write">
<Description>
<![CDATA[Jam Restart PushButton]]>
</Description>
</Member>
<Member Name="EStop_PB" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_M13" BitNumber="7" ExternalAccess="Read/Write">
<Description>
<![CDATA[Emergency Stop PushButton]]>
</Description>
</Member>
<Member Name="ZZZZZZZZZZUDT_CTRL_M22" DataType="SINT" Dimension="0" Radix="Decimal" Hidden="true" ExternalAccess="Read/Write"/>
<Member Name="Unacknowldge_All" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_M22" BitNumber="0" ExternalAccess="Read/Write">
<Description>
<![CDATA[Unacknowledge all Alarms]]>
</Description>
</Member>
<Member Name="Aknowledgement_ID" DataType="STRING" Dimension="0" Radix="NullType" Hidden="false" ExternalAccess="Read/Write">
<Description>
<![CDATA[Aknowledgement ID]]>
</Description>
</Member>
<Member Name="ZZZZZZZZZZUDT_CTRL_M25" DataType="SINT" Dimension="0" Radix="Decimal" Hidden="true" ExternalAccess="Read/Write"/>
<Member Name="Setup_Speeds" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_M25" BitNumber="0" ExternalAccess="Read/Write">
<Description>
<![CDATA[Set Up Speeds of Conveyors]]>
</Description>
</Member>
</Members>
</DataType>
<DataType Name="UDT_CTRL_SIO_FIO" Family="NoFamily" Class="User">
<Members>
<Member Name="STS" DataType="UDT_CTRL_SIO_FIO_STS" Dimension="0" Radix="NullType" Hidden="false" ExternalAccess="Read/Write"/>
</Members>
<Dependencies>
<Dependency Type="DataType" Name="UDT_CTRL_SIO_FIO_STS"/>
</Dependencies>
</DataType>
<DataType Name="UDT_CTRL_SIO_FIO_STS" Family="NoFamily" Class="User">
<Members>
<Member Name="ZZZZZZZZZZUDT_CTRL_S0" DataType="SINT" Dimension="0" Radix="Decimal" Hidden="true" ExternalAccess="Read/Write"/>
<Member Name="Communication_Fault" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_S0" BitNumber="0" ExternalAccess="Read/Write">
<Description>
<![CDATA[Ethernet Communication Faulted]]>
</Description>
</Member>
</Members>
</DataType>
<DataType Name="UDT_CTRL_STATION" Family="NoFamily" Class="User">
<Members>
<Member Name="CMD" DataType="UDT_CTRL_STATION_CMD" Dimension="0" Radix="NullType" Hidden="false" ExternalAccess="Read/Write"/>
<Member Name="STS" DataType="UDT_CTRL_STATION_STS" Dimension="0" Radix="NullType" Hidden="false" ExternalAccess="Read/Write"/>
</Members>
<Dependencies>
<Dependency Type="DataType" Name="UDT_CTRL_STATION_CMD"/>
<Dependency Type="DataType" Name="UDT_CTRL_STATION_STS"/>
</Dependencies>
</DataType>
<DataType Name="UDT_CTRL_STATION_CMD" Family="NoFamily" Class="User">
<Members>
<Member Name="ZZZZZZZZZZUDT_CTRL_S0" DataType="SINT" Dimension="0" Radix="Decimal" Hidden="true" ExternalAccess="Read/Write"/>
<Member Name="Jammed" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_S0" BitNumber="0" ExternalAccess="Read/Write">
<Description>
<![CDATA[Conveyor]]>
</Description>
</Member>
<Member Name="EStop_Actuated" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_S0" BitNumber="1" ExternalAccess="Read/Write">
<Description>
<![CDATA[Emergency Stop Actuated]]>
</Description>
</Member>
<Member Name="Log" DataType="STRING" Dimension="0" Radix="NullType" Hidden="false" ExternalAccess="Read/Write">
<Description>
<![CDATA[Log]]>
</Description>
</Member>
</Members>
</DataType>
<DataType Name="UDT_CTRL_STATION_STS" Family="NoFamily" Class="User">
<Members>
<Member Name="ZZZZZZZZZZUDT_CTRL_S0" DataType="SINT" Dimension="0" Radix="Decimal" Hidden="true" ExternalAccess="Read/Write"/>
<Member Name="Start" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_S0" BitNumber="0" ExternalAccess="Read/Write">
<Description>
<![CDATA[Start command For/From Partner Stations]]>
</Description>
</Member>
<Member Name="Stop" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_S0" BitNumber="1" ExternalAccess="Read/Write">
<Description>
<![CDATA[Stop command For/From Partner Stations]]>
</Description>
</Member>
<Member Name="EStop_Was_Actuated" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_S0" BitNumber="2" ExternalAccess="Read/Write">
<Description>
<![CDATA[Emergency Stop was Actuated]]>
</Description>
</Member>
<Member Name="Log" DataType="STRING" Dimension="0" Radix="NullType" Hidden="false" ExternalAccess="Read/Write">
<Description>
<![CDATA[Log]]>
</Description>
</Member>
<Member Name="ZZZZZZZZZZUDT_CTRL_S5" DataType="SINT" Dimension="0" Radix="Decimal" Hidden="true" ExternalAccess="Read/Write"/>
<Member Name="JR_PB_LT" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_S5" BitNumber="0" ExternalAccess="Read/Write">
<Description>
<![CDATA[Jam Reset Push Button Light]]>
</Description>
</Member>
<Member Name="Jam_Fault" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_S5" BitNumber="1" ExternalAccess="Read/Write">
<Description>
<![CDATA[Conveyor Jammed]]>
</Description>
</Member>
</Members>
</DataType>
<DataType Name="UDT_HMI_STATION" Family="NoFamily" Class="User">
<Members>
<Member Name="Name" DataType="STRING" Dimension="0" Radix="NullType" Hidden="false" ExternalAccess="Read/Write">
<Description>
<![CDATA[Station Name]]>
</Description>
</Member>
<Member Name="MCM_Name" DataType="STRING" Dimension="0" Radix="NullType" Hidden="false" ExternalAccess="Read/Write">
<Description>
<![CDATA[MCM Name]]>
</Description>
</Member>
<Member Name="Conveyor_Name" DataType="STRING" Dimension="0" Radix="NullType" Hidden="false" ExternalAccess="Read/Write">
<Description>
<![CDATA[Conveyor Name]]>
</Description>
</Member>
<Member Name="Alarm" DataType="UDT_ALARMS_STATION" Dimension="0" Radix="NullType" Hidden="false" ExternalAccess="Read/Write">
<Description>
<![CDATA[Station Alarms]]>
</Description>
</Member>
<Member Name="ZZZZZZZZZZUDT_HMI_ST4" DataType="SINT" Dimension="0" Radix="Decimal" Hidden="true" ExternalAccess="Read/Write"/>
<Member Name="Start_PB" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_HMI_ST4" BitNumber="0" ExternalAccess="Read/Write">
<Description>
<![CDATA[Start PushButton]]>
</Description>
</Member>
<Member Name="Stop_PB" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_HMI_ST4" BitNumber="1" ExternalAccess="Read/Write">
<Description>
<![CDATA[Stop PushButton]]>
</Description>
</Member>
<Member Name="Start_Color" DataType="DINT" Dimension="0" Radix="Decimal" Hidden="false" ExternalAccess="Read/Write">
<Description>
<![CDATA[Start Color]]>
</Description>
</Member>
<Member Name="Stop_Color" DataType="DINT" Dimension="0" Radix="Decimal" Hidden="false" ExternalAccess="Read/Write">
<Description>
<![CDATA[Stop Color]]>
</Description>
</Member>
<Member Name="ZZZZZZZZZZUDT_HMI_ST9" DataType="SINT" Dimension="0" Radix="Decimal" Hidden="true" ExternalAccess="Read/Write"/>
<Member Name="JR_PB_LT" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_HMI_ST9" BitNumber="0" ExternalAccess="Read/Write">
<Description>
<![CDATA[Jam Restart PushButton Light]]>
</Description>
</Member>
</Members>
<Dependencies>
<Dependency Type="DataType" Name="UDT_ALARMS_STATION"/>
</Dependencies>
</DataType>
</DataTypes>
<AddOnInstructionDefinitions Use="Context">
<AddOnInstructionDefinition Name="AOI_FLIP_FLOP" Class="Standard" Revision="1.0" ExecutePrescan="false" ExecutePostscan="false" ExecuteEnableInFalse="false" CreatedDate="2022-03-10T21:16:26.590Z" CreatedBy="DESKTOP-T9CCJM5\autStand" EditedDate="2025-05-21T10:05:03.350Z" EditedBy="LCIBATUMI\ilia.gurielidze" SoftwareRevision="v36.00"
>
<Parameters>
<Parameter Name="EnableIn" TagType="Base" DataType="BOOL" Usage="Input" Radix="Decimal" Required="false" Visible="false" ExternalAccess="Read Only">
<Description>
<![CDATA[Enable Input - System Defined Parameter]]>
</Description>
</Parameter>
<Parameter Name="EnableOut" TagType="Base" DataType="BOOL" Usage="Output" Radix="Decimal" Required="false" Visible="false" ExternalAccess="Read Only">
<Description>
<![CDATA[Enable Output - System Defined Parameter]]>
</Description>
</Parameter>
<Parameter Name="On" TagType="Base" DataType="DINT" Usage="Input" Radix="Decimal" Required="true" Visible="true" ExternalAccess="Read/Write">
<Description>
<![CDATA[Amount of time Beacon is On while Flashing]]>
</Description>
<DefaultData Format="L5K">
<![CDATA[0]]>
</DefaultData>
<DefaultData Format="Decorated">
<DataValue DataType="DINT" Radix="Decimal" Value="0"/>
</DefaultData>
</Parameter>
<Parameter Name="Off" TagType="Base" DataType="DINT" Usage="Input" Radix="Decimal" Required="true" Visible="true" ExternalAccess="Read/Write">
<Description>
<![CDATA[Amount of time Beacon is Off while Flashing]]>
</Description>
<DefaultData Format="L5K">
<![CDATA[0]]>
</DefaultData>
<DefaultData Format="Decorated">
<DataValue DataType="DINT" Radix="Decimal" Value="0"/>
</DefaultData>
</Parameter>
<Parameter Name="Flash" TagType="Base" DataType="BOOL" Usage="Output" Radix="Decimal" Required="false" Visible="true" ExternalAccess="Read Only">
<DefaultData Format="L5K">
<![CDATA[0]]>
</DefaultData>
<DefaultData Format="Decorated">
<DataValue DataType="BOOL" Radix="Decimal" Value="0"/>
</DefaultData>
</Parameter>
</Parameters>
<LocalTags>
<LocalTag Name="Flip" DataType="TIMER" ExternalAccess="None">
<DefaultData Format="L5K">
<![CDATA[[0,0,0]]]>
</DefaultData>
<DefaultData Format="Decorated">
<Structure DataType="TIMER">
<DataValueMember Name="PRE" DataType="DINT" Radix="Decimal" Value="0"/>
<DataValueMember Name="ACC" DataType="DINT" Radix="Decimal" Value="0"/>
<DataValueMember Name="EN" DataType="BOOL" Value="0"/>
<DataValueMember Name="TT" DataType="BOOL" Value="0"/>
<DataValueMember Name="DN" DataType="BOOL" Value="0"/>
</Structure>
</DefaultData>
</LocalTag>
<LocalTag Name="Flop" DataType="TIMER" ExternalAccess="None">
<DefaultData Format="L5K">
<![CDATA[[0,0,0]]]>
</DefaultData>
<DefaultData Format="Decorated">
<Structure DataType="TIMER">
<DataValueMember Name="PRE" DataType="DINT" Radix="Decimal" Value="0"/>
<DataValueMember Name="ACC" DataType="DINT" Radix="Decimal" Value="0"/>
<DataValueMember Name="EN" DataType="BOOL" Value="0"/>
<DataValueMember Name="TT" DataType="BOOL" Value="0"/>
<DataValueMember Name="DN" DataType="BOOL" Value="0"/>
</Structure>
</DefaultData>
</LocalTag>
</LocalTags>
<Routines>
<Routine Name="Logic" Type="RLL">
<RLLContent>
<Rung Number="0" Type="N">
<Text>
<![CDATA[MOVE(On,Flip.PRE)MOVE(Off,Flop.PRE);]]>
</Text>
</Rung>
<Rung Number="1" Type="N">
<Text>
<![CDATA[XIO(Flop.DN)TON(Flip,?,?);]]>
</Text>
</Rung>
<Rung Number="2" Type="N">
<Text>
<![CDATA[XIC(Flip.DN)TON(Flop,?,?);]]>
</Text>
</Rung>
<Rung Number="3" Type="N">
<Text>
<![CDATA[XIC(Flip.DN)OTE(Flash)OTE(EnableOut);]]>
</Text>
</Rung>
</RLLContent>
</Routine>
</Routines>
</AddOnInstructionDefinition>
<AddOnInstructionDefinition Use="Target" Name="AOI_STATION_EPC" Class="Standard" Revision="1.0" Vendor="Automation Standard" ExecutePrescan="true" ExecutePostscan="false" ExecuteEnableInFalse="false" CreatedDate="2012-02-01T16:00:09.261Z" CreatedBy="Not Available" EditedDate="2025-05-22T12:50:54.097Z"
 EditedBy="LCIBATUMI\ilia.gurielidze" SoftwareRevision="v36.00">
<Description>
<![CDATA[EMERGENSY STOP STATION PUSH BUTTON]]>
</Description>
<Parameters>
<Parameter Name="EnableIn" TagType="Base" DataType="BOOL" Usage="Input" Radix="Decimal" Required="false" Visible="false" ExternalAccess="Read Only"/>
<Parameter Name="EnableOut" TagType="Base" DataType="BOOL" Usage="Output" Radix="Decimal" Required="false" Visible="false" ExternalAccess="Read Only"/>
<Parameter Name="MCM" TagType="Base" DataType="UDT_CTRL_MCM" Usage="InOut" Required="true" Visible="true" Constant="false"/>
<Parameter Name="HMI" TagType="Base" DataType="UDT_HMI_STATION" Usage="InOut" Required="true" Visible="true" Constant="false"/>
<Parameter Name="Station" TagType="Base" DataType="UDT_CTRL_STATION" Usage="InOut" Required="true" Visible="true" Constant="false"/>
<Parameter Name="SIO" TagType="Base" DataType="UDT_CTRL_SIO_FIO" Usage="InOut" Required="true" Visible="true" Constant="false"/>
<Parameter Name="In_EStop" TagType="Base" DataType="BOOL" Usage="Input" Radix="Decimal" Required="true" Visible="true" ExternalAccess="Read/Write">
<Description>
<![CDATA[Emergency Pull Cord(NC)]]>
</Description>
<DefaultData Format="L5K">
<![CDATA[0]]>
</DefaultData>
<DefaultData Format="Decorated">
<DataValue DataType="BOOL" Radix="Decimal" Value="0"/>
</DefaultData>
</Parameter>
<Parameter Name="EStop_Actuated" TagType="Base" DataType="BOOL" Usage="Output" Radix="Decimal" Required="false" Visible="true" ExternalAccess="Read/Write">
<Description>
<![CDATA[Emergency Stop Actuated]]>
</Description>
<DefaultData Format="L5K">
<![CDATA[0]]>
</DefaultData>
<DefaultData Format="Decorated">
<DataValue DataType="BOOL" Radix="Decimal" Value="0"/>
</DefaultData>
</Parameter>
<Parameter Name="Out_Beacon_Light" TagType="Base" DataType="BOOL" Usage="InOut" Radix="Decimal" Required="true" Visible="true" Constant="false">
<Description>
<![CDATA[Beacon Light]]>
</Description>
</Parameter>
</Parameters>
<LocalTags>
<LocalTag Name="Restart" DataType="BOOL" Radix="Decimal" ExternalAccess="None">
<DefaultData Format="L5K">
<![CDATA[0]]>
</DefaultData>
<DefaultData Format="Decorated">
<DataValue DataType="BOOL" Radix="Decimal" Value="0"/>
</DefaultData>
</LocalTag>
<LocalTag Name="Beacon_ONS" DataType="BOOL" Radix="Decimal" ExternalAccess="None">
<Description>
<![CDATA[To Unlatch Beacon Light once if Emergency Stop was not Actuated]]>
</Description>
<DefaultData Format="L5K">
<![CDATA[0]]>
</DefaultData>
<DefaultData Format="Decorated">
<DataValue DataType="BOOL" Radix="Decimal" Value="0"/>
</DefaultData>
</LocalTag>
<LocalTag Name="Flip_Flop" DataType="AOI_FLIP_FLOP" ExternalAccess="None">
<Description>
<![CDATA[Beacon Flip Flop]]>
</Description>
<DefaultData Format="L5K">
<![CDATA[[1,0,0,[0,0,0],[0,0,0]]]]>
</DefaultData>
<DefaultData Format="Decorated">
<Structure DataType="AOI_FLIP_FLOP">
<DataValueMember Name="EnableIn" DataType="BOOL" Value="1"/>
<DataValueMember Name="EnableOut" DataType="BOOL" Value="0"/>
<DataValueMember Name="On" DataType="DINT" Radix="Decimal" Value="0"/>
<DataValueMember Name="Off" DataType="DINT" Radix="Decimal" Value="0"/>
<DataValueMember Name="Flash" DataType="BOOL" Value="0"/>
</Structure>
</DefaultData>
</LocalTag>
<LocalTag Name="Estop_Was_Actuated" DataType="BOOL" Radix="Decimal" ExternalAccess="None">
<Description>
<![CDATA[Emergency Stop was Actuated]]>
</Description>
<DefaultData Format="L5K">
<![CDATA[0]]>
</DefaultData>
<DefaultData Format="Decorated">
<DataValue DataType="BOOL" Radix="Decimal" Value="0"/>
</DefaultData>
</LocalTag>
<LocalTag Name="Concatenated_String" DataType="STRING" ExternalAccess="None">
<Description>
<![CDATA[Sring for Log]]>
</Description>
<DefaultData Format="L5K">
<![CDATA[[0,'$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00']]]>
</DefaultData>
<DefaultData Format="String" Length="0">
<![CDATA['']]>
</DefaultData>
</LocalTag>
<LocalTag Name="Acknowledge_ONS" DataType="BOOL" Radix="Decimal" ExternalAccess="None">
<Description>
<![CDATA[To Unlatch the Ucknoledgement once the Emergency Stop Actuated]]>
</Description>
<DefaultData Format="L5K">
<![CDATA[0]]>
</DefaultData>
<DefaultData Format="Decorated">
<DataValue DataType="BOOL" Radix="Decimal" Value="0"/>
</DefaultData>
</LocalTag>
<LocalTag Name="Acknowledge" DataType="BOOL" Radix="Decimal" ExternalAccess="None">
<Description>
<![CDATA[Emergency Stop Acknowledgment]]>
</Description>
<DefaultData Format="L5K">
<![CDATA[0]]>
</DefaultData>
<DefaultData Format="Decorated">
<DataValue DataType="BOOL" Radix="Decimal" Value="0"/>
</DefaultData>
</LocalTag>
</LocalTags>
<Routines>
<Routine Name="Logic" Type="RLL">
<RLLContent>
<Rung Number="0" Type="N">
<Text>
<![CDATA[XIO(In_EStop)XIO(SIO.STS.Communication_Fault)OTL(Station.CMD.EStop_Actuated)OTL(Estop_Was_Actuated)OTL(MCM.CMD.EStop_Actuated)OTE(EStop_Actuated);]]>
</Text>
</Rung>
<Rung Number="1" Type="N">
<Text>
<![CDATA[XIO(Station.STS.EStop_Was_Actuated)OTU(Estop_Was_Actuated);]]>
</Text>
</Rung>
<Rung Number="2" Type="N">
<Text>
<![CDATA[XIO(Estop_Was_Actuated)[ONS(Beacon_ONS) OTU(Out_Beacon_Light) ,JMP(JMP) ];]]>
</Text>
</Rung>
<Rung Number="3" Type="N">
<Text>
<![CDATA[[XIC(EStop_Actuated) AOI_FLIP_FLOP(Flip_Flop,500,500) ,XIC(Station.STS.EStop_Was_Actuated) XIC(In_EStop) ]OTE(Out_Beacon_Light);]]>
</Text>
</Rung>
<Rung Number="4" Type="N">
<Text>
<![CDATA[LBL(JMP)NOP();]]>
</Text>
</Rung>
<Rung Number="5" Type="N">
<Comment>
<![CDATA[ALARM
]]>
</Comment>
<Text>
<![CDATA[XIC(EStop_Actuated)OTE(HMI.Alarm.EStopped);]]>
</Text>
</Rung>
<Rung Number="6" Type="N">
<Comment>
<![CDATA[Colors of Animation
]]>
</Comment>
<Text>
<![CDATA[NOP();]]>
</Text>
</Rung>
<Rung Number="7" Type="N">
<Comment>
<![CDATA[Conveyor Running - Green (0.255.0)
]]>
</Comment>
<Text>
<![CDATA[MOVE(2,HMI.Stop_Color);]]>
</Text>
</Rung>
<Rung Number="8" Type="N">
<Comment>
<![CDATA[EStop Actuated - Red (255.0.0)
]]>
</Comment>
<Text>
<![CDATA[XIC(EStop_Actuated)MOVE(1,HMI.Stop_Color);]]>
</Text>
</Rung>
<Rung Number="9" Type="N">
<Text>
<![CDATA[XIC(MCM.STS.Unacknowldge_All)OTU(Acknowledge);]]>
</Text>
</Rung>
<Rung Number="10" Type="N">
<Text>
<![CDATA[[XIC(EStop_Actuated) ONS(Acknowledge_ONS) OTU(Acknowledge) ,XIC(EStop_Actuated) [XIO(Acknowledge) MOVE(' TRIPPED',Concatenated_String) CONCAT(HMI.Name,Concatenated_String,MCM.CMD.Log) ADD(MCM.CMD.Log_Quantity,1,MCM.CMD.Log_Quantity) ,MOVE(' TRIPPED',Concatenated_String) CONCAT(HMI.Name,Concatenated_String,Station.CMD.Log) ] ,NE(MCM.STS.Aknowledgement_ID,'') EQ(MCM.CMD.Log,MCM.STS.Aknowledgement_ID) OTL(Acknowledge) MOVE('',MCM.STS.Aknowledgement_ID) ];]]>
</Text>
</Rung>
</RLLContent>
</Routine>
<Routine Name="Prescan" Type="RLL">
<RLLContent>
<Rung Number="0" Type="N">
<Text>
<![CDATA[NOP();]]>
</Text>
</Rung>
<Rung Number="1" Type="N">
<Text>
<![CDATA[FLL(0,HMI.Alarm,1);]]>
</Text>
</Rung>
</RLLContent>
</Routine>
</Routines>
<Dependencies>
<Dependency Type="AddOnInstructionDefinition" Name="AOI_FLIP_FLOP"/>
<Dependency Type="DataType" Name="UDT_HMI_STATION"/>
<Dependency Type="DataType" Name="UDT_CTRL_MCM"/>
<Dependency Type="DataType" Name="UDT_CTRL_SIO_FIO"/>
<Dependency Type="DataType" Name="UDT_CTRL_STATION"/>
</Dependencies>
</AddOnInstructionDefinition>
</AddOnInstructionDefinitions>
</Controller>
</RSLogix5000Content>
