<?xml version="1.0" encoding="UTF-8" standalone="yes"?>
<RSLogix5000Content SchemaRevision="1.0" SoftwareRevision="36.00" TargetName="UDT_ALARMS_STATION" TargetType="DataType" ContainsContext="true" ExportDate="Sat May 24 15:48:10 2025" ExportOptions="References NoRawData L5KData DecoratedData Context Dependencies ForceProtectedEncoding AllProjDocTrans">
<Controller Use="Context" Name="MTN6_MCM01">
<DataTypes Use="Context">
<DataType Name="UDT_ALARMS_VFD" Family="NoFamily" Class="User">
<Members>
<Member Name="ZZZZZZZZZZUDT_ALARMS0" DataType="SINT" Dimension="0" Radix="Decimal" Hidden="true" ExternalAccess="Read/Write"/>
<Member Name="Communication_Fault" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_ALARMS0" BitNumber="0" ExternalAccess="Read/Write">
<Description>
<![CDATA[Ethernet Communication is Faulted]]>
</Description>
</Member>
<Member Name="Disconnected" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_ALARMS0" BitNumber="1" ExternalAccess="Read/Write">
<Description>
<![CDATA[Disconnected VFD]]>
</Description>
</Member>
<Member Name="VFD_Fault" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_ALARMS0" BitNumber="2" ExternalAccess="Read/Write">
<Description>
<![CDATA[VFD Faulted]]>
</Description>
</Member>
<Member Name="Safe_Off_Fault" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_ALARMS0" BitNumber="3" ExternalAccess="Read/Write">
<Description>
<![CDATA[VFD Safety Torque Fault]]>
</Description>
</Member>
<Member Name="Reset_VFD" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_ALARMS0" BitNumber="4" ExternalAccess="Read/Write">
<Description>
<![CDATA[VFD Reset]]>
</Description>
</Member>
<Member Name="Reset_Communication_Fault" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_ALARMS0" BitNumber="5" ExternalAccess="Read/Write">
<Description>
<![CDATA[Reset Comunication Fault]]>
</Description>
</Member>
</Members>
</DataType>
<DataType Name="UDT_CTRL_SIO_FIO" Family="NoFamily" Class="User">
<Members>
<Member Name="STS" DataType="UDT_CTRL_SIO_FIO_STS" Dimension="0" Radix="NullType" Hidden="false" ExternalAccess="Read/Write"/>
</Members>
<Dependencies>
<Dependency Type="DataType" Name="UDT_CTRL_SIO_FIO_STS"/>
</Dependencies>
</DataType>
<DataType Name="UDT_CTRL_SIO_FIO_STS" Family="NoFamily" Class="User">
<Members>
<Member Name="ZZZZZZZZZZUDT_CTRL_S0" DataType="SINT" Dimension="0" Radix="Decimal" Hidden="true" ExternalAccess="Read/Write"/>
<Member Name="Communication_Fault" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_S0" BitNumber="0" ExternalAccess="Read/Write">
<Description>
<![CDATA[Ethernet Communication Faulted]]>
</Description>
</Member>
</Members>
</DataType>
<DataType Name="UDT_CTRL_VFD" Family="NoFamily" Class="User">
<Members>
<Member Name="CMD" DataType="UDT_CTRL_VFD_CMD" Dimension="0" Radix="NullType" Hidden="false" ExternalAccess="Read/Write"/>
<Member Name="STS" DataType="UDT_CTRL_VFD_STS" Dimension="0" Radix="NullType" Hidden="false" ExternalAccess="Read/Write"/>
</Members>
<Dependencies>
<Dependency Type="DataType" Name="UDT_CTRL_VFD_CMD"/>
<Dependency Type="DataType" Name="UDT_CTRL_VFD_STS"/>
</Dependencies>
</DataType>
<DataType Name="UDT_CTRL_VFD_CMD" Family="NoFamily" Class="User">
<Members>
<Member Name="ZZZZZZZZZZUDT_CTRL_V0" DataType="SINT" Dimension="0" Radix="Decimal" Hidden="true" ExternalAccess="Read/Write"/>
<Member Name="Start" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_V0" BitNumber="0" ExternalAccess="Read/Write">
<Description>
<![CDATA[Start the Conveyor Locally in Auto Mode]]>
</Description>
</Member>
<Member Name="Stop_Require_Start" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_V0" BitNumber="1" ExternalAccess="Read/Write">
<Description>
<![CDATA[Stops the Motor
, requires Start command to Restart]]>
</Description>
</Member>
<Member Name="Stop_Auto_Restart" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_V0" BitNumber="2" ExternalAccess="Read/Write">
<Description>
<![CDATA[Stops the Motor, which will restart automatically when False]]>
</Description>
</Member>
<Member Name="Jammed" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_V0" BitNumber="3" ExternalAccess="Read/Write">
<Description>
<![CDATA[Conveyor]]>
</Description>
</Member>
<Member Name="Disable" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_V0" BitNumber="4" ExternalAccess="Read/Write">
<Description>
<![CDATA[Conveyor]]>
</Description>
</Member>
<Member Name="Run_Up_Enabled" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_V0" BitNumber="5" ExternalAccess="Read/Write">
<Description>
<![CDATA[When Downstream Conveyors are Stopped, Conveyor keeps running unill Discharge PE is Blocked]]>
</Description>
</Member>
<Member Name="Power_Saving_Mode_ON" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_V0" BitNumber="6" ExternalAccess="Read/Write">
<Description>
<![CDATA[VFD
is in Power Saving Mode]]>
</Description>
</Member>
<Member Name="Interlock" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_V0" BitNumber="7" ExternalAccess="Read/Write">
<Description>
<![CDATA[Downstream is Running]]>
</Description>
</Member>
<Member Name="ZZZZZZZZZZUDT_CTRL_V9" DataType="SINT" Dimension="0" Radix="Decimal" Hidden="true" ExternalAccess="Read/Write"/>
<Member Name="Stopped_By_Stop_PB" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_V9" BitNumber="0" ExternalAccess="Read/Write">
<Description>
<![CDATA[Conveyor
Stopped by Station Stop PushButton]]>
</Description>
</Member>
<Member Name="Log" DataType="STRING" Dimension="0" Radix="NullType" Hidden="false" ExternalAccess="Read/Write">
<Description>
<![CDATA[Log]]>
</Description>
</Member>
<Member Name="Acknowledge_Log" DataType="STRING" Dimension="0" Radix="NullType" Hidden="false" ExternalAccess="Read/Write">
<Description>
<![CDATA[Acknowledge Log]]>
</Description>
</Member>
<Member Name="ZZZZZZZZZZUDT_CTRL_V13" DataType="SINT" Dimension="0" Radix="Decimal" Hidden="true" ExternalAccess="Read/Write"/>
<Member Name="Full" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_V13" BitNumber="0" ExternalAccess="Read/Write">
<Description>
<![CDATA[Conveyor]]>
</Description>
</Member>
<Member Name="Encoder_Fault" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_V13" BitNumber="1" ExternalAccess="Read/Write">
<Description>
<![CDATA[Encoder Faulted or Conveyor is Running at Low Speed]]>
</Description>
</Member>
<Member Name="Speed_FPM" DataType="DINT" Dimension="0" Radix="Decimal" Hidden="false" ExternalAccess="Read/Write">
<Description>
<![CDATA[Speed in Feet per Minute]]>
</Description>
</Member>
</Members>
</DataType>
<DataType Name="UDT_CTRL_VFD_STS" Family="NoFamily" Class="User">
<Members>
<Member Name="ZZZZZZZZZZUDT_CTRL_V0" DataType="SINT" Dimension="0" Radix="Decimal" Hidden="true" ExternalAccess="Read/Write"/>
<Member Name="Running" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_V0" BitNumber="0" ExternalAccess="Read/Write">
<Description>
<![CDATA[Running]]>
</Description>
</Member>
<Member Name="VFD_Fault" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_V0" BitNumber="1" ExternalAccess="Read/Write">
<Description>
<![CDATA[VFD Faulted]]>
</Description>
</Member>
<Member Name="Communication_Fault" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_V0" BitNumber="2" ExternalAccess="Read/Write">
<Description>
<![CDATA[Ethernet Communicationb Faulted]]>
</Description>
</Member>
<Member Name="Interlock" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_V0" BitNumber="3" ExternalAccess="Read/Write">
<Description>
<![CDATA[Downstream Conveyor is Running]]>
</Description>
</Member>
<Member Name="Current_Speed" DataType="DINT" Dimension="0" Radix="Decimal" Hidden="false" ExternalAccess="Read/Write">
<Description>
<![CDATA[Current Speed of Conveyor in FPM]]>
</Description>
</Member>
<Member Name="Requested_Speed" DataType="DINT" Dimension="0" Radix="Decimal" Hidden="false" ExternalAccess="Read/Write">
<Description>
<![CDATA[Requested Speed of Conveyor in FPM]]>
</Description>
</Member>
<Member Name="ZZZZZZZZZZUDT_CTRL_V7" DataType="SINT" Dimension="0" Radix="Decimal" Hidden="true" ExternalAccess="Read/Write"/>
<Member Name="In_Power_Saving_Mode" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_V7" BitNumber="0" ExternalAccess="Read/Write">
<Description>
<![CDATA[In Power Saving Mode]]>
</Description>
</Member>
<Member Name="Maintenance_Mode" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_V7" BitNumber="1" ExternalAccess="Read/Write">
<Description>
<![CDATA[In Maintenance Mode]]>
</Description>
</Member>
<Member Name="MCM_Started" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_V7" BitNumber="2" ExternalAccess="Read/Write">
<Description>
<![CDATA[MCM Started]]>
</Description>
</Member>
<Member Name="EStopped" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_V7" BitNumber="3" ExternalAccess="Read/Write">
<Description>
<![CDATA[Conveyor Emergency Stopped]]>
</Description>
</Member>
<Member Name="Jammed" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_V7" BitNumber="4" ExternalAccess="Read/Write">
<Description>
<![CDATA[Conveyor]]>
</Description>
</Member>
<Member Name="Full" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_V7" BitNumber="5" ExternalAccess="Read/Write">
<Description>
<![CDATA[Conveyor]]>
</Description>
</Member>
<Member Name="Enabled" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_V7" BitNumber="6" ExternalAccess="Read/Write">
<Description>
<![CDATA[Conveyor]]>
</Description>
</Member>
<Member Name="Local_Stopped" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_V7" BitNumber="7" ExternalAccess="Read/Write">
<Description>
<![CDATA[Conveyor is Stopped Locally]]>
</Description>
</Member>
<Member Name="Log" DataType="STRING" Dimension="0" Radix="NullType" Hidden="false" ExternalAccess="Read/Write">
<Description>
<![CDATA[Log]]>
</Description>
</Member>
<Member Name="ZZZZZZZZZZUDT_CTRL_V17" DataType="SINT" Dimension="0" Radix="Decimal" Hidden="true" ExternalAccess="Read/Write"/>
<Member Name="Encoder_Fault" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_V17" BitNumber="0" ExternalAccess="Read/Write">
<Description>
<![CDATA[Encoder Faulted or Conveyor is Running at Low Speed]]>
</Description>
</Member>
<Member Name="MCM_JR_PB_Pressed" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_V17" BitNumber="1" ExternalAccess="Read/Write">
<Description>
<![CDATA[Jam Reset PushButton Pressed on MCM]]>
</Description>
</Member>
<Member Name="Disabled" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_V17" BitNumber="2" ExternalAccess="Read/Write">
<Description>
<![CDATA[Conveyor]]>
</Description>
</Member>
<Member Name="MCM_Start_PB_Pressed" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_V17" BitNumber="3" ExternalAccess="Read/Write">
<Description>
<![CDATA[Start PushButton Pressed on MCM]]>
</Description>
</Member>
<Member Name="MCM_EStop_PB_Pressed" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_V17" BitNumber="4" ExternalAccess="Read/Write">
<Description>
<![CDATA[Emergency Stop PushButton Pressed on MCM]]>
</Description>
</Member>
</Members>
</DataType>
<DataType Name="UDT_HMI_STATION" Family="NoFamily" Class="User">
<Members>
<Member Name="Name" DataType="STRING" Dimension="0" Radix="NullType" Hidden="false" ExternalAccess="Read/Write">
<Description>
<![CDATA[Station Name]]>
</Description>
</Member>
<Member Name="MCM_Name" DataType="STRING" Dimension="0" Radix="NullType" Hidden="false" ExternalAccess="Read/Write">
<Description>
<![CDATA[MCM Name]]>
</Description>
</Member>
<Member Name="Conveyor_Name" DataType="STRING" Dimension="0" Radix="NullType" Hidden="false" ExternalAccess="Read/Write">
<Description>
<![CDATA[Conveyor Name]]>
</Description>
</Member>
<Member Name="Alarm" DataType="UDT_ALARMS_STATION" Dimension="0" Radix="NullType" Hidden="false" ExternalAccess="Read/Write">
<Description>
<![CDATA[Station Alarms]]>
</Description>
</Member>
<Member Name="ZZZZZZZZZZUDT_HMI_ST4" DataType="SINT" Dimension="0" Radix="Decimal" Hidden="true" ExternalAccess="Read/Write"/>
<Member Name="Start_PB" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_HMI_ST4" BitNumber="0" ExternalAccess="Read/Write">
<Description>
<![CDATA[Start PushButton]]>
</Description>
</Member>
<Member Name="Stop_PB" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_HMI_ST4" BitNumber="1" ExternalAccess="Read/Write">
<Description>
<![CDATA[Stop PushButton]]>
</Description>
</Member>
<Member Name="Start_Color" DataType="DINT" Dimension="0" Radix="Decimal" Hidden="false" ExternalAccess="Read/Write">
<Description>
<![CDATA[Start Color]]>
</Description>
</Member>
<Member Name="Stop_Color" DataType="DINT" Dimension="0" Radix="Decimal" Hidden="false" ExternalAccess="Read/Write">
<Description>
<![CDATA[Stop Color]]>
</Description>
</Member>
<Member Name="ZZZZZZZZZZUDT_HMI_ST9" DataType="SINT" Dimension="0" Radix="Decimal" Hidden="true" ExternalAccess="Read/Write"/>
<Member Name="JR_PB_LT" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_HMI_ST9" BitNumber="0" ExternalAccess="Read/Write">
<Description>
<![CDATA[Jam Restart PushButton Light]]>
</Description>
</Member>
</Members>
<Dependencies>
<Dependency Type="DataType" Name="UDT_ALARMS_STATION"/>
</Dependencies>
</DataType>
<DataType Use="Target" Name="UDT_ALARMS_STATION" Family="NoFamily" Class="User">
<Members>
<Member Name="ZZZZZZZZZZUDT_ALARMS0" DataType="SINT" Dimension="0" Radix="Decimal" Hidden="true" ExternalAccess="Read/Write"/>
<Member Name="EStopped" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_ALARMS0" BitNumber="0" ExternalAccess="Read/Write">
<Description>
<![CDATA[Conveyor Emergency Stopped]]>
</Description>
</Member>
<Member Name="Stopped" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_ALARMS0" BitNumber="1" ExternalAccess="Read/Write">
<Description>
<![CDATA[Conveyor Stopped]]>
</Description>
</Member>
</Members>
</DataType>
<DataType Use="Target" Name="UDT_AOI_STATION_SS_PB" Family="NoFamily" Class="User">
<Members>
<Member Name="AOI" DataType="AOI_STATION_SS_PB" Dimension="0" Radix="NullType" Hidden="false" ExternalAccess="Read/Write"/>
<Member Name="HMI" DataType="UDT_HMI_STATION" Dimension="0" Radix="NullType" Hidden="false" ExternalAccess="Read/Write"/>
<Member Name="CTRL" DataType="UDT_CTRL_STATION" Dimension="0" Radix="NullType" Hidden="false" ExternalAccess="Read/Write"/>
</Members>
<Dependencies>
<Dependency Type="AddOnInstructionDefinition" Name="AOI_STATION_SS_PB"/>
<Dependency Type="DataType" Name="UDT_HMI_STATION"/>
<Dependency Type="DataType" Name="UDT_CTRL_STATION"/>
</Dependencies>
</DataType>
<DataType Use="Target" Name="UDT_CTRL_STATION" Family="NoFamily" Class="User">
<Members>
<Member Name="CMD" DataType="UDT_CTRL_STATION_CMD" Dimension="0" Radix="NullType" Hidden="false" ExternalAccess="Read/Write"/>
<Member Name="STS" DataType="UDT_CTRL_STATION_STS" Dimension="0" Radix="NullType" Hidden="false" ExternalAccess="Read/Write"/>
</Members>
<Dependencies>
<Dependency Type="DataType" Name="UDT_CTRL_STATION_CMD"/>
<Dependency Type="DataType" Name="UDT_CTRL_STATION_STS"/>
</Dependencies>
</DataType>
<DataType Use="Target" Name="UDT_CTRL_STATION_CMD" Family="NoFamily" Class="User">
<Members>
<Member Name="ZZZZZZZZZZUDT_CTRL_S0" DataType="SINT" Dimension="0" Radix="Decimal" Hidden="true" ExternalAccess="Read/Write"/>
<Member Name="Jammed" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_S0" BitNumber="0" ExternalAccess="Read/Write">
<Description>
<![CDATA[Conveyor]]>
</Description>
</Member>
<Member Name="EStop_Actuated" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_S0" BitNumber="1" ExternalAccess="Read/Write">
<Description>
<![CDATA[Emergency Stop Actuated]]>
</Description>
</Member>
<Member Name="Log" DataType="STRING" Dimension="0" Radix="NullType" Hidden="false" ExternalAccess="Read/Write">
<Description>
<![CDATA[Log]]>
</Description>
</Member>
</Members>
</DataType>
<DataType Use="Target" Name="UDT_CTRL_STATION_STS" Family="NoFamily" Class="User">
<Members>
<Member Name="ZZZZZZZZZZUDT_CTRL_S0" DataType="SINT" Dimension="0" Radix="Decimal" Hidden="true" ExternalAccess="Read/Write"/>
<Member Name="Start" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_S0" BitNumber="0" ExternalAccess="Read/Write">
<Description>
<![CDATA[Start command For/From Partner Stations]]>
</Description>
</Member>
<Member Name="Stop" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_S0" BitNumber="1" ExternalAccess="Read/Write">
<Description>
<![CDATA[Stop command For/From Partner Stations]]>
</Description>
</Member>
<Member Name="EStop_Was_Actuated" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_S0" BitNumber="2" ExternalAccess="Read/Write">
<Description>
<![CDATA[Emergency Stop was Actuated]]>
</Description>
</Member>
<Member Name="Log" DataType="STRING" Dimension="0" Radix="NullType" Hidden="false" ExternalAccess="Read/Write">
<Description>
<![CDATA[Log]]>
</Description>
</Member>
<Member Name="ZZZZZZZZZZUDT_CTRL_S5" DataType="SINT" Dimension="0" Radix="Decimal" Hidden="true" ExternalAccess="Read/Write"/>
<Member Name="JR_PB_LT" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_S5" BitNumber="0" ExternalAccess="Read/Write">
<Description>
<![CDATA[Jam Reset Push Button Light]]>
</Description>
</Member>
<Member Name="Jam_Fault" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_S5" BitNumber="1" ExternalAccess="Read/Write">
<Description>
<![CDATA[Conveyor Jammed]]>
</Description>
</Member>
</Members>
</DataType>
<DataType Use="Target" Name="UDT_HMI_TIPPER" Family="NoFamily" Class="User">
<Members>
<Member Name="Name" DataType="STRING" Dimension="0" Radix="NullType" Hidden="false" ExternalAccess="Read/Write">
<Description>
<![CDATA[Conveyor Name]]>
</Description>
</Member>
<Member Name="MCM_Name" DataType="STRING" Dimension="0" Radix="NullType" Hidden="false" ExternalAccess="Read/Write">
<Description>
<![CDATA[MCM Name]]>
</Description>
</Member>
<Member Name="IP_Address" DataType="STRING" Dimension="0" Radix="NullType" Hidden="false" ExternalAccess="Read/Write">
<Description>
<![CDATA[IP]]>
</Description>
</Member>
<Member Name="Alarm" DataType="UDT_ALARMS_VFD" Dimension="0" Radix="NullType" Hidden="false" ExternalAccess="Read/Write">
<Description>
<![CDATA[Gaylord Alarms]]>
</Description>
</Member>
<Member Name="Color" DataType="DINT" Dimension="0" Radix="Decimal" Hidden="false" ExternalAccess="Read/Write">
<Description>
<![CDATA[HMI Color Animation]]>
</Description>
</Member>
<Member Name="ZZZZZZZZZZUDT_HMI_GA5" DataType="SINT" Dimension="0" Radix="Decimal" Hidden="true" ExternalAccess="Read/Write"/>
<Member Name="MaintStartPB" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_HMI_GA5" BitNumber="0" ExternalAccess="Read/Write">
<Description>
<![CDATA[Maintenance Mode Start Command]]>
</Description>
</Member>
<Member Name="MaintStopPB" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_HMI_GA5" BitNumber="1" ExternalAccess="Read/Write">
<Description>
<![CDATA[Maintenance Mode Stop Command]]>
</Description>
</Member>
<Member Name="MaintJogPB" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_HMI_GA5" BitNumber="2" ExternalAccess="Read/Write">
<Description>
<![CDATA[Maintenance Mode Jog Command]]>
</Description>
</Member>
<Member Name="MaintDirectionPB" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_HMI_GA5" BitNumber="3" ExternalAccess="Read/Write">
<Description>
<![CDATA[Conveyor Direction Command Toggle Button (1 = reverse)]]>
</Description>
</Member>
<Member Name="MaintStartLT" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_HMI_GA5" BitNumber="4" ExternalAccess="Read/Write">
<Description>
<![CDATA[Start light control for run/jog screen]]>
</Description>
</Member>
<Member Name="MaintStopLT" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_HMI_GA5" BitNumber="5" ExternalAccess="Read/Write">
<Description>
<![CDATA[Stop light control for run/jog screen]]>
</Description>
</Member>
<Member Name="MaintJogLT" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_HMI_GA5" BitNumber="6" ExternalAccess="Read/Write">
<Description>
<![CDATA[Maintenance Mode Jog Light]]>
</Description>
</Member>
<Member Name="MaintDirectionLT" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_HMI_GA5" BitNumber="7" ExternalAccess="Read/Write">
<Description>
<![CDATA[Maintenance Direction indicator Light]]>
</Description>
</Member>
<Member Name="ZZZZZZZZZZUDT_HMI_GA14" DataType="SINT" Dimension="0" Radix="Decimal" Hidden="true" ExternalAccess="Read/Write"/>
<Member Name="MaintDirectionVisible" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_HMI_GA14" BitNumber="0" ExternalAccess="Read/Write">
<Description>
<![CDATA[Conveyor Direction Command Button Visible]]>
</Description>
</Member>
<Member Name="MaintBypassPB" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_HMI_GA14" BitNumber="1" ExternalAccess="Read/Write">
<Description>
<![CDATA[Bypass Conveyor, show run signal to prevent flow-stop]]>
</Description>
</Member>
<Member Name="MaintBypassLT" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_HMI_GA14" BitNumber="2" ExternalAccess="Read/Write">
<Description>
<![CDATA[Bypass Conveyor, show run signal to prevent flow-stop]]>
</Description>
</Member>
<Member Name="SpeedAt60Hz" DataType="DINT" Dimension="0" Radix="Decimal" Hidden="false" ExternalAccess="Read/Write">
<Description>
<![CDATA[Speed of Conveyor at 60hz frequency to calculate ratio]]>
</Description>
</Member>
<Member Name="MaintSpeed" DataType="DINT" Dimension="0" Radix="Decimal" Hidden="false" ExternalAccess="Read/Write">
<Description>
<![CDATA[Speed Of Conveyor In Maintenance Mode]]>
</Description>
</Member>
<Member Name="Current" DataType="INT" Dimension="0" Radix="Decimal" Hidden="false" ExternalAccess="Read/Write">
<Description>
<![CDATA[VFD Output Current]]>
</Description>
</Member>
<Member Name="Voltage" DataType="INT" Dimension="0" Radix="Decimal" Hidden="false" ExternalAccess="Read/Write">
<Description>
<![CDATA[VFD Output Voltage]]>
</Description>
</Member>
<Member Name="Frequency" DataType="INT" Dimension="0" Radix="Decimal" Hidden="false" ExternalAccess="Read/Write">
<Description>
<![CDATA[VFD Output Frequency]]>
</Description>
</Member>
<Member Name="FPM" DataType="INT" Dimension="0" Radix="Decimal" Hidden="false" ExternalAccess="Read/Write">
<Description>
<![CDATA[Conveyor FPM]]>
</Description>
</Member>
<Member Name="Speed" DataType="DINT" Dimension="0" Radix="Decimal" Hidden="false" ExternalAccess="Read/Write">
<Description>
<![CDATA[Adjustable Full Speed from GDU]]>
</Description>
</Member>
<Member Name="CommFCode" DataType="DINT" Dimension="0" Radix="Decimal" Hidden="false" ExternalAccess="Read/Write">
<Description>
<![CDATA[VFD Ethernet Fault Code]]>
</Description>
</Member>
<Member Name="MotorFCode" DataType="DINT" Dimension="0" Radix="Decimal" Hidden="false" ExternalAccess="Read/Write">
<Description>
<![CDATA[VFD Fault Code]]>
</Description>
</Member>
<Member Name="LastMotorFCode" DataType="DINT" Dimension="0" Radix="Decimal" Hidden="false" ExternalAccess="Read/Write"/>
<Member Name="StatusVFD" DataType="DINT" Dimension="0" Radix="Decimal" Hidden="false" ExternalAccess="Read/Write"/>
<Member Name="ZZZZZZZZZZUDT_HMI_GA29" DataType="SINT" Dimension="0" Radix="Decimal" Hidden="true" ExternalAccess="Read/Write"/>
<Member Name="MaintMode" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_HMI_GA29" BitNumber="0" ExternalAccess="Read/Write">
<Description>
<![CDATA[Maint Mode Enable]]>
</Description>
</Member>
<Member Name="PowerSaveTime" DataType="DINT" Dimension="0" Radix="Decimal" Hidden="false" ExternalAccess="Read/Write"/>
<Member Name="CurrentkWhday" DataType="REAL" Dimension="0" Radix="Float" Hidden="false" ExternalAccess="Read/Write">
<Description>
<![CDATA[Accumulated output energy of the drive per day in kWh]]>
</Description>
</Member>
</Members>
<Dependencies>
<Dependency Type="DataType" Name="UDT_ALARMS_VFD"/>
</Dependencies>
</DataType>
</DataTypes>
<AddOnInstructionDefinitions Use="Context">
<AddOnInstructionDefinition Name="AOI_FLIP_FLOP" Class="Standard" Revision="1.0" ExecutePrescan="false" ExecutePostscan="false" ExecuteEnableInFalse="false" CreatedDate="2022-03-10T21:16:26.590Z" CreatedBy="DESKTOP-T9CCJM5\autStand" EditedDate="2025-05-21T10:05:03.350Z" EditedBy="LCIBATUMI\ilia.gurielidze" SoftwareRevision="v36.00"
>
<Parameters>
<Parameter Name="EnableIn" TagType="Base" DataType="BOOL" Usage="Input" Radix="Decimal" Required="false" Visible="false" ExternalAccess="Read Only">
<Description>
<![CDATA[Enable Input - System Defined Parameter]]>
</Description>
</Parameter>
<Parameter Name="EnableOut" TagType="Base" DataType="BOOL" Usage="Output" Radix="Decimal" Required="false" Visible="false" ExternalAccess="Read Only">
<Description>
<![CDATA[Enable Output - System Defined Parameter]]>
</Description>
</Parameter>
<Parameter Name="On" TagType="Base" DataType="DINT" Usage="Input" Radix="Decimal" Required="true" Visible="true" ExternalAccess="Read/Write">
<Description>
<![CDATA[Amount of time Beacon is On while Flashing]]>
</Description>
<DefaultData Format="L5K">
<![CDATA[0]]>
</DefaultData>
<DefaultData Format="Decorated">
<DataValue DataType="DINT" Radix="Decimal" Value="0"/>
</DefaultData>
</Parameter>
<Parameter Name="Off" TagType="Base" DataType="DINT" Usage="Input" Radix="Decimal" Required="true" Visible="true" ExternalAccess="Read/Write">
<Description>
<![CDATA[Amount of time Beacon is Off while Flashing]]>
</Description>
<DefaultData Format="L5K">
<![CDATA[0]]>
</DefaultData>
<DefaultData Format="Decorated">
<DataValue DataType="DINT" Radix="Decimal" Value="0"/>
</DefaultData>
</Parameter>
<Parameter Name="Flash" TagType="Base" DataType="BOOL" Usage="Output" Radix="Decimal" Required="false" Visible="true" ExternalAccess="Read Only">
<DefaultData Format="L5K">
<![CDATA[0]]>
</DefaultData>
<DefaultData Format="Decorated">
<DataValue DataType="BOOL" Radix="Decimal" Value="0"/>
</DefaultData>
</Parameter>
</Parameters>
<LocalTags>
<LocalTag Name="Flip" DataType="TIMER" ExternalAccess="None">
<DefaultData Format="L5K">
<![CDATA[[0,0,0]]]>
</DefaultData>
<DefaultData Format="Decorated">
<Structure DataType="TIMER">
<DataValueMember Name="PRE" DataType="DINT" Radix="Decimal" Value="0"/>
<DataValueMember Name="ACC" DataType="DINT" Radix="Decimal" Value="0"/>
<DataValueMember Name="EN" DataType="BOOL" Value="0"/>
<DataValueMember Name="TT" DataType="BOOL" Value="0"/>
<DataValueMember Name="DN" DataType="BOOL" Value="0"/>
</Structure>
</DefaultData>
</LocalTag>
<LocalTag Name="Flop" DataType="TIMER" ExternalAccess="None">
<DefaultData Format="L5K">
<![CDATA[[0,0,0]]]>
</DefaultData>
<DefaultData Format="Decorated">
<Structure DataType="TIMER">
<DataValueMember Name="PRE" DataType="DINT" Radix="Decimal" Value="0"/>
<DataValueMember Name="ACC" DataType="DINT" Radix="Decimal" Value="0"/>
<DataValueMember Name="EN" DataType="BOOL" Value="0"/>
<DataValueMember Name="TT" DataType="BOOL" Value="0"/>
<DataValueMember Name="DN" DataType="BOOL" Value="0"/>
</Structure>
</DefaultData>
</LocalTag>
</LocalTags>
<Routines>
<Routine Name="Logic" Type="RLL">
<RLLContent>
<Rung Number="0" Type="N">
<Text>
<![CDATA[MOVE(On,Flip.PRE)MOVE(Off,Flop.PRE);]]>
</Text>
</Rung>
<Rung Number="1" Type="N">
<Text>
<![CDATA[XIO(Flop.DN)TON(Flip,?,?);]]>
</Text>
</Rung>
<Rung Number="2" Type="N">
<Text>
<![CDATA[XIC(Flip.DN)TON(Flop,?,?);]]>
</Text>
</Rung>
<Rung Number="3" Type="N">
<Text>
<![CDATA[XIC(Flip.DN)OTE(Flash)OTE(EnableOut);]]>
</Text>
</Rung>
</RLLContent>
</Routine>
</Routines>
</AddOnInstructionDefinition>
<AddOnInstructionDefinition Name="AOI_STATION_SS_PB" Class="Standard" Revision="1.0" Vendor="Automation Standard" ExecutePrescan="true" ExecutePostscan="false" ExecuteEnableInFalse="false" CreatedDate="2012-02-01T16:00:09.261Z" CreatedBy="Not Available" EditedDate="2025-05-22T12:51:32.133Z" EditedBy="LCIBATUMI\ilia.gurielidze"
 SoftwareRevision="v36.00">
<Description>
<![CDATA[START/STOP STATION PUSH BUTTON]]>
</Description>
<Parameters>
<Parameter Name="EnableIn" TagType="Base" DataType="BOOL" Usage="Input" Radix="Decimal" Required="false" Visible="false" ExternalAccess="Read Only"/>
<Parameter Name="EnableOut" TagType="Base" DataType="BOOL" Usage="Output" Radix="Decimal" Required="false" Visible="false" ExternalAccess="Read Only"/>
<Parameter Name="HMI" TagType="Base" DataType="UDT_HMI_STATION" Usage="InOut" Required="true" Visible="true" Constant="false"/>
<Parameter Name="CTRL" TagType="Base" DataType="UDT_CTRL_STATION" Usage="InOut" Required="true" Visible="true" Constant="false"/>
<Parameter Name="Partner" TagType="Base" DataType="UDT_CTRL_STATION" Usage="InOut" Required="true" Visible="true" Constant="false"/>
<Parameter Name="Motor" TagType="Base" DataType="UDT_CTRL_VFD" Usage="InOut" Required="true" Visible="true" Constant="false"/>
<Parameter Name="SIO" TagType="Base" DataType="UDT_CTRL_SIO_FIO" Usage="InOut" Required="true" Visible="true" Constant="false"/>
<Parameter Name="In_Start_PB" TagType="Base" DataType="BOOL" Usage="Input" Radix="Decimal" Required="true" Visible="true" ExternalAccess="None">
<Description>
<![CDATA[Start Push Button (NO)]]>
</Description>
<DefaultData Format="L5K">
<![CDATA[0]]>
</DefaultData>
<DefaultData Format="Decorated">
<DataValue DataType="BOOL" Radix="Decimal" Value="0"/>
</DefaultData>
</Parameter>
<Parameter Name="In_Stop_PB" TagType="Base" DataType="BOOL" Usage="Input" Radix="Decimal" Required="true" Visible="true" ExternalAccess="Read/Write">
<Description>
<![CDATA[Stop Push Button (NC)]]>
</Description>
<DefaultData Format="L5K">
<![CDATA[0]]>
</DefaultData>
<DefaultData Format="Decorated">
<DataValue DataType="BOOL" Radix="Decimal" Value="0"/>
</DefaultData>
</Parameter>
<Parameter Name="Out_Beacon_Light" TagType="Base" DataType="BOOL" Usage="Output" Radix="Decimal" Required="true" Visible="true" ExternalAccess="Read Only">
<Description>
<![CDATA[Beacon Light]]>
</Description>
<DefaultData Format="L5K">
<![CDATA[0]]>
</DefaultData>
<DefaultData Format="Decorated">
<DataValue DataType="BOOL" Radix="Decimal" Value="0"/>
</DefaultData>
</Parameter>
<Parameter Name="Stop_Pressed" TagType="Base" DataType="BOOL" Usage="Output" Radix="Decimal" Required="false" Visible="true" ExternalAccess="Read/Write">
<Description>
<![CDATA[Stop Conveyors / System]]>
</Description>
<DefaultData Format="L5K">
<![CDATA[0]]>
</DefaultData>
<DefaultData Format="Decorated">
<DataValue DataType="BOOL" Radix="Decimal" Value="0"/>
</DefaultData>
</Parameter>
</Parameters>
<LocalTags>
<LocalTag Name="Flip_Flop" DataType="AOI_FLIP_FLOP" ExternalAccess="None">
<Description>
<![CDATA[Flip Flop for Flashing Beacon]]>
</Description>
<DefaultData Format="L5K">
<![CDATA[[1,0,0,[0,0,0],[0,0,0]]]]>
</DefaultData>
<DefaultData Format="Decorated">
<Structure DataType="AOI_FLIP_FLOP">
<DataValueMember Name="EnableIn" DataType="BOOL" Value="1"/>
<DataValueMember Name="EnableOut" DataType="BOOL" Value="0"/>
<DataValueMember Name="On" DataType="DINT" Radix="Decimal" Value="0"/>
<DataValueMember Name="Off" DataType="DINT" Radix="Decimal" Value="0"/>
<DataValueMember Name="Flash" DataType="BOOL" Value="0"/>
</Structure>
</DefaultData>
</LocalTag>
<LocalTag Name="Concatenated_String" DataType="STRING" ExternalAccess="None">
<Description>
<![CDATA[String for Log]]>
</Description>
<DefaultData Format="L5K">
<![CDATA[[0,'$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00']]]>
</DefaultData>
<DefaultData Format="String" Length="0">
<![CDATA['']]>
</DefaultData>
</LocalTag>
<LocalTag Name="ONS" DataType="DINT" Radix="Decimal" ExternalAccess="None">
<Description>
<![CDATA[One Shot Instruction to unlatch Stop_pressed when Stop_PB not pressed, command for partner stations started and]]>
</Description>
<DefaultData Format="L5K">
<![CDATA[0]]>
</DefaultData>
<DefaultData Format="Decorated">
<DataValue DataType="DINT" Radix="Decimal" Value="0"/>
</DefaultData>
</LocalTag>
<LocalTag Name="Jam_Latch" DataType="BOOL" Radix="Decimal" ExternalAccess="None">
<Description>
<![CDATA[Sync flashing pilot lights in a group of partned SS stations]]>
</Description>
<DefaultData Format="L5K">
<![CDATA[0]]>
</DefaultData>
<DefaultData Format="Decorated">
<DataValue DataType="BOOL" Radix="Decimal" Value="0"/>
</DefaultData>
</LocalTag>
</LocalTags>
<Routines>
<Routine Name="Logic" Type="RLL">
<RLLContent>
<Rung Number="0" Type="N">
<Text>
<![CDATA[MOVE(CTRL.CMD.Log,CTRL.STS.Log);]]>
</Text>
</Rung>
<Rung Number="1" Type="N">
<Text>
<![CDATA[XIC(CTRL.CMD.EStop_Actuated)OTL(CTRL.STS.EStop_Was_Actuated);]]>
</Text>
</Rung>
<Rung Number="2" Type="N">
<Text>
<![CDATA[[XIC(In_Start_PB) ,XIC(Motor.STS.MCM_Start_PB_Pressed) ]OTU(CTRL.STS.EStop_Was_Actuated);]]>
</Text>
</Rung>
<Rung Number="3" Type="N">
<Text>
<![CDATA[XIC(CTRL.CMD.Jammed)OTE(CTRL.STS.Jam_Fault);]]>
</Text>
</Rung>
<Rung Number="4" Type="N">
<Text>
<![CDATA[[XIO(Motor.STS.In_Power_Saving_Mode) XIC(Motor.STS.Enabled) XIO(CTRL.CMD.Jammed) ,XIO(CTRL.STS.EStop_Was_Actuated) [XIC(CTRL.CMD.Jammed) ,[XIC(Partner.STS.JR_PB_LT) ,XIC(Jam_Latch) ] [XIC(CTRL.CMD.Jammed) ,XIC(Partner.STS.Jam_Fault) ] ] OTE(Jam_Latch) AOI_FLIP_FLOP(Flip_Flop,500,500) ,XIO(Motor.STS.MCM_EStop_PB_Pressed) XIO(CTRL.CMD.EStop_Actuated) XIC(CTRL.STS.EStop_Was_Actuated) AOI_FLIP_FLOP(Flip_Flop,100,100) ,XIC(Motor.STS.In_Power_Saving_Mode) XIO(CTRL.STS.EStop_Was_Actuated) AOI_FLIP_FLOP(Flip_Flop,1000,1000) ]OTE(CTRL.STS.JR_PB_LT)OTE(Out_Beacon_Light);]]>
</Text>
</Rung>
<Rung Number="5" Type="N">
<Comment>
<![CDATA[Commands to Motor]]>
</Comment>
<Text>
<![CDATA[NOP();]]>
</Text>
</Rung>
<Rung Number="6" Type="N">
<Text>
<![CDATA[XIC(In_Stop_PB)[XIC(In_Start_PB) ,XIC(HMI.Start_PB) ,XIC(Motor.STS.MCM_Start_PB_Pressed) XIO(CTRL.STS.Jam_Fault) XIO(Partner.STS.Jam_Fault) ,XIC(Partner.STS.Start) ONS(ONS.0) ][XIC(Stop_Pressed) ,XIC(Motor.STS.In_Power_Saving_Mode) ,XIC(CTRL.STS.Jam_Fault) ,XIC(Partner.STS.Jam_Fault) ]OTE(CTRL.STS.Start)OTU(Motor.STS.In_Power_Saving_Mode)OTL(Motor.CMD.Start)OTU(HMI.Start_PB)OTU(Stop_Pressed);]]>
</Text>
</Rung>
<Rung Number="7" Type="N">
<Text>
<![CDATA[XIC(Motor.STS.MCM_Started)[XIO(SIO.STS.Communication_Fault) XIO(In_Stop_PB) ,XIC(HMI.Stop_PB) ]OTE(CTRL.STS.Stop)OTL(Stop_Pressed)OTU(HMI.Stop_PB);]]>
</Text>
</Rung>
<Rung Number="8" Type="N">
<Text>
<![CDATA[XIC(Stop_Pressed)MOVE(' STOP',Concatenated_String)CONCAT(HMI.Name,Concatenated_String,Motor.CMD.Log)OTL(Motor.CMD.Stop_Require_Start)OTL(Motor.CMD.Stopped_By_Stop_PB)OTE(HMI.Alarm.Stopped);]]>
</Text>
</Rung>
<Rung Number="9" Type="N">
<Comment>
<![CDATA[SS Station HMI Color]]>
</Comment>
<Text>
<![CDATA[NOP();]]>
</Text>
</Rung>
<Rung Number="10" Type="N">
<Text>
<![CDATA[XIO(Out_Beacon_Light)MOVE(4,HMI.Start_Color);]]>
</Text>
</Rung>
<Rung Number="11" Type="N">
<Text>
<![CDATA[XIO(Out_Beacon_Light)[XIC(In_Start_PB) ,XIC(HMI.Start_PB) ]MOVE(3,HMI.Start_Color);]]>
</Text>
</Rung>
<Rung Number="12" Type="N">
<Text>
<![CDATA[XIC(Out_Beacon_Light)MOVE(2,HMI.Start_Color);]]>
</Text>
</Rung>
<Rung Number="13" Type="N">
<Text>
<![CDATA[XIC(Out_Beacon_Light)[XIC(In_Start_PB) ,XIC(HMI.Start_PB) ]MOVE(1,HMI.Start_Color);]]>
</Text>
</Rung>
<Rung Number="14" Type="N">
<Text>
<![CDATA[NOP();]]>
</Text>
</Rung>
<Rung Number="15" Type="N">
<Text>
<![CDATA[XIO(Stop_Pressed)MOVE(4,HMI.Stop_Color);]]>
</Text>
</Rung>
<Rung Number="16" Type="N">
<Text>
<![CDATA[XIO(Stop_Pressed)[XIO(In_Stop_PB) ,XIC(HMI.Stop_PB) ]MOVE(3,HMI.Stop_Color);]]>
</Text>
</Rung>
<Rung Number="17" Type="N">
<Text>
<![CDATA[XIC(Stop_Pressed)MOVE(2,HMI.Stop_Color);]]>
</Text>
</Rung>
<Rung Number="18" Type="N">
<Text>
<![CDATA[XIC(Stop_Pressed)[XIO(In_Stop_PB) ,XIC(HMI.Stop_PB) ]MOVE(1,HMI.Stop_Color);]]>
</Text>
</Rung>
<Rung Number="19" Type="N">
<Text>
<![CDATA[OTU(CTRL.CMD.EStop_Actuated)OTU(CTRL.CMD.Jammed)MOVE('',CTRL.CMD.Log);]]>
</Text>
</Rung>
</RLLContent>
</Routine>
<Routine Name="Prescan" Type="RLL">
<RLLContent>
<Rung Number="0" Type="N">
<Text>
<![CDATA[NOP();]]>
</Text>
</Rung>
<Rung Number="1" Type="N">
<Text>
<![CDATA[FLL(0,HMI.Alarm,1)OTU(HMI.Start_PB)OTU(HMI.Stop_PB)OTU(Stop_Pressed);]]>
</Text>
</Rung>
</RLLContent>
</Routine>
</Routines>
<Dependencies>
<Dependency Type="DataType" Name="UDT_CTRL_STATION"/>
<Dependency Type="AddOnInstructionDefinition" Name="AOI_FLIP_FLOP"/>
<Dependency Type="DataType" Name="UDT_HMI_STATION"/>
<Dependency Type="DataType" Name="UDT_CTRL_VFD"/>
<Dependency Type="DataType" Name="UDT_CTRL_SIO_FIO"/>
</Dependencies>
</AddOnInstructionDefinition>
</AddOnInstructionDefinitions>
</Controller>
</RSLogix5000Content>
