<?xml version="1.0" encoding="UTF-8" standalone="yes"?>
<!--TIPPER-->
<RSLogix5000Content SchemaRevision="1.0" SoftwareRevision="36.00" TargetName="AOI_TIPPER" TargetType="AddOnInstructionDefinition" TargetClass="Standard" TargetRevision="1.0 " TargetLastEdited="2025-05-22T12:52:09.134Z" ContainsContext="true" ExportDate="Fri May 23 22:12:30 2025" ExportOptions="References NoRawData L5KData DecoratedData Context Dependencies ForceProtectedEncoding AllProjDocTrans">
<Controller Use="Context" Name="MTN6_Simulations">
<DataTypes Use="Context">
<DataType Name="UDT_ALARMS_VFD" Family="NoFamily" Class="User">
<Members>
<Member Name="ZZZZZZZZZZUDT_ALARMS0" DataType="SINT" Dimension="0" Radix="Decimal" Hidden="true" ExternalAccess="Read/Write"/>
<Member Name="Communication_Fault" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_ALARMS0" BitNumber="0" ExternalAccess="Read/Write">
<Description>
<![CDATA[Ethernet Communication is Faulted]]>
</Description>
</Member>
<Member Name="Disconnected" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_ALARMS0" BitNumber="1" ExternalAccess="Read/Write">
<Description>
<![CDATA[Disconnected VFD]]>
</Description>
</Member>
<Member Name="VFD_Fault" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_ALARMS0" BitNumber="2" ExternalAccess="Read/Write">
<Description>
<![CDATA[VFD Faulted]]>
</Description>
</Member>
<Member Name="Safe_Off_Fault" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_ALARMS0" BitNumber="3" ExternalAccess="Read/Write">
<Description>
<![CDATA[VFD Safety Torque Fault]]>
</Description>
</Member>
<Member Name="Reset_VFD" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_ALARMS0" BitNumber="4" ExternalAccess="Read/Write">
<Description>
<![CDATA[VFD Reset]]>
</Description>
</Member>
<Member Name="Reset_Communication_Fault" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_ALARMS0" BitNumber="5" ExternalAccess="Read/Write">
<Description>
<![CDATA[Reset Comunication Fault]]>
</Description>
</Member>
</Members>
</DataType>
<DataType Name="UDT_CTRL_MCM" Family="NoFamily" Class="User">
<Members>
<Member Name="CMD" DataType="UDT_CTRL_MCM_CMD" Dimension="0" Radix="NullType" Hidden="false" ExternalAccess="Read/Write">
<Description>
<![CDATA[Command To MCM]]>
</Description>
</Member>
<Member Name="STS" DataType="UDT_CTRL_MCM_STS" Dimension="0" Radix="NullType" Hidden="false" ExternalAccess="Read/Write">
<Description>
<![CDATA[Status From MCM]]>
</Description>
</Member>
</Members>
<Dependencies>
<Dependency Type="DataType" Name="UDT_CTRL_MCM_CMD"/>
<Dependency Type="DataType" Name="UDT_CTRL_MCM_STS"/>
</Dependencies>
</DataType>
<DataType Name="UDT_CTRL_MCM_CMD" Family="NoFamily" Class="User">
<Members>
<Member Name="ZZZZZZZZZZUDT_CTRL_M0" DataType="SINT" Dimension="0" Radix="Decimal" Hidden="true" ExternalAccess="Read/Write"/>
<Member Name="EStop_Actuated" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_M0" BitNumber="0" ExternalAccess="Read/Write">
<Description>
<![CDATA[Emergency Stop Actuated]]>
</Description>
</Member>
<Member Name="Started" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_M0" BitNumber="1" ExternalAccess="Read/Write">
<Description>
<![CDATA[MCM]]>
</Description>
</Member>
<Member Name="Maintenance_Mode" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_M0" BitNumber="2" ExternalAccess="Read/Write">
<Description>
<![CDATA[In Maitenance Mode]]>
</Description>
</Member>
<Member Name="Jam_Fault" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_M0" BitNumber="3" ExternalAccess="Read/Write">
<Description>
<![CDATA[Conveyor is Jammed]]>
</Description>
</Member>
<Member Name="Communication_Was_Faulted" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_M0" BitNumber="4" ExternalAccess="Read/Write">
<Description>
<![CDATA[Ethernet Communication was Faulted]]>
</Description>
</Member>
<Member Name="VFD_Was_Faulted" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_M0" BitNumber="5" ExternalAccess="Read/Write">
<Description>
<![CDATA[VFD Was Faulted]]>
</Description>
</Member>
<Member Name="EStop_Was_Actuated" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_M0" BitNumber="6" ExternalAccess="Read/Write">
<Description>
<![CDATA[Emergency Stop was Actuated]]>
</Description>
</Member>
<Member Name="Log" DataType="STRING" Dimension="0" Radix="NullType" Hidden="false" ExternalAccess="Read/Write">
<Description>
<![CDATA[Log]]>
</Description>
</Member>
<Member Name="ZZZZZZZZZZUDT_CTRL_M9" DataType="SINT" Dimension="0" Radix="Decimal" Hidden="true" ExternalAccess="Read/Write"/>
<Member Name="Acknowledge_Log" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_M9" BitNumber="0" ExternalAccess="Read/Write">
<Description>
<![CDATA[Acknowledge Log]]>
</Description>
</Member>
<Member Name="All_Unacknowledge_Log" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_M9" BitNumber="1" ExternalAccess="Read/Write">
<Description>
<![CDATA[All Unacknowledge Logs]]>
</Description>
</Member>
<Member Name="VFD_Faulted" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_M9" BitNumber="2" ExternalAccess="Read/Write">
<Description>
<![CDATA[VFD Faulted]]>
</Description>
</Member>
<Member Name="Communication_Faulted" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_M9" BitNumber="3" ExternalAccess="Read/Write">
<Description>
<![CDATA[Ethernet Communication Faulted]]>
</Description>
</Member>
<Member Name="Log_Quantity" DataType="DINT" Dimension="0" Radix="Decimal" Hidden="false" ExternalAccess="Read/Write">
<Description>
<![CDATA[Log Quantity]]>
</Description>
</Member>
<Member Name="ZZZZZZZZZZUDT_CTRL_M15" DataType="SINT" Dimension="0" Radix="Decimal" Hidden="true" ExternalAccess="Read/Write"/>
<Member Name="VFD_In_Power_Saving_Mode" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_M15" BitNumber="0" ExternalAccess="Read/Write">
<Description>
<![CDATA[VFD in Power Saving Mode]]>
</Description>
</Member>
<Member Name="Encoder_Fault" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_M15" BitNumber="1" ExternalAccess="Read/Write">
<Description>
<![CDATA[Encoder Faulted or Conveyor is running at Low Speed]]>
</Description>
</Member>
<Member Name="LAP_PB" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_M15" BitNumber="2" ExternalAccess="Read/Write">
<Description>
<![CDATA[Low Air Pressure PushButton]]>
</Description>
</Member>
<Member Name="LAP_PB_LT" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_M15" BitNumber="3" ExternalAccess="Read/Write">
<Description>
<![CDATA[Low Air Pressure PushButton Light]]>
</Description>
</Member>
<Member Name="Start_PB" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_M15" BitNumber="4" ExternalAccess="Read/Write">
<Description>
<![CDATA[Start PushButton]]>
</Description>
</Member>
<Member Name="Stop_PB" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_M15" BitNumber="5" ExternalAccess="Read/Write">
<Description>
<![CDATA[Stop PushButton]]>
</Description>
</Member>
<Member Name="VFD_Fault_Reset_PB" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_M15" BitNumber="6" ExternalAccess="Read/Write">
<Description>
<![CDATA[VFD Fault Reset PushButton]]>
</Description>
</Member>
<Member Name="Jam_Restart_PB" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_M15" BitNumber="7" ExternalAccess="Read/Write">
<Description>
<![CDATA[Jam Reset PushButton]]>
</Description>
</Member>
<Member Name="ZZZZZZZZZZUDT_CTRL_M24" DataType="SINT" Dimension="0" Radix="Decimal" Hidden="true" ExternalAccess="Read/Write"/>
<Member Name="EStop_PB" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_M24" BitNumber="0" ExternalAccess="Read/Write">
<Description>
<![CDATA[Emergency Stop PushButton]]>
</Description>
</Member>
</Members>
</DataType>
<DataType Name="UDT_CTRL_MCM_STS" Family="NoFamily" Class="User">
<Members>
<Member Name="ZZZZZZZZZZUDT_CTRL_M0" DataType="SINT" Dimension="0" Radix="Decimal" Hidden="true" ExternalAccess="Read/Write"/>
<Member Name="EStopped" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_M0" BitNumber="0" ExternalAccess="Read/Write">
<Description>
<![CDATA[Emergency Stopped]]>
</Description>
</Member>
<Member Name="Maintenance_Mode" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_M0" BitNumber="1" ExternalAccess="Read/Write">
<Description>
<![CDATA[In Maitenance Mode]]>
</Description>
</Member>
<Member Name="System_Started" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_M0" BitNumber="2" ExternalAccess="Read/Write">
<Description>
<![CDATA[The System is Started]]>
</Description>
</Member>
<Member Name="VFD_Faulted" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_M0" BitNumber="3" ExternalAccess="Read/Write">
<Description>
<![CDATA[VFD Faulted]]>
</Description>
</Member>
<Member Name="Jam_Fault" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_M0" BitNumber="4" ExternalAccess="Read/Write">
<Description>
<![CDATA[Conveyor Jammed]]>
</Description>
</Member>
<Member Name="Communication_Fault" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_M0" BitNumber="5" ExternalAccess="Read/Write">
<Description>
<![CDATA[Ethernet Communication Faulted]]>
</Description>
</Member>
<Member Name="Log" DataType="STRING" Dimension="0" Radix="NullType" Hidden="false" ExternalAccess="Read/Write">
<Description>
<![CDATA[Log]]>
</Description>
</Member>
<Member Name="Acknowledge_Log" DataType="STRING" Dimension="0" Radix="NullType" Hidden="false" ExternalAccess="Read/Write">
<Description>
<![CDATA[Acknowledge Log]]>
</Description>
</Member>
<Member Name="ZZZZZZZZZZUDT_CTRL_M9" DataType="SINT" Dimension="0" Radix="Decimal" Hidden="true" ExternalAccess="Read/Write"/>
<Member Name="All_Unacknowledge_Log" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_M9" BitNumber="0" ExternalAccess="Read/Write">
<Description>
<![CDATA[All Unacknowledged Logs]]>
</Description>
</Member>
<Member Name="Start_Request" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_M9" BitNumber="1" ExternalAccess="Read/Write">
<Description>
<![CDATA[System Start Requested]]>
</Description>
</Member>
<Member Name="Log_Quantity" DataType="DINT" Dimension="0" Radix="Decimal" Hidden="false" ExternalAccess="Read/Write">
<Description>
<![CDATA[Log Quantity]]>
</Description>
</Member>
<Member Name="ZZZZZZZZZZUDT_CTRL_M13" DataType="SINT" Dimension="0" Radix="Decimal" Hidden="true" ExternalAccess="Read/Write"/>
<Member Name="Encoder_Fault" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_M13" BitNumber="0" ExternalAccess="Read/Write">
<Description>
<![CDATA[Encoder Faulted or Conveyor is running at Low Speed]]>
</Description>
</Member>
<Member Name="LAP_PB" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_M13" BitNumber="1" ExternalAccess="Read/Write">
<Description>
<![CDATA[Low Air Pressure PushButton]]>
</Description>
</Member>
<Member Name="LAP_PB_LT" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_M13" BitNumber="2" ExternalAccess="Read/Write">
<Description>
<![CDATA[Low Air Pressure PushButton Light]]>
</Description>
</Member>
<Member Name="Start_PB" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_M13" BitNumber="3" ExternalAccess="Read/Write">
<Description>
<![CDATA[Start PushButton]]>
</Description>
</Member>
<Member Name="Stop_PB" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_M13" BitNumber="4" ExternalAccess="Read/Write">
<Description>
<![CDATA[Stop PushButton]]>
</Description>
</Member>
<Member Name="Motor_Fault_Reset_PB" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_M13" BitNumber="5" ExternalAccess="Read/Write">
<Description>
<![CDATA[Motor Fault Reset PushButton]]>
</Description>
</Member>
<Member Name="Jam_Restart_PB" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_M13" BitNumber="6" ExternalAccess="Read/Write">
<Description>
<![CDATA[Jam Restart PushButton]]>
</Description>
</Member>
<Member Name="EStop_PB" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_M13" BitNumber="7" ExternalAccess="Read/Write">
<Description>
<![CDATA[Emergency Stop PushButton]]>
</Description>
</Member>
<Member Name="ZZZZZZZZZZUDT_CTRL_M22" DataType="SINT" Dimension="0" Radix="Decimal" Hidden="true" ExternalAccess="Read/Write"/>
<Member Name="Unacknowldge_All" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_M22" BitNumber="0" ExternalAccess="Read/Write">
<Description>
<![CDATA[Unacknowledge all Alarms]]>
</Description>
</Member>
<Member Name="Aknowledgement_ID" DataType="STRING" Dimension="0" Radix="NullType" Hidden="false" ExternalAccess="Read/Write">
<Description>
<![CDATA[Aknowledgement ID]]>
</Description>
</Member>
<Member Name="ZZZZZZZZZZUDT_CTRL_M25" DataType="SINT" Dimension="0" Radix="Decimal" Hidden="true" ExternalAccess="Read/Write"/>
<Member Name="Setup_Speeds" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_M25" BitNumber="0" ExternalAccess="Read/Write">
<Description>
<![CDATA[Set Up Speeds of Conveyors]]>
</Description>
</Member>
</Members>
</DataType>
<DataType Name="UDT_CTRL_TIPPER" Family="NoFamily" Class="User">
<Members>
<Member Name="CMD" DataType="UDT_CTRL_TIPPER_CMD" Dimension="0" Radix="NullType" Hidden="false" ExternalAccess="Read/Write"/>
<Member Name="STS" DataType="UDT_CTRL_TIPPER_STS" Dimension="0" Radix="NullType" Hidden="false" ExternalAccess="Read/Write"/>
</Members>
<Dependencies>
<Dependency Type="DataType" Name="UDT_CTRL_TIPPER_CMD"/>
<Dependency Type="DataType" Name="UDT_CTRL_TIPPER_STS"/>
</Dependencies>
</DataType>
<DataType Name="UDT_CTRL_TIPPER_CMD" Family="NoFamily" Class="User">
<Members>
<Member Name="ZZZZZZZZZZUDT_CTRL_T0" DataType="SINT" Dimension="0" Radix="Decimal" Hidden="true" ExternalAccess="Read/Write"/>
<Member Name="Start" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_T0" BitNumber="0" ExternalAccess="Read/Write">
<Description>
<![CDATA[Start Motor Command]]>
</Description>
</Member>
<Member Name="Stop_Require_Start" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_T0" BitNumber="1" ExternalAccess="Read/Write">
<Description>
<![CDATA[Stops the Motor, requires Start Command to Restart]]>
</Description>
</Member>
<Member Name="Stop_Auto_Restart" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_T0" BitNumber="2" ExternalAccess="Read/Write">
<Description>
<![CDATA[Stops the Motor, Starts Automaticaly]]>
</Description>
</Member>
<Member Name="Jammed" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_T0" BitNumber="3" ExternalAccess="Read/Write">
<Description>
<![CDATA[Motor]]>
</Description>
</Member>
<Member Name="Disable" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_T0" BitNumber="4" ExternalAccess="Read/Write">
<Description>
<![CDATA[Motor]]>
</Description>
</Member>
<Member Name="Run_Up" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_T0" BitNumber="5" ExternalAccess="Read/Write">
<Description>
<![CDATA[When Downsream Conveyors are Stopped, Conveyor keeps Running  untill Discharge PE is Blocked]]>
</Description>
</Member>
<Member Name="Power_Saving_Mode" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_T0" BitNumber="6" ExternalAccess="Read/Write">
<Description>
<![CDATA[In Power Saving Mode]]>
</Description>
</Member>
<Member Name="Interlock" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_T0" BitNumber="7" ExternalAccess="Read/Write">
<Description>
<![CDATA[Downstream is Running]]>
</Description>
</Member>
<Member Name="ZZZZZZZZZZUDT_CTRL_T9" DataType="SINT" Dimension="0" Radix="Decimal" Hidden="true" ExternalAccess="Read/Write"/>
<Member Name="Stopped_By_MCM_Stop_PB" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_T9" BitNumber="0" ExternalAccess="Read/Write">
<Description>
<![CDATA[Motor Stopped by MCM Stop Push Button]]>
</Description>
</Member>
<Member Name="Log" DataType="STRING" Dimension="0" Radix="NullType" Hidden="false" ExternalAccess="Read/Write">
<Description>
<![CDATA[Log]]>
</Description>
</Member>
<Member Name="Acknoledgement_ID" DataType="STRING" Dimension="0" Radix="NullType" Hidden="false" ExternalAccess="Read/Write">
<Description>
<![CDATA[Aknowledgement ID]]>
</Description>
</Member>
<Member Name="ZZZZZZZZZZUDT_CTRL_T13" DataType="SINT" Dimension="0" Radix="Decimal" Hidden="true" ExternalAccess="Read/Write"/>
<Member Name="Full" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_T13" BitNumber="0" ExternalAccess="Read/Write">
<Description>
<![CDATA[Conveyor]]>
</Description>
</Member>
<Member Name="Encoder_Fault" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_T13" BitNumber="1" ExternalAccess="Read/Write">
<Description>
<![CDATA[Encode Faulted or Conveyor is Running at Low Speed]]>
</Description>
</Member>
<Member Name="Speed_FPM" DataType="DINT" Dimension="0" Radix="Decimal" Hidden="false" ExternalAccess="Read/Write">
<Description>
<![CDATA[Speed of Conveyor in Feet Per Minute]]>
</Description>
</Member>
</Members>
</DataType>
<DataType Name="UDT_CTRL_TIPPER_STS" Family="NoFamily" Class="User">
<Members>
<Member Name="ZZZZZZZZZZUDT_CTRL_T0" DataType="SINT" Dimension="0" Radix="Decimal" Hidden="true" ExternalAccess="Read/Write"/>
<Member Name="Running" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_T0" BitNumber="0" ExternalAccess="Read/Write">
<Description>
<![CDATA[Tipper]]>
</Description>
</Member>
<Member Name="VFD_Fault" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_T0" BitNumber="1" ExternalAccess="Read/Write">
<Description>
<![CDATA[Tipper VFD Fault]]>
</Description>
</Member>
<Member Name="Communication_Fault" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_T0" BitNumber="2" ExternalAccess="Read/Write">
<Description>
<![CDATA[Communication Fault]]>
</Description>
</Member>
<Member Name="Interlock" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_T0" BitNumber="3" ExternalAccess="Read/Write">
<Description>
<![CDATA[Downstream Conveyor Running]]>
</Description>
</Member>
<Member Name="Current_Speed" DataType="DINT" Dimension="0" Radix="Decimal" Hidden="false" ExternalAccess="Read/Write">
<Description>
<![CDATA[Current Speed of conveyor in FPM]]>
</Description>
</Member>
<Member Name="Requested_Speed" DataType="DINT" Dimension="0" Radix="Decimal" Hidden="false" ExternalAccess="Read/Write">
<Description>
<![CDATA[Requested Speed of Conveyor in FPM]]>
</Description>
</Member>
<Member Name="ZZZZZZZZZZUDT_CTRL_T7" DataType="SINT" Dimension="0" Radix="Decimal" Hidden="true" ExternalAccess="Read/Write"/>
<Member Name="In_Maintenance_Mode" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_T7" BitNumber="0" ExternalAccess="Read/Write">
<Description>
<![CDATA[Tipper in Maintenance Mode]]>
</Description>
</Member>
<Member Name="MCM_Started" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_T7" BitNumber="1" ExternalAccess="Read/Write">
<Description>
<![CDATA[MCM Started]]>
</Description>
</Member>
<Member Name="Disabled" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_T7" BitNumber="2" ExternalAccess="Read/Write">
<Description>
<![CDATA[Tipper]]>
</Description>
</Member>
<Member Name="Jammed" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_T7" BitNumber="3" ExternalAccess="Read/Write">
<Description>
<![CDATA[Tipper]]>
</Description>
</Member>
<Member Name="Full" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_T7" BitNumber="4" ExternalAccess="Read/Write">
<Description>
<![CDATA[Tipper]]>
</Description>
</Member>
<Member Name="Run_Enabled" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_T7" BitNumber="5" ExternalAccess="Read/Write">
<Description>
<![CDATA[Tipper can Run]]>
</Description>
</Member>
<Member Name="Stopped_MCM_Stop_PB" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_T7" BitNumber="6" ExternalAccess="Read/Write">
<Description>
<![CDATA[Stopped by Stop PushButton on MCM]]>
</Description>
</Member>
<Member Name="Log" DataType="STRING" Dimension="0" Radix="NullType" Hidden="false" ExternalAccess="Read/Write">
<Description>
<![CDATA[Log]]>
</Description>
</Member>
<Member Name="ZZZZZZZZZZUDT_CTRL_T16" DataType="SINT" Dimension="0" Radix="Decimal" Hidden="true" ExternalAccess="Read/Write"/>
<Member Name="No_Motor" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_T16" BitNumber="0" ExternalAccess="Read/Write">
<Description>
<![CDATA[Tipper has no Motor]]>
</Description>
</Member>
<Member Name="Encoder_Fault" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_T16" BitNumber="1" ExternalAccess="Read/Write">
<Description>
<![CDATA[Encode Faulted or Tipper is Runnning at Low Speed]]>
</Description>
</Member>
<Member Name="Dumping" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_T16" BitNumber="2" ExternalAccess="Read/Write">
<Description>
<![CDATA[Tipper]]>
</Description>
</Member>
</Members>
</DataType>
<DataType Name="UDT_HMI_TIPPER" Family="NoFamily" Class="User">
<Members>
<Member Name="Name" DataType="STRING" Dimension="0" Radix="NullType" Hidden="false" ExternalAccess="Read/Write">
<Description>
<![CDATA[Conveyor Name]]>
</Description>
</Member>
<Member Name="MCM_Name" DataType="STRING" Dimension="0" Radix="NullType" Hidden="false" ExternalAccess="Read/Write">
<Description>
<![CDATA[MCM Name]]>
</Description>
</Member>
<Member Name="IP_Address" DataType="STRING" Dimension="0" Radix="NullType" Hidden="false" ExternalAccess="Read/Write">
<Description>
<![CDATA[IP]]>
</Description>
</Member>
<Member Name="Alarm" DataType="UDT_ALARMS_VFD" Dimension="0" Radix="NullType" Hidden="false" ExternalAccess="Read/Write">
<Description>
<![CDATA[Gaylord Alarms]]>
</Description>
</Member>
<Member Name="Color" DataType="DINT" Dimension="0" Radix="Decimal" Hidden="false" ExternalAccess="Read/Write">
<Description>
<![CDATA[HMI Color Animation]]>
</Description>
</Member>
<Member Name="ZZZZZZZZZZUDT_HMI_GA5" DataType="SINT" Dimension="0" Radix="Decimal" Hidden="true" ExternalAccess="Read/Write"/>
<Member Name="MaintStartPB" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_HMI_GA5" BitNumber="0" ExternalAccess="Read/Write">
<Description>
<![CDATA[Maintenance Mode Start Command]]>
</Description>
</Member>
<Member Name="MaintStopPB" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_HMI_GA5" BitNumber="1" ExternalAccess="Read/Write">
<Description>
<![CDATA[Maintenance Mode Stop Command]]>
</Description>
</Member>
<Member Name="MaintJogPB" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_HMI_GA5" BitNumber="2" ExternalAccess="Read/Write">
<Description>
<![CDATA[Maintenance Mode Jog Command]]>
</Description>
</Member>
<Member Name="MaintDirectionPB" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_HMI_GA5" BitNumber="3" ExternalAccess="Read/Write">
<Description>
<![CDATA[Conveyor Direction Command Toggle Button (1 = reverse)]]>
</Description>
</Member>
<Member Name="MaintStartLT" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_HMI_GA5" BitNumber="4" ExternalAccess="Read/Write">
<Description>
<![CDATA[Start light control for run/jog screen]]>
</Description>
</Member>
<Member Name="MaintStopLT" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_HMI_GA5" BitNumber="5" ExternalAccess="Read/Write">
<Description>
<![CDATA[Stop light control for run/jog screen]]>
</Description>
</Member>
<Member Name="MaintJogLT" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_HMI_GA5" BitNumber="6" ExternalAccess="Read/Write">
<Description>
<![CDATA[Maintenance Mode Jog Light]]>
</Description>
</Member>
<Member Name="MaintDirectionLT" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_HMI_GA5" BitNumber="7" ExternalAccess="Read/Write">
<Description>
<![CDATA[Maintenance Direction indicator Light]]>
</Description>
</Member>
<Member Name="ZZZZZZZZZZUDT_HMI_GA14" DataType="SINT" Dimension="0" Radix="Decimal" Hidden="true" ExternalAccess="Read/Write"/>
<Member Name="MaintDirectionVisible" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_HMI_GA14" BitNumber="0" ExternalAccess="Read/Write">
<Description>
<![CDATA[Conveyor Direction Command Button Visible]]>
</Description>
</Member>
<Member Name="MaintBypassPB" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_HMI_GA14" BitNumber="1" ExternalAccess="Read/Write">
<Description>
<![CDATA[Bypass Conveyor, show run signal to prevent flow-stop]]>
</Description>
</Member>
<Member Name="MaintBypassLT" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_HMI_GA14" BitNumber="2" ExternalAccess="Read/Write">
<Description>
<![CDATA[Bypass Conveyor, show run signal to prevent flow-stop]]>
</Description>
</Member>
<Member Name="SpeedAt60Hz" DataType="DINT" Dimension="0" Radix="Decimal" Hidden="false" ExternalAccess="Read/Write">
<Description>
<![CDATA[Speed of Conveyor at 60hz frequency to calculate ratio]]>
</Description>
</Member>
<Member Name="MaintSpeed" DataType="DINT" Dimension="0" Radix="Decimal" Hidden="false" ExternalAccess="Read/Write">
<Description>
<![CDATA[Speed Of Conveyor In Maintenance Mode]]>
</Description>
</Member>
<Member Name="Current" DataType="INT" Dimension="0" Radix="Decimal" Hidden="false" ExternalAccess="Read/Write">
<Description>
<![CDATA[VFD Output Current]]>
</Description>
</Member>
<Member Name="Voltage" DataType="INT" Dimension="0" Radix="Decimal" Hidden="false" ExternalAccess="Read/Write">
<Description>
<![CDATA[VFD Output Voltage]]>
</Description>
</Member>
<Member Name="Frequency" DataType="INT" Dimension="0" Radix="Decimal" Hidden="false" ExternalAccess="Read/Write">
<Description>
<![CDATA[VFD Output Frequency]]>
</Description>
</Member>
<Member Name="FPM" DataType="INT" Dimension="0" Radix="Decimal" Hidden="false" ExternalAccess="Read/Write">
<Description>
<![CDATA[Conveyor FPM]]>
</Description>
</Member>
<Member Name="Speed" DataType="DINT" Dimension="0" Radix="Decimal" Hidden="false" ExternalAccess="Read/Write">
<Description>
<![CDATA[Adjustable Full Speed from GDU]]>
</Description>
</Member>
<Member Name="CommFCode" DataType="DINT" Dimension="0" Radix="Decimal" Hidden="false" ExternalAccess="Read/Write">
<Description>
<![CDATA[VFD Ethernet Fault Code]]>
</Description>
</Member>
<Member Name="MotorFCode" DataType="DINT" Dimension="0" Radix="Decimal" Hidden="false" ExternalAccess="Read/Write">
<Description>
<![CDATA[VFD Fault Code]]>
</Description>
</Member>
<Member Name="LastMotorFCode" DataType="DINT" Dimension="0" Radix="Decimal" Hidden="false" ExternalAccess="Read/Write"/>
<Member Name="StatusVFD" DataType="DINT" Dimension="0" Radix="Decimal" Hidden="false" ExternalAccess="Read/Write"/>
<Member Name="ZZZZZZZZZZUDT_HMI_GA29" DataType="SINT" Dimension="0" Radix="Decimal" Hidden="true" ExternalAccess="Read/Write"/>
<Member Name="MaintMode" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_HMI_GA29" BitNumber="0" ExternalAccess="Read/Write">
<Description>
<![CDATA[Maint Mode Enable]]>
</Description>
</Member>
<Member Name="PowerSaveTime" DataType="DINT" Dimension="0" Radix="Decimal" Hidden="false" ExternalAccess="Read/Write"/>
<Member Name="CurrentkWhday" DataType="REAL" Dimension="0" Radix="Float" Hidden="false" ExternalAccess="Read/Write">
<Description>
<![CDATA[Accumulated output energy of the drive per day in kWh]]>
</Description>
</Member>
</Members>
<Dependencies>
<Dependency Type="DataType" Name="UDT_ALARMS_VFD"/>
</Dependencies>
</DataType>
</DataTypes>
<AddOnInstructionDefinitions Use="Context">
<AddOnInstructionDefinition Name="AOI_FLIP_FLOP" Class="Standard" Revision="1.0" ExecutePrescan="false" ExecutePostscan="false" ExecuteEnableInFalse="false" CreatedDate="2022-03-10T21:16:26.590Z" CreatedBy="DESKTOP-T9CCJM5\autStand" EditedDate="2025-05-21T10:05:03.350Z" EditedBy="LCIBATUMI\ilia.gurielidze" SoftwareRevision="v36.00"
>
<Parameters>
<Parameter Name="EnableIn" TagType="Base" DataType="BOOL" Usage="Input" Radix="Decimal" Required="false" Visible="false" ExternalAccess="Read Only">
<Description>
<![CDATA[Enable Input - System Defined Parameter]]>
</Description>
</Parameter>
<Parameter Name="EnableOut" TagType="Base" DataType="BOOL" Usage="Output" Radix="Decimal" Required="false" Visible="false" ExternalAccess="Read Only">
<Description>
<![CDATA[Enable Output - System Defined Parameter]]>
</Description>
</Parameter>
<Parameter Name="On" TagType="Base" DataType="DINT" Usage="Input" Radix="Decimal" Required="true" Visible="true" ExternalAccess="Read/Write">
<Description>
<![CDATA[Amount of time Beacon is On while Flashing]]>
</Description>
<DefaultData Format="L5K">
<![CDATA[0]]>
</DefaultData>
<DefaultData Format="Decorated">
<DataValue DataType="DINT" Radix="Decimal" Value="0"/>
</DefaultData>
</Parameter>
<Parameter Name="Off" TagType="Base" DataType="DINT" Usage="Input" Radix="Decimal" Required="true" Visible="true" ExternalAccess="Read/Write">
<Description>
<![CDATA[Amount of time Beacon is Off while Flashing]]>
</Description>
<DefaultData Format="L5K">
<![CDATA[0]]>
</DefaultData>
<DefaultData Format="Decorated">
<DataValue DataType="DINT" Radix="Decimal" Value="0"/>
</DefaultData>
</Parameter>
<Parameter Name="Flash" TagType="Base" DataType="BOOL" Usage="Output" Radix="Decimal" Required="false" Visible="true" ExternalAccess="Read Only">
<DefaultData Format="L5K">
<![CDATA[0]]>
</DefaultData>
<DefaultData Format="Decorated">
<DataValue DataType="BOOL" Radix="Decimal" Value="0"/>
</DefaultData>
</Parameter>
</Parameters>
<LocalTags>
<LocalTag Name="Flip" DataType="TIMER" ExternalAccess="None">
<DefaultData Format="L5K">
<![CDATA[[0,0,0]]]>
</DefaultData>
<DefaultData Format="Decorated">
<Structure DataType="TIMER">
<DataValueMember Name="PRE" DataType="DINT" Radix="Decimal" Value="0"/>
<DataValueMember Name="ACC" DataType="DINT" Radix="Decimal" Value="0"/>
<DataValueMember Name="EN" DataType="BOOL" Value="0"/>
<DataValueMember Name="TT" DataType="BOOL" Value="0"/>
<DataValueMember Name="DN" DataType="BOOL" Value="0"/>
</Structure>
</DefaultData>
</LocalTag>
<LocalTag Name="Flop" DataType="TIMER" ExternalAccess="None">
<DefaultData Format="L5K">
<![CDATA[[0,0,0]]]>
</DefaultData>
<DefaultData Format="Decorated">
<Structure DataType="TIMER">
<DataValueMember Name="PRE" DataType="DINT" Radix="Decimal" Value="0"/>
<DataValueMember Name="ACC" DataType="DINT" Radix="Decimal" Value="0"/>
<DataValueMember Name="EN" DataType="BOOL" Value="0"/>
<DataValueMember Name="TT" DataType="BOOL" Value="0"/>
<DataValueMember Name="DN" DataType="BOOL" Value="0"/>
</Structure>
</DefaultData>
</LocalTag>
</LocalTags>
<Routines>
<Routine Name="Logic" Type="RLL">
<RLLContent>
<Rung Number="0" Type="N">
<Text>
<![CDATA[MOVE(On,Flip.PRE)MOVE(Off,Flop.PRE);]]>
</Text>
</Rung>
<Rung Number="1" Type="N">
<Text>
<![CDATA[XIO(Flop.DN)TON(Flip,?,?);]]>
</Text>
</Rung>
<Rung Number="2" Type="N">
<Text>
<![CDATA[XIC(Flip.DN)TON(Flop,?,?);]]>
</Text>
</Rung>
<Rung Number="3" Type="N">
<Text>
<![CDATA[XIC(Flip.DN)OTE(Flash)OTE(EnableOut);]]>
</Text>
</Rung>
</RLLContent>
</Routine>
</Routines>
</AddOnInstructionDefinition>
<AddOnInstructionDefinition Use="Target" Name="AOI_TIPPER" Class="Standard" Revision="1.0" Vendor="Automation Standard" ExecutePrescan="true" ExecutePostscan="false" ExecuteEnableInFalse="false" CreatedDate="2011-11-21T18:20:13.957Z" CreatedBy="Not Available" EditedDate="2025-05-22T12:52:09.134Z"
 EditedBy="LCIBATUMI\ilia.gurielidze" SoftwareRevision="v36.00">
<Description>
<![CDATA[TIPPER]]>
</Description>
<Parameters>
<Parameter Name="EnableIn" TagType="Base" DataType="BOOL" Usage="Input" Radix="Decimal" Required="false" Visible="false" ExternalAccess="Read Only"/>
<Parameter Name="EnableOut" TagType="Base" DataType="BOOL" Usage="Output" Radix="Decimal" Required="false" Visible="false" ExternalAccess="Read Only"/>
<Parameter Name="HMI" TagType="Base" DataType="UDT_HMI_TIPPER" Usage="InOut" Required="true" Visible="true" Constant="false"/>
<Parameter Name="CTRL" TagType="Base" DataType="UDT_CTRL_TIPPER" Usage="InOut" Required="true" Visible="true" Constant="false"/>
<Parameter Name="MCM" TagType="Base" DataType="UDT_CTRL_MCM" Usage="InOut" Required="true" Visible="true" Constant="false"/>
<Parameter Name="ReadMSG" TagType="Base" DataType="MESSAGE" Usage="InOut" Required="true" Visible="true"/>
<Parameter Name="WriteMSG" TagType="Base" DataType="MESSAGE" Usage="InOut" Required="true" Visible="true"/>
<Parameter Name="In_Communication_Fault" TagType="Base" DataType="BOOL" Usage="Input" Radix="Decimal" Required="true" Visible="true" ExternalAccess="Read/Write">
<Description>
<![CDATA[Ethernet Communication Fault]]>
</Description>
<DefaultData Format="L5K">
<![CDATA[0]]>
</DefaultData>
<DefaultData Format="Decorated">
<DataValue DataType="BOOL" Radix="Decimal" Value="0"/>
</DefaultData>
</Parameter>
<Parameter Name="Running" TagType="Base" DataType="BOOL" Usage="Output" Radix="Decimal" Required="false" Visible="true" ExternalAccess="Read/Write">
<Description>
<![CDATA[Tipper Running]]>
</Description>
<DefaultData Format="L5K">
<![CDATA[0]]>
</DefaultData>
<DefaultData Format="Decorated">
<DataValue DataType="BOOL" Radix="Decimal" Value="0"/>
</DefaultData>
</Parameter>
<Parameter Name="Run_Enabled" TagType="Base" DataType="BOOL" Usage="Output" Radix="Decimal" Required="false" Visible="true" ExternalAccess="Read/Write">
<Description>
<![CDATA[Tipper Can Run]]>
</Description>
<DefaultData Format="L5K">
<![CDATA[0]]>
</DefaultData>
<DefaultData Format="Decorated">
<DataValue DataType="BOOL" Radix="Decimal" Value="0"/>
</DefaultData>
</Parameter>
<Parameter Name="Run" TagType="Base" DataType="BOOL" Usage="Output" Radix="Decimal" Required="false" Visible="true" ExternalAccess="Read/Write">
<Description>
<![CDATA[Run Tipper]]>
</Description>
<DefaultData Format="L5K">
<![CDATA[0]]>
</DefaultData>
<DefaultData Format="Decorated">
<DataValue DataType="BOOL" Radix="Decimal" Value="0"/>
</DefaultData>
</Parameter>
<Parameter Name="EStopped" TagType="Base" DataType="BOOL" Usage="Output" Radix="Decimal" Required="false" Visible="true" ExternalAccess="Read/Write">
<Description>
<![CDATA[Emergency Stop Actuated]]>
</Description>
<DefaultData Format="L5K">
<![CDATA[0]]>
</DefaultData>
<DefaultData Format="Decorated">
<DataValue DataType="BOOL" Radix="Decimal" Value="0"/>
</DefaultData>
</Parameter>
<Parameter Name="Disabled" TagType="Base" DataType="BOOL" Usage="Output" Radix="Decimal" Required="false" Visible="true" ExternalAccess="Read Only">
<Description>
<![CDATA[Tipper]]>
</Description>
<DefaultData Format="L5K">
<![CDATA[0]]>
</DefaultData>
<DefaultData Format="Decorated">
<DataValue DataType="BOOL" Radix="Decimal" Value="0"/>
</DefaultData>
</Parameter>
<Parameter Name="VFD_Fault" TagType="Base" DataType="BOOL" Usage="Output" Radix="Decimal" Required="false" Visible="true" ExternalAccess="Read/Write">
<Description>
<![CDATA[VFD Faulted]]>
</Description>
<DefaultData Format="L5K">
<![CDATA[0]]>
</DefaultData>
<DefaultData Format="Decorated">
<DataValue DataType="BOOL" Radix="Decimal" Value="0"/>
</DefaultData>
</Parameter>
<Parameter Name="Read_Data" TagType="Base" DataType="DINT" Usage="Input" Radix="Decimal" Required="false" Visible="false" ExternalAccess="Read/Write">
<Comments>
<Comment Operand=".0">
<![CDATA[Hearbeat from Conveyor]]>
</Comment>
<Comment Operand=".1">
<![CDATA[Dumper in Auto Mode]]>
</Comment>
<Comment Operand=".2">
<![CDATA[Dumper in Manual Mode]]>
</Comment>
<Comment Operand=".3">
<![CDATA[Dumper Emergency Stopped]]>
</Comment>
<Comment Operand=".4">
<![CDATA[Dumper Running in Auto Mode]]>
</Comment>
<Comment Operand=".5">
<![CDATA[Dumper Faulted]]>
</Comment>
</Comments>
<DefaultData Format="L5K">
<![CDATA[0]]>
</DefaultData>
<DefaultData Format="Decorated">
<DataValue DataType="DINT" Radix="Decimal" Value="0"/>
</DefaultData>
</Parameter>
<Parameter Name="Write_Data" TagType="Base" DataType="DINT" Usage="Output" Radix="Decimal" Required="false" Visible="false" ExternalAccess="None">
<Comments>
<Comment Operand=".0">
<![CDATA[Hearbeat to Conveyor]]>
</Comment>
<Comment Operand=".1">
<![CDATA[Dumper is Ready to Dump Package from Conveyor]]>
</Comment>
</Comments>
<DefaultData Format="L5K">
<![CDATA[0]]>
</DefaultData>
<DefaultData Format="Decorated">
<DataValue DataType="DINT" Radix="Decimal" Value="0"/>
</DefaultData>
</Parameter>
<Parameter Name="Communication_Fault" TagType="Base" DataType="BOOL" Usage="Output" Radix="Decimal" Required="false" Visible="true" ExternalAccess="None">
<Description>
<![CDATA[Ethernet Communication Fault]]>
</Description>
<DefaultData Format="L5K">
<![CDATA[0]]>
</DefaultData>
<DefaultData Format="Decorated">
<DataValue DataType="BOOL" Radix="Decimal" Value="0"/>
</DefaultData>
</Parameter>
<Parameter Name="Maintenance_Mode" TagType="Base" DataType="BOOL" Usage="Output" Radix="Decimal" Required="false" Visible="true" ExternalAccess="Read/Write">
<Description>
<![CDATA[In Maintance Mode]]>
</Description>
<DefaultData Format="L5K">
<![CDATA[0]]>
</DefaultData>
<DefaultData Format="Decorated">
<DataValue DataType="BOOL" Radix="Decimal" Value="0"/>
</DefaultData>
</Parameter>
</Parameters>
<LocalTags>
<LocalTag Name="Jammed_Latch" DataType="BOOL" Radix="Decimal" ExternalAccess="None">
<Description>
<![CDATA[Unlatches the Data in PreScan]]>
</Description>
<DefaultData Format="L5K">
<![CDATA[0]]>
</DefaultData>
<DefaultData Format="Decorated">
<DataValue DataType="BOOL" Radix="Decimal" Value="0"/>
</DefaultData>
</LocalTag>
<LocalTag Name="Heartbeat_Timer" DataType="TIMER" Dimensions="2" ExternalAccess="None">
<Description>
<![CDATA[After Timer is Done, which means that Hearbeat Stopped reports Communication Fault]]>
</Description>
<DefaultData Format="L5K">
<![CDATA[[[0,1000,0],[0,1000,0]]]]>
</DefaultData>
<DefaultData Format="Decorated">
<Array DataType="TIMER" Dimensions="2">
<Element Index="[0]">
<Structure DataType="TIMER">
<DataValueMember Name="PRE" DataType="DINT" Radix="Decimal" Value="1000"/>
<DataValueMember Name="ACC" DataType="DINT" Radix="Decimal" Value="0"/>
<DataValueMember Name="EN" DataType="BOOL" Value="0"/>
<DataValueMember Name="TT" DataType="BOOL" Value="0"/>
<DataValueMember Name="DN" DataType="BOOL" Value="0"/>
</Structure>
</Element>
<Element Index="[1]">
<Structure DataType="TIMER">
<DataValueMember Name="PRE" DataType="DINT" Radix="Decimal" Value="1000"/>
<DataValueMember Name="ACC" DataType="DINT" Radix="Decimal" Value="0"/>
<DataValueMember Name="EN" DataType="BOOL" Value="0"/>
<DataValueMember Name="TT" DataType="BOOL" Value="0"/>
<DataValueMember Name="DN" DataType="BOOL" Value="0"/>
</Structure>
</Element>
</Array>
</DefaultData>
</LocalTag>
<LocalTag Name="Data_Timer" DataType="TIMER" ExternalAccess="None">
<Description>
<![CDATA[Limit Messages not to Overflow the Controller]]>
</Description>
<DefaultData Format="L5K">
<![CDATA[[0,100,0]]]>
</DefaultData>
<DefaultData Format="Decorated">
<Structure DataType="TIMER">
<DataValueMember Name="PRE" DataType="DINT" Radix="Decimal" Value="100"/>
<DataValueMember Name="ACC" DataType="DINT" Radix="Decimal" Value="0"/>
<DataValueMember Name="EN" DataType="BOOL" Value="0"/>
<DataValueMember Name="TT" DataType="BOOL" Value="0"/>
<DataValueMember Name="DN" DataType="BOOL" Value="0"/>
</Structure>
</DefaultData>
</LocalTag>
<LocalTag Name="Flip_Flop" DataType="AOI_FLIP_FLOP" ExternalAccess="None">
<Description>
<![CDATA[Toggles On and Off,  tries to Write Hearbeat to Tipper Module]]>
</Description>
<DefaultData Format="L5K">
<![CDATA[[1,0,0,[0,0,0],[0,0,0]]]]>
</DefaultData>
<DefaultData Format="Decorated">
<Structure DataType="AOI_FLIP_FLOP">
<DataValueMember Name="EnableIn" DataType="BOOL" Value="1"/>
<DataValueMember Name="EnableOut" DataType="BOOL" Value="0"/>
<DataValueMember Name="On" DataType="DINT" Radix="Decimal" Value="0"/>
<DataValueMember Name="Off" DataType="DINT" Radix="Decimal" Value="0"/>
<DataValueMember Name="Flash" DataType="BOOL" Value="0"/>
</Structure>
</DefaultData>
</LocalTag>
</LocalTags>
<Routines>
<Routine Name="Logic" Type="RLL">
<RLLContent>
<Rung Number="0" Type="N">
<Text>
<![CDATA[XIO(Data_Timer.DN)TON(Data_Timer,?,?);]]>
</Text>
</Rung>
<Rung Number="1" Type="N">
<Text>
<![CDATA[XIC(Data_Timer.DN)MSG(ReadMSG)MSG(WriteMSG);]]>
</Text>
</Rung>
<Rung Number="2" Type="N">
<Text>
<![CDATA[XIO(Communication_Fault)XIC(Read_Data.3)OTE(EStopped);]]>
</Text>
</Rung>
<Rung Number="3" Type="N">
<Text>
<![CDATA[XIO(Communication_Fault)XIC(Read_Data.4)OTE(CTRL.STS.Dumping);]]>
</Text>
</Rung>
<Rung Number="4" Type="N">
<Text>
<![CDATA[XIO(Communication_Fault)XIC(HMI.MaintMode)OTE(CTRL.STS.In_Maintenance_Mode)OTE(Maintenance_Mode);]]>
</Text>
</Rung>
<Rung Number="5" Type="N">
<Text>
<![CDATA[[XIO(Read_Data.3) XIC(Read_Data.5) ,XIC(Communication_Fault) ]OTE(VFD_Fault)OTE(CTRL.STS.VFD_Fault);]]>
</Text>
</Rung>
<Rung Number="6" Type="N">
<Text>
<![CDATA[[AOI_FLIP_FLOP(Flip_Flop,1000,1000) OTE(Write_Data.0) ,XIC(Read_Data.0) TON(Heartbeat_Timer[0],?,?) ,XIO(Read_Data.0) TON(Heartbeat_Timer[1],?,?) ];]]>
</Text>
</Rung>
<Rung Number="7" Type="N">
<Text>
<![CDATA[XIO(In_Communication_Fault)[XIC(Heartbeat_Timer[0].DN) ,XIC(Heartbeat_Timer[1].DN) ]OTE(Communication_Fault)OTE(CTRL.STS.Communication_Fault);]]>
</Text>
</Rung>
<Rung Number="8" Type="N">
<Text>
<![CDATA[XIC(MCM.STS.System_Started)XIO(Disabled)XIC(Read_Data.1)OTE(Run_Enabled);]]>
</Text>
</Rung>
<Rung Number="9" Type="N">
<Text>
<![CDATA[XIC(CTRL.CMD.Interlock)OTE(Write_Data.1)OTE(Running)OTE(CTRL.STS.Running)OTE(CTRL.STS.Interlock);]]>
</Text>
</Rung>
<Rung Number="10" Type="N">
<Comment>
<![CDATA[Alarms
]]>
</Comment>
<Text>
<![CDATA[XIC(Communication_Fault)OTE(HMI.Alarm.Communication_Fault);]]>
</Text>
</Rung>
<Rung Number="11" Type="N">
<Text>
<![CDATA[XIC(VFD_Fault)OTE(HMI.Alarm.VFD_Fault);]]>
</Text>
</Rung>
<Rung Number="12" Type="N">
<Comment>
<![CDATA[Colors of Animation
]]>
</Comment>
<Text>
<![CDATA[NOP();]]>
</Text>
</Rung>
<Rung Number="13" Type="N">
<Comment>
<![CDATA[Disabled or Not Running - Medium Gray (96.96.96)
]]>
</Comment>
<Text>
<![CDATA[[XIC(Disabled) ,XIO(MCM.STS.System_Started) XIO(Running) ]MOVE(13,HMI.Color);]]>
</Text>
</Rung>
<Rung Number="14" Type="N">
<Comment>
<![CDATA[Not Running - White Color (0.0.0)
]]>
</Comment>
<Text>
<![CDATA[XIC(MCM.STS.System_Started)XIO(Running)MOVE(12,HMI.Color);]]>
</Text>
</Rung>
<Rung Number="15" Type="N">
<Comment>
<![CDATA[Running - Green (0.255.0)
]]>
</Comment>
<Text>
<![CDATA[XIC(Running)MOVE(10,HMI.Color);]]>
</Text>
</Rung>
<Rung Number="16" Type="N">
<Comment>
<![CDATA[Motor Ethernet Fault - Blue (0.0.255)
]]>
</Comment>
<Text>
<![CDATA[XIC(Communication_Fault)MOVE(2,HMI.Color);]]>
</Text>
</Rung>
<Rung Number="17" Type="N">
<Comment>
<![CDATA[Motor VFD Fault - Blue (0.0.255)
]]>
</Comment>
<Text>
<![CDATA[XIC(VFD_Fault)MOVE(2,HMI.Color);]]>
</Text>
</Rung>
<Rung Number="18" Type="N">
<Comment>
<![CDATA[Emergency Stopped - Red (255.0.0)
]]>
</Comment>
<Text>
<![CDATA[XIC(EStopped)MOVE(1,HMI.Color);]]>
</Text>
</Rung>
<Rung Number="19" Type="N">
<Text>
<![CDATA[OTU(CTRL.CMD.Start)OTU(CTRL.CMD.Stop_Require_Start)OTU(CTRL.CMD.Jammed)OTU(CTRL.CMD.Full)OTU(CTRL.CMD.Disable)OTU(CTRL.CMD.Run_Up)OTU(CTRL.CMD.Stopped_By_MCM_Stop_PB)MOVE('',CTRL.CMD.Log);]]>
</Text>
</Rung>
</RLLContent>
</Routine>
<Routine Name="Prescan" Type="RLL">
<RLLContent>
<Rung Number="0" Type="N">
<Text>
<![CDATA[FLL(0,CTRL,1)FLL(0,HMI.Alarm,1);]]>
</Text>
</Rung>
<Rung Number="1" Type="N">
<Text>
<![CDATA[MOVE(5000,Heartbeat_Timer[0].PRE)MOVE(5000,Heartbeat_Timer[1].PRE);]]>
</Text>
</Rung>
<Rung Number="2" Type="N">
<Text>
<![CDATA[OTU(Jammed_Latch);]]>
</Text>
</Rung>
</RLLContent>
</Routine>
</Routines>
<Dependencies>
<Dependency Type="DataType" Name="UDT_CTRL_TIPPER"/>
<Dependency Type="AddOnInstructionDefinition" Name="AOI_FLIP_FLOP"/>
<Dependency Type="DataType" Name="UDT_HMI_TIPPER"/>
<Dependency Type="DataType" Name="UDT_CTRL_MCM"/>
</Dependencies>
</AddOnInstructionDefinition>
</AddOnInstructionDefinitions>
</Controller>
</RSLogix5000Content>
