<?xml version="1.0" encoding="UTF-8" standalone="yes"?>
<!--JAM RESET STATION PUSH BUTTON
-->
<RSLogix5000Content SchemaRevision="1.0" SoftwareRevision="36.00" TargetName="AOI_STATION_JR_PB" TargetType="AddOnInstructionDefinition" TargetRevision="1.0 " TargetLastEdited="2025-05-26T17:59:22.000Z" ContainsContext="true" ExportDate="Thu Jun 12 20:35:55 2025" ExportOptions="References NoRawData L5KData DecoratedData Context Dependencies ForceProtectedEncoding AllProjDocTrans">
<Controller Use="Context" Name="BaseProgram">
<DataTypes Use="Context">
<DataType Name="UDT_ALARMS_STATION" Family="NoFamily" Class="User">
<Members>
<Member Name="ZZZZZZZZZZUDT_ALARMS0" DataType="SINT" Dimension="0" Radix="Decimal" Hidden="true" ExternalAccess="Read/Write"/>
<Member Name="EStopped" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_ALARMS0" BitNumber="0" ExternalAccess="Read/Write">
<Description>
<![CDATA[Conveyor Emergency Stopped]]>
</Description>
</Member>
<Member Name="Stopped" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_ALARMS0" BitNumber="1" ExternalAccess="Read/Write">
<Description>
<![CDATA[Conveyor Stopped]]>
</Description>
</Member>
</Members>
</DataType>
<DataType Name="UDT_CTRL_STATION" Family="NoFamily" Class="User">
<Members>
<Member Name="CMD" DataType="UDT_CTRL_STATION_CMD" Dimension="0" Radix="NullType" Hidden="false" ExternalAccess="Read/Write"/>
<Member Name="STS" DataType="UDT_CTRL_STATION_STS" Dimension="0" Radix="NullType" Hidden="false" ExternalAccess="Read/Write"/>
</Members>
<Dependencies>
<Dependency Type="DataType" Name="UDT_CTRL_STATION_CMD"/>
<Dependency Type="DataType" Name="UDT_CTRL_STATION_STS"/>
</Dependencies>
</DataType>
<DataType Name="UDT_CTRL_STATION_CMD" Family="NoFamily" Class="User">
<Members>
<Member Name="ZZZZZZZZZZUDT_CTRL_S0" DataType="SINT" Dimension="0" Radix="Decimal" Hidden="true" ExternalAccess="Read/Write"/>
<Member Name="Jammed" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_S0" BitNumber="0" ExternalAccess="Read/Write">
<Description>
<![CDATA[Conveyor]]>
</Description>
</Member>
<Member Name="EStop_Actuated" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_S0" BitNumber="1" ExternalAccess="Read/Write">
<Description>
<![CDATA[Emergency Stop Actuated]]>
</Description>
</Member>
<Member Name="Log" DataType="STRING" Dimension="0" Radix="NullType" Hidden="false" ExternalAccess="Read/Write">
<Description>
<![CDATA[Log]]>
</Description>
</Member>
</Members>
</DataType>
<DataType Name="UDT_CTRL_STATION_STS" Family="NoFamily" Class="User">
<Members>
<Member Name="ZZZZZZZZZZUDT_CTRL_S0" DataType="SINT" Dimension="0" Radix="Decimal" Hidden="true" ExternalAccess="Read/Write"/>
<Member Name="Start" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_S0" BitNumber="0" ExternalAccess="Read/Write">
<Description>
<![CDATA[Start command For/From Partner Stations]]>
</Description>
</Member>
<Member Name="Stop" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_S0" BitNumber="1" ExternalAccess="Read/Write">
<Description>
<![CDATA[Stop command For/From Partner Stations]]>
</Description>
</Member>
<Member Name="EStop_Was_Actuated" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_S0" BitNumber="2" ExternalAccess="Read/Write">
<Description>
<![CDATA[Emergency Stop was Actuated]]>
</Description>
</Member>
<Member Name="Log" DataType="STRING" Dimension="0" Radix="NullType" Hidden="false" ExternalAccess="Read/Write">
<Description>
<![CDATA[Log]]>
</Description>
</Member>
<Member Name="ZZZZZZZZZZUDT_CTRL_S5" DataType="SINT" Dimension="0" Radix="Decimal" Hidden="true" ExternalAccess="Read/Write"/>
<Member Name="JR_PB_LT" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_S5" BitNumber="0" ExternalAccess="Read/Write">
<Description>
<![CDATA[Jam Reset Push Button Light]]>
</Description>
</Member>
<Member Name="Jam_Fault" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_S5" BitNumber="1" ExternalAccess="Read/Write">
<Description>
<![CDATA[Conveyor Jammed]]>
</Description>
</Member>
</Members>
</DataType>
<DataType Name="UDT_CTRL_VFD" Family="NoFamily" Class="User">
<Members>
<Member Name="CMD" DataType="UDT_CTRL_VFD_CMD" Dimension="0" Radix="NullType" Hidden="false" ExternalAccess="Read/Write"/>
<Member Name="STS" DataType="UDT_CTRL_VFD_STS" Dimension="0" Radix="NullType" Hidden="false" ExternalAccess="Read/Write"/>
</Members>
<Dependencies>
<Dependency Type="DataType" Name="UDT_CTRL_VFD_CMD"/>
<Dependency Type="DataType" Name="UDT_CTRL_VFD_STS"/>
</Dependencies>
</DataType>
<DataType Name="UDT_CTRL_VFD_CMD" Family="NoFamily" Class="User">
<Members>
<Member Name="ZZZZZZZZZZUDT_CTRL_V0" DataType="SINT" Dimension="0" Radix="Decimal" Hidden="true" ExternalAccess="Read/Write"/>
<Member Name="Start" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_V0" BitNumber="0" ExternalAccess="Read/Write">
<Description>
<![CDATA[Start the Conveyor Locally in Auto Mode]]>
</Description>
</Member>
<Member Name="Stop_Require_Start" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_V0" BitNumber="1" ExternalAccess="Read/Write">
<Description>
<![CDATA[Stops the Motor
, requires Start command to Restart]]>
</Description>
</Member>
<Member Name="Stop_Auto_Restart" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_V0" BitNumber="2" ExternalAccess="Read/Write">
<Description>
<![CDATA[Stops the Motor, which will restart automatically when False]]>
</Description>
</Member>
<Member Name="Jammed" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_V0" BitNumber="3" ExternalAccess="Read/Write">
<Description>
<![CDATA[Conveyor]]>
</Description>
</Member>
<Member Name="Disable" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_V0" BitNumber="4" ExternalAccess="Read/Write">
<Description>
<![CDATA[Conveyor]]>
</Description>
</Member>
<Member Name="Run_Up_Enabled" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_V0" BitNumber="5" ExternalAccess="Read/Write">
<Description>
<![CDATA[When Downstream Conveyors are Stopped, Conveyor keeps running unill Discharge PE is Blocked]]>
</Description>
</Member>
<Member Name="Power_Saving_Mode_ON" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_V0" BitNumber="6" ExternalAccess="Read/Write">
<Description>
<![CDATA[VFD
is in Power Saving Mode]]>
</Description>
</Member>
<Member Name="Interlock" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_V0" BitNumber="7" ExternalAccess="Read/Write">
<Description>
<![CDATA[Downstream is Running]]>
</Description>
</Member>
<Member Name="ZZZZZZZZZZUDT_CTRL_V9" DataType="SINT" Dimension="0" Radix="Decimal" Hidden="true" ExternalAccess="Read/Write"/>
<Member Name="Stopped_By_Stop_PB" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_V9" BitNumber="0" ExternalAccess="Read/Write">
<Description>
<![CDATA[Conveyor
Stopped by Station Stop PushButton]]>
</Description>
</Member>
<Member Name="Log" DataType="STRING" Dimension="0" Radix="NullType" Hidden="false" ExternalAccess="Read/Write">
<Description>
<![CDATA[Log]]>
</Description>
</Member>
<Member Name="Acknowledge_Log" DataType="STRING" Dimension="0" Radix="NullType" Hidden="false" ExternalAccess="Read/Write">
<Description>
<![CDATA[Acknowledge Log]]>
</Description>
</Member>
<Member Name="ZZZZZZZZZZUDT_CTRL_V13" DataType="SINT" Dimension="0" Radix="Decimal" Hidden="true" ExternalAccess="Read/Write"/>
<Member Name="Full" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_V13" BitNumber="0" ExternalAccess="Read/Write">
<Description>
<![CDATA[Conveyor]]>
</Description>
</Member>
<Member Name="Encoder_Fault" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_V13" BitNumber="1" ExternalAccess="Read/Write">
<Description>
<![CDATA[Encoder Faulted or Conveyor is Running at Low Speed]]>
</Description>
</Member>
<Member Name="Speed_FPM" DataType="DINT" Dimension="0" Radix="Decimal" Hidden="false" ExternalAccess="Read/Write">
<Description>
<![CDATA[Speed in Feet per Minute]]>
</Description>
</Member>
</Members>
</DataType>
<DataType Name="UDT_CTRL_VFD_STS" Family="NoFamily" Class="User">
<Members>
<Member Name="ZZZZZZZZZZUDT_CTRL_V0" DataType="SINT" Dimension="0" Radix="Decimal" Hidden="true" ExternalAccess="Read/Write"/>
<Member Name="Running" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_V0" BitNumber="0" ExternalAccess="Read/Write">
<Description>
<![CDATA[Running]]>
</Description>
</Member>
<Member Name="VFD_Fault" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_V0" BitNumber="1" ExternalAccess="Read/Write">
<Description>
<![CDATA[VFD Faulted]]>
</Description>
</Member>
<Member Name="Communication_Fault" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_V0" BitNumber="2" ExternalAccess="Read/Write">
<Description>
<![CDATA[Ethernet Communicationb Faulted]]>
</Description>
</Member>
<Member Name="Interlock" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_V0" BitNumber="3" ExternalAccess="Read/Write">
<Description>
<![CDATA[Downstream Conveyor is Running]]>
</Description>
</Member>
<Member Name="Current_Speed" DataType="DINT" Dimension="0" Radix="Decimal" Hidden="false" ExternalAccess="Read/Write">
<Description>
<![CDATA[Current Speed of Conveyor in FPM]]>
</Description>
</Member>
<Member Name="Requested_Speed" DataType="DINT" Dimension="0" Radix="Decimal" Hidden="false" ExternalAccess="Read/Write">
<Description>
<![CDATA[Requested Speed of Conveyor in FPM]]>
</Description>
</Member>
<Member Name="ZZZZZZZZZZUDT_CTRL_V7" DataType="SINT" Dimension="0" Radix="Decimal" Hidden="true" ExternalAccess="Read/Write"/>
<Member Name="In_Power_Saving_Mode" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_V7" BitNumber="0" ExternalAccess="Read/Write">
<Description>
<![CDATA[In Power Saving Mode]]>
</Description>
</Member>
<Member Name="Maintenance_Mode" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_V7" BitNumber="1" ExternalAccess="Read/Write">
<Description>
<![CDATA[In Maintenance Mode]]>
</Description>
</Member>
<Member Name="MCM_Started" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_V7" BitNumber="2" ExternalAccess="Read/Write">
<Description>
<![CDATA[MCM Started]]>
</Description>
</Member>
<Member Name="EStopped" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_V7" BitNumber="3" ExternalAccess="Read/Write">
<Description>
<![CDATA[Conveyor Emergency Stopped]]>
</Description>
</Member>
<Member Name="Jammed" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_V7" BitNumber="4" ExternalAccess="Read/Write">
<Description>
<![CDATA[Conveyor]]>
</Description>
</Member>
<Member Name="Full" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_V7" BitNumber="5" ExternalAccess="Read/Write">
<Description>
<![CDATA[Conveyor]]>
</Description>
</Member>
<Member Name="Enabled" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_V7" BitNumber="6" ExternalAccess="Read/Write">
<Description>
<![CDATA[Conveyor]]>
</Description>
</Member>
<Member Name="Local_Stopped" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_V7" BitNumber="7" ExternalAccess="Read/Write">
<Description>
<![CDATA[Conveyor is Stopped Locally]]>
</Description>
</Member>
<Member Name="Log" DataType="STRING" Dimension="0" Radix="NullType" Hidden="false" ExternalAccess="Read/Write">
<Description>
<![CDATA[Log]]>
</Description>
</Member>
<Member Name="ZZZZZZZZZZUDT_CTRL_V17" DataType="SINT" Dimension="0" Radix="Decimal" Hidden="true" ExternalAccess="Read/Write"/>
<Member Name="Encoder_Fault" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_V17" BitNumber="0" ExternalAccess="Read/Write">
<Description>
<![CDATA[Encoder Faulted or Conveyor is Running at Low Speed]]>
</Description>
</Member>
<Member Name="MCM_JR_PB_Pressed" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_V17" BitNumber="1" ExternalAccess="Read/Write">
<Description>
<![CDATA[Jam Reset PushButton Pressed on MCM]]>
</Description>
</Member>
<Member Name="Disabled" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_V17" BitNumber="2" ExternalAccess="Read/Write">
<Description>
<![CDATA[Conveyor]]>
</Description>
</Member>
<Member Name="MCM_Start_PB_Pressed" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_V17" BitNumber="3" ExternalAccess="Read/Write">
<Description>
<![CDATA[Start PushButton Pressed on MCM]]>
</Description>
</Member>
<Member Name="MCM_EStop_PB_Pressed" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_CTRL_V17" BitNumber="4" ExternalAccess="Read/Write">
<Description>
<![CDATA[Emergency Stop PushButton Pressed on MCM]]>
</Description>
</Member>
</Members>
</DataType>
<DataType Name="UDT_HMI_STATION" Family="NoFamily" Class="User">
<Members>
<Member Name="Name" DataType="STRING" Dimension="0" Radix="NullType" Hidden="false" ExternalAccess="Read/Write">
<Description>
<![CDATA[Station Name]]>
</Description>
</Member>
<Member Name="MCM_Name" DataType="STRING" Dimension="0" Radix="NullType" Hidden="false" ExternalAccess="Read/Write">
<Description>
<![CDATA[MCM Name]]>
</Description>
</Member>
<Member Name="Conveyor_Name" DataType="STRING" Dimension="0" Radix="NullType" Hidden="false" ExternalAccess="Read/Write">
<Description>
<![CDATA[Conveyor Name]]>
</Description>
</Member>
<Member Name="Alarm" DataType="UDT_ALARMS_STATION" Dimension="0" Radix="NullType" Hidden="false" ExternalAccess="Read/Write">
<Description>
<![CDATA[Station Alarms]]>
</Description>
</Member>
<Member Name="ZZZZZZZZZZUDT_HMI_ST4" DataType="SINT" Dimension="0" Radix="Decimal" Hidden="true" ExternalAccess="Read/Write"/>
<Member Name="Start_PB" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_HMI_ST4" BitNumber="0" ExternalAccess="Read/Write">
<Description>
<![CDATA[Start PushButton]]>
</Description>
</Member>
<Member Name="Stop_PB" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_HMI_ST4" BitNumber="1" ExternalAccess="Read/Write">
<Description>
<![CDATA[Stop PushButton]]>
</Description>
</Member>
<Member Name="STATE" DataType="DINT" Dimension="0" Radix="Decimal" Hidden="false" ExternalAccess="Read/Write">
<Description>
<![CDATA[Start Color]]>
</Description>
</Member>
<Member Name="Stop_Color" DataType="DINT" Dimension="0" Radix="Decimal" Hidden="false" ExternalAccess="Read/Write">
<Description>
<![CDATA[Stop Color]]>
</Description>
</Member>
<Member Name="ZZZZZZZZZZUDT_HMI_ST9" DataType="SINT" Dimension="0" Radix="Decimal" Hidden="true" ExternalAccess="Read/Write"/>
<Member Name="JR_PB_LT" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_HMI_ST9" BitNumber="0" ExternalAccess="Read/Write">
<Description>
<![CDATA[Jam Restart PushButton Light]]>
</Description>
</Member>
<Member Name="ALARMST" DataType="DINT" Dimension="0" Radix="Decimal" Hidden="false" ExternalAccess="Read/Write"/>
<Member Name="DISC" DataType="DINT" Dimension="0" Radix="Decimal" Hidden="false" ExternalAccess="Read/Write"/>
<Member Name="ZZZZZZZZZZUDT_HMI_ST13" DataType="SINT" Dimension="0" Radix="Decimal" Hidden="true" ExternalAccess="Read/Write"/>
<Member Name="JR_Pressed" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZUDT_HMI_ST13" BitNumber="0" ExternalAccess="Read/Write"/>
</Members>
<Dependencies>
<Dependency Type="DataType" Name="UDT_ALARMS_STATION"/>
</Dependencies>
</DataType>
</DataTypes>
<AddOnInstructionDefinitions Use="Context">
<AddOnInstructionDefinition Use="Target" Name="AOI_STATION_JR_PB" Revision="1.0" Vendor="Automation Standard" ExecutePrescan="true" ExecutePostscan="false" ExecuteEnableInFalse="false" CreatedDate="2011-11-21T15:10:22.337Z" CreatedBy="Not Available" EditedDate="2025-05-26T17:59:22.000Z" EditedBy="LCIBATUMI\ilia.gurielidze"
 SoftwareRevision="v36.00">
<Description>
<![CDATA[JAM RESET STATION PUSH BUTTON
]]>
</Description>
<Parameters>
<Parameter Name="EnableIn" TagType="Base" DataType="BOOL" Usage="Input" Radix="Decimal" Required="false" Visible="false" ExternalAccess="Read Only">
<Description>
<![CDATA[Enable Input - System Defined Parameter]]>
</Description>
</Parameter>
<Parameter Name="EnableOut" TagType="Base" DataType="BOOL" Usage="Output" Radix="Decimal" Required="false" Visible="false" ExternalAccess="Read Only">
<Description>
<![CDATA[Enable Output - System Defined Parameter]]>
</Description>
</Parameter>
<Parameter Name="HMI" TagType="Base" DataType="UDT_HMI_STATION" Usage="InOut" Required="true" Visible="true" Constant="false"/>
<Parameter Name="CTRL" TagType="Base" DataType="UDT_CTRL_STATION" Usage="InOut" Required="true" Visible="true" Constant="false"/>
<Parameter Name="Partner" TagType="Base" DataType="UDT_CTRL_STATION" Usage="InOut" Required="true" Visible="true" Constant="false"/>
<Parameter Name="Motor" TagType="Base" DataType="UDT_CTRL_VFD" Usage="InOut" Required="true" Visible="true" Constant="false"/>
<Parameter Name="In_JR_PB" TagType="Base" DataType="BOOL" Usage="Input" Radix="Decimal" Required="true" Visible="true" ExternalAccess="Read/Write">
<Description>
<![CDATA[Jam Reset PushButton (NO)]]>
</Description>
<DefaultData Format="L5K">
<![CDATA[0]]>
</DefaultData>
<DefaultData Format="Decorated">
<DataValue DataType="BOOL" Radix="Decimal" Value="0"/>
</DefaultData>
</Parameter>
<Parameter Name="Out_JR_PB_LT" TagType="Base" DataType="BOOL" Usage="Output" Radix="Decimal" Required="true" Visible="true" ExternalAccess="Read Only">
<Description>
<![CDATA[Jam Reset PushButton Light]]>
</Description>
<DefaultData Format="L5K">
<![CDATA[0]]>
</DefaultData>
<DefaultData Format="Decorated">
<DataValue DataType="BOOL" Radix="Decimal" Value="0"/>
</DefaultData>
</Parameter>
</Parameters>
<LocalTags>
<LocalTag Name="ONS" DataType="DINT" Radix="Decimal" ExternalAccess="None">
<Description>
<![CDATA[To prevent the Lathing of Start Signal between Partner Stations]]>
</Description>
<DefaultData Format="L5K">
<![CDATA[0]]>
</DefaultData>
<DefaultData Format="Decorated">
<DataValue DataType="DINT" Radix="Decimal" Value="0"/>
</DefaultData>
</LocalTag>
<LocalTag Name="Jammed" DataType="BOOL" Radix="Decimal" ExternalAccess="None">
<Description>
<![CDATA[Conveyor Jammed]]>
</Description>
<DefaultData Format="L5K">
<![CDATA[0]]>
</DefaultData>
<DefaultData Format="Decorated">
<DataValue DataType="BOOL" Radix="Decimal" Value="0"/>
</DefaultData>
</LocalTag>
<LocalTag Name="Empty_String" DataType="STRING" ExternalAccess="None">
<Description>
<![CDATA[String contains ""]]>
</Description>
<DefaultData Format="L5K">
<![CDATA[[0,'$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00$00']]]>
</DefaultData>
<DefaultData Format="String" Length="0">
<![CDATA['']]>
</DefaultData>
</LocalTag>
<LocalTag Name="ONS_Diagnostic_Alram" DataType="BOOL" Radix="Decimal" ExternalAccess="None">
<DefaultData Format="L5K">
<![CDATA[0]]>
</DefaultData>
<DefaultData Format="Decorated">
<DataValue DataType="BOOL" Radix="Decimal" Value="0"/>
</DefaultData>
</LocalTag>
</LocalTags>
<Routines>
<Routine Name="Logic" Type="RLL">
<RLLContent>
<Rung Number="0" Type="N">
<Text>
<![CDATA[COP(CTRL.CMD.Log,CTRL.STS.Log,1);]]>
</Text>
</Rung>
<Rung Number="1" Type="N">
<Text>
<![CDATA[[XIC(In_JR_PB) ,XIC(HMI.Start_PB) ,XIC(Partner.STS.Start) ONS(ONS.0) ]OTE(CTRL.STS.Start)OTU(HMI.Start_PB);]]>
</Text>
</Rung>
<Rung Number="2" Type="N">
<Text>
<![CDATA[[XIC(CTRL.CMD.Jammed) ,XIO(Jammed) XIC(Partner.STS.JR_PB_LT) ]OTE(CTRL.STS.JR_PB_LT)OTE(Out_JR_PB_LT)OTE(HMI.JR_PB_LT);]]>
</Text>
</Rung>
<Rung Number="3" Type="N">
<Text>
<![CDATA[XIC(CTRL.CMD.Jammed)OTE(Jammed);]]>
</Text>
</Rung>
<Rung Number="4" Type="N">
<Comment>
<![CDATA[Alarms
]]>
</Comment>
<Text>
<![CDATA[NOP();]]>
</Text>
</Rung>
<Rung Number="5" Type="N">
<Text>
<![CDATA[XIC(In_JR_PB)ONS(ONS_Diagnostic_Alram)MOVE(1,HMI.ALARMST);]]>
</Text>
</Rung>
<Rung Number="6" Type="N">
<Text>
<![CDATA[XIO(In_JR_PB)MOVE(0,HMI.ALARMST);]]>
</Text>
</Rung>
<Rung Number="7" Type="N">
<Comment>
<![CDATA[Colors of Animation
]]>
</Comment>
<Text>
<![CDATA[NOP();]]>
</Text>
</Rung>
<Rung Number="8" Type="N">
<Comment>
<![CDATA[Gray
]]>
</Comment>
<Text>
<![CDATA[XIO(Out_JR_PB_LT)MOVE(0,HMI.STATE);]]>
</Text>
</Rung>
<Rung Number="9" Type="N">
<Comment>
<![CDATA[White
]]>
</Comment>
<Text>
<![CDATA[XIC(Out_JR_PB_LT)MOVE(1,HMI.STATE);]]>
</Text>
</Rung>
<Rung Number="10" Type="N">
<Comment>
<![CDATA[Yellow
]]>
</Comment>
<Text>
<![CDATA[XIO(Out_JR_PB_LT)[XIC(In_JR_PB) ,XIC(HMI.Start_PB) ]MOVE(3,HMI.STATE);]]>
</Text>
</Rung>
<Rung Number="11" Type="N">
<Comment>
<![CDATA[Green
]]>
</Comment>
<Text>
<![CDATA[XIC(Out_JR_PB_LT)[XIC(In_JR_PB) ,XIC(HMI.Start_PB) ]MOVE(2,HMI.STATE);]]>
</Text>
</Rung>
<Rung Number="12" Type="N">
<Text>
<![CDATA[COP(Empty_String,CTRL.CMD.Log,1)OTU(CTRL.CMD.Jammed);]]>
</Text>
</Rung>
</RLLContent>
</Routine>
<Routine Name="Prescan" Type="RLL">
<RLLContent>
<Rung Number="0" Type="N">
<Text>
<![CDATA[NOP();]]>
</Text>
</Rung>
<Rung Number="1" Type="N">
<Text>
<![CDATA[FLL(0,HMI.Alarm,1)OTU(HMI.Start_PB);]]>
</Text>
</Rung>
</RLLContent>
</Routine>
</Routines>
<Dependencies>
<Dependency Type="DataType" Name="UDT_CTRL_STATION"/>
<Dependency Type="DataType" Name="UDT_HMI_STATION"/>
<Dependency Type="DataType" Name="UDT_CTRL_VFD"/>
</Dependencies>
</AddOnInstructionDefinition>
</AddOnInstructionDefinitions>
</Controller>
</RSLogix5000Content>
